[] - automode - BOOL - read only
[] - cfgcflasetting - REAL - WRITEABLE
[] - cfgcleartripcountafter - DINT - WRITEABLE
[] - cfgctripenablecontrol - UINT - WRITEABLE
[] - cfgcwarningenablecontrol - UINT - WRITEABLE
[] - cfggfgroundfaultinhibittime - USINT - WRITEABLE
[] - cfggfgroundfaulttripdelay - REAL - WRITEABLE
[] - cfggfgroundfaulttriplevel - REAL - WRITEABLE
[] - cfggfgroundfaultwarningdelay - REAL - WRITEABLE
[] - cfggfgroundfaultwarninglevel - REAL - WRITEABLE
[] - cfgictprimary - UINT - WRITEABLE
[] - cfgictsecondary - UINT - WRITEABLE
[] - cfgicurrentimbalanceinhibittim - USINT - WRITEABLE
[] - cfgicurrentimbalancetripdelay - USINT - WRITEABLE
[] - cfgicurrentimbalancetriplevel - USINT - WRITEABLE
[] - cfgicurrentimbalancewarninglev - USINT - WRITEABLE
[] - cfgijaminhibittime - USINT - WRITEABLE
[] - cfgijamtripdelay - USINT - WRITEABLE
[] - cfgijamtriplevel - UINT - read only
[] - cfgijamwarninglevel - UINT - WRITEABLE
[] - cfgilinelossinhibittime - USINT - WRITEABLE
[] - cfgilinelosstripdelay - REAL - WRITEABLE
[] - cfgiovercurrentinhibittime - USINT - WRITEABLE
[] - cfgiovercurrenttripdelay - REAL - WRITEABLE
[] - cfgiovercurrenttriplevel - USINT - WRITEABLE
[] - cfgiovercurrentwarninglevel - USINT - WRITEABLE
[] - cfgistallenabledtime - USINT - WRITEABLE
[] - cfgistalltriplevel - UINT - WRITEABLE
[] - cfgiundercurrentinhibittime - USINT - WRITEABLE
[] - cfgiundercurrenttripdelay - REAL - WRITEABLE
[] - cfgiundercurrenttriplevel - USINT - WRITEABLE
[] - cfgiundercurrentwarninglevel - USINT - WRITEABLE
[] - cfgiunderloadinhibittime - USINT - WRITEABLE
[] - cfgiunderloadtripdelay - REAL - WRITEABLE
[] - cfgiunderloadtriplevel - USINT - WRITEABLE
[] - cfgiunderloadwarninglevel - USINT - WRITEABLE
[] - cfgoverloadtripcountlimit - DINT - WRITEABLE
[] - cfgplphaselossinhibittime - USINT - WRITEABLE
[] - cfgplphaselosstripdelay - REAL - WRITEABLE
[] - cfgread - BOOL - WRITEABLE
[] - cfgspecificgravity - REAL - WRITEABLE
[] - cfgtcuolresetlevel - USINT - read only
[] - cfgtcuolwarninglevel - USINT - read only
[] - cfgtcutripclass - USINT - WRITEABLE
[] - cfgtimermodeenabled - BOOL - WRITEABLE
[] - cfgtimerruntime - DINT - WRITEABLE
[] - cfgtimerwaittime - DINT - WRITEABLE
[] - cfgtripcountlimit - DINT - WRITEABLE
[] - cfgvoverfrequencyinhibittime - USINT - WRITEABLE
[] - cfgvoverfrequencytripdelay - REAL - WRITEABLE
[] - cfgvoverfrequencytriplevel - USINT - WRITEABLE
[] - cfgvoverfrequencywarninglevel - USINT - WRITEABLE
[] - cfgvovervoltageinhibittime - USINT - WRITEABLE
[] - cfgvovervoltagetripdelay - REAL - WRITEABLE
[] - cfgvovervoltagetriplevel - REAL - WRITEABLE
[] - cfgvovervoltagewarninglevel - REAL - WRITEABLE
[] - cfgvphaserotationinhibittime - USINT - WRITEABLE
[] - cfgvphaserotationtriptype - USINT - WRITEABLE
[] - cfgvptprimary - UINT - WRITEABLE
[] - cfgvptsecondary - UINT - WRITEABLE
[] - cfgvunderfrequencyinhibittime - USINT - WRITEABLE
[] - cfgvunderfrequencytripdelay - REAL - WRITEABLE
[] - cfgvunderfrequencytriplevel - USINT - WRITEABLE
[] - cfgvunderfrequencywarninglevel - USINT - WRITEABLE
[] - cfgvundervoltageinhibittime - USINT - WRITEABLE
[] - cfgvundervoltagetripdelay - REAL - WRITEABLE
[] - cfgvundervoltagetriplevel - REAL - WRITEABLE
[] - cfgvundervoltagewarninglevel - REAL - WRITEABLE
[] - cfgvvoltageimbalanceinhibittim - USINT - WRITEABLE
[] - cfgvvoltageimbalancetripdelay - REAL - WRITEABLE
[] - cfgvvoltageimbalancetriplevel - USINT - WRITEABLE
[] - cfgvvoltageimbalancewarninglev - USINT - WRITEABLE
[] - cfgvvoltagemode - USINT - WRITEABLE
[] - cfgwrite - BOOL - WRITEABLE
[] - contactorstatus - BOOL - read only
[] - dhdownholestatusint - UINT - read only
[] - dhfluidlevel - REAL - read only
[] - dhintakepressure - REAL - read only
[] - dhintaketemperature - REAL - read only
[] - dhmaxintakepressureforever - UINT - read only
[] - dhmaxintakepressurestartup - UINT - read only
[] - dhmaxintaketemperatureforever - REAL - read only
[] - dhmaxintaketemperaturestartup - REAL - read only
[] - dhnumchannels - UINT - read only
[] - dhpsirating - UINT - read only
[] - dhtooltype - UINT - read only
[] - dhtoolvoltage - UINT - read only
[] - downholetoolenabled - BOOL - read only
[] - downtimetimeparameter - DINT - WRITEABLE
[] - downtimetimeparameterol - DINT - WRITEABLE
[] - e300averagecurrent - REAL - read only
[] - e300averagellvoltage - REAL - read only
[] - e300averagelnvoltage - REAL - read only
[] - e300kwh - REAL - read only
[] - e300kwhregen - REAL - read only
[] - e300l1apparentpower - REAL - read only
[] - e300l1current - REAL - read only
[] - e300l1l2voltage - REAL - read only
[] - e300l1nvoltage - REAL - read only
[] - e300l1reactivepower - REAL - read only
[] - e300l1realpower - REAL - read only
[] - e300l1truepowerfactor - REAL - read only
[] - e300l2apparentpower - REAL - read only
[] - e300l2current - REAL - read only
[] - e300l2l3voltage - REAL - read only
[] - e300l2nvoltage - REAL - read only
[] - e300l2reactivepower - REAL - read only
[] - e300l2realpower - REAL - read only
[] - e300l2truepowerfactor - REAL - read only
[] - e300l3apparentpower - REAL - read only
[] - e300l3current - REAL - read only
[] - e300l3l1voltage - REAL - read only
[] - e300l3nvoltage - REAL - read only
[] - e300l3reactivepower - REAL - read only
[] - e300l3realpower - REAL - read only
[] - e300l3truepowerfactor - REAL - read only
[] - e300linefrequency - REAL - read only
[] - e300percentcurrentunbalance - REAL - read only
[] - e300percentvoltageunbalance - REAL - read only
[] - e300threephasetruepowerfactor - REAL - read only
[] - e300totalapparentpower - REAL - read only
[] - e300totalreactivepower - REAL - read only
[] - e300totalrealpower - REAL - read only
[] - handmode - BOOL - read only
[] - overloadtrip - BOOL - read only
[] - pressurealarmdelay - UDINT - WRITEABLE
[] - pressurealarmstartupdelay - DINT - WRITEABLE
[] - pressureeumax - REAL - WRITEABLE
[] - pressureeumin - REAL - WRITEABLE
[] - pressurehi - BOOL - read only
[] - pressurehisp - REAL - WRITEABLE
[] - pressurein - REAL - read only
[] - pressurelo - BOOL - read only
[] - pressurelosp - REAL - WRITEABLE
[] - pressureok - BOOL - read only
[] - pressureshutdown - REAL - WRITEABLE
[] - pressureshutdownenabled - BOOL - WRITEABLE
[] - pressurestartup - REAL - WRITEABLE
[] - pressurestartupenabled - BOOL - WRITEABLE
[] - pressureswitchenabled - BOOL - WRITEABLE
[] - pressuretransducerenabled - BOOL - WRITEABLE
[] - rpmode - BOOL - read only
[] - rppressure - BOOL - read only
[] - rptemperature - BOOL - read only
[] - rptrip - BOOL - read only
[] - rptubingpressure - BOOL - read only
[] - runpermissive - BOOL - read only
[] - shutdowntime - DINT - read only
[] - spmode - BOOL - read only
[] - sppressure - BOOL - read only
[] - sptemperature - BOOL - read only
[] - sptrip - BOOL - read only
[] - spvoltage - BOOL - read only
[] - startbutton - BOOL - read only
[] - startcommand - BOOL - WRITEABLE
[] - startpermissive - BOOL - read only
[] - stopcommand - BOOL - WRITEABLE
[] - tempshutdown - REAL - WRITEABLE
[] - tempshutdownenabled - BOOL - WRITEABLE
[] - tempstartup - REAL - WRITEABLE
[] - tempstartupenabled - BOOL - WRITEABLE
[] - testmode - BOOL - read only
[] - tripenabledicurrentimbalance - BOOL - WRITEABLE
[] - tripenabledigroundfault - BOOL - WRITEABLE
[] - tripenabledijam - BOOL - WRITEABLE
[] - tripenabledilineloss - BOOL - WRITEABLE
[] - tripenablediovercurrent - BOOL - WRITEABLE
[] - tripenabledioverload - BOOL - WRITEABLE
[] - tripenablediphaseloss - BOOL - WRITEABLE
[] - tripenabledistall - BOOL - WRITEABLE
[] - tripenablediundercurrent - BOOL - WRITEABLE
[] - tripenablediunderload - BOOL - WRITEABLE
[] - tripenablevoverfrequency - BOOL - WRITEABLE
[] - tripenablevovervoltage - BOOL - WRITEABLE
[] - tripenablevphaserotation - BOOL - WRITEABLE
[] - tripenablevunderfrequency - BOOL - WRITEABLE
[] - tripenablevundervoltage - BOOL - WRITEABLE
[] - tripenablevvoltageunbalance - BOOL - WRITEABLE
[] - tripresetcmd - BOOL - WRITEABLE
[] - tripstatus - BOOL - read only
[] - tripstatuscontrolint - UINT - read only
[] - tripstatuscurrentint - UINT - read only
[] - tripstatuspowerint - UINT - read only
[] - tripstatusvoltageint - UINT - read only
[] - valoverloadtripcount - DINT - read only
[] - valtripcount - DINT - read only
[] - voltageok - BOOL - read only
[] - warningenabledicurrentimbalanc - BOOL - WRITEABLE
[] - warningenabledigroundfault - BOOL - WRITEABLE
[] - warningenabledijam - BOOL - WRITEABLE
[] - warningenabledilineloss - BOOL - WRITEABLE
[] - warningenablediovercurrent - BOOL - WRITEABLE
[] - warningenabledioverload - BOOL - WRITEABLE
[] - warningenablediphaseloss - BOOL - WRITEABLE
[] - warningenabledistall - BOOL - WRITEABLE
[] - warningenablediundercurrent - BOOL - WRITEABLE
[] - warningenablediunderload - BOOL - WRITEABLE
[] - warningenablevoverfrequency - BOOL - WRITEABLE
[] - warningenablevovervoltage - BOOL - WRITEABLE
[] - warningenablevphaserotation - BOOL - WRITEABLE
[] - warningenablevunderfrequency - BOOL - WRITEABLE
[] - warningenablevundervoltage - BOOL - WRITEABLE
[] - warningenablevvoltageunbalance - BOOL - WRITEABLE
[] - warningstatus - BOOL - read only
[] - warningstatuscontrolint - UINT - read only
[] - warningstatuscurrentint - UINT - read only
[] - warningstatuspowerint - UINT - read only
[] - warningstatusvoltageint - UINT - read only
