def ipp_cfgcflasetting(self, name, value):
	print('trying to set cfg_C_FLASetting to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_C_FLASetting', float(value))

def ipp_cfgcleartripcountafter(self, name, value):
	print('trying to set cfg_ClearTripCountAfter to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_ClearTripCountAfter', int(value))

def ipp_cfgctripenablecontrol(self, name, value):
	print('trying to set cfg_C_TripEnableControl to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_C_TripEnableControl', int(value))

def ipp_cfgcwarningenablecontrol(self, name, value):
	print('trying to set cfg_C_WarningEnableControl to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_C_WarningEnableControl', int(value))

def ipp_cfggfgroundfaultinhibittime(self, name, value):
	print('trying to set cfg_GF_GroundFaultInhibitTime to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_GF_GroundFaultInhibitTime', int(value))

def ipp_cfggfgroundfaulttripdelay(self, name, value):
	print('trying to set cfg_GF_GroundFaultTripDelay to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_GF_GroundFaultTripDelay', float(value))

def ipp_cfggfgroundfaulttriplevel(self, name, value):
	print('trying to set cfg_GF_GroundFaultTripLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_GF_GroundFaultTripLevel', float(value))

def ipp_cfggfgroundfaultwarningdelay(self, name, value):
	print('trying to set cfg_GF_GroundFaultWarningDelay to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_GF_GroundFaultWarningDelay', float(value))

def ipp_cfggfgroundfaultwarninglevel(self, name, value):
	print('trying to set cfg_GF_GroundFaultWarningLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_GF_GroundFaultWarningLevel', float(value))

def ipp_cfgictprimary(self, name, value):
	print('trying to set cfg_I_CTPrimary to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_CTPrimary', int(value))

def ipp_cfgictsecondary(self, name, value):
	print('trying to set cfg_I_CTSecondary to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_CTSecondary', int(value))

def ipp_cfgicurrentimbalanceinhibittim(self, name, value):
	print('trying to set cfg_I_CurrentImbalanceInhibitTime to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_CurrentImbalanceInhibitTime', int(value))

def ipp_cfgicurrentimbalancetripdelay(self, name, value):
	print('trying to set cfg_I_CurrentImbalanceTripDelay to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_CurrentImbalanceTripDelay', int(value))

def ipp_cfgicurrentimbalancetriplevel(self, name, value):
	print('trying to set cfg_I_CurrentImbalanceTripLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_CurrentImbalanceTripLevel', int(value))

def ipp_cfgicurrentimbalancewarninglev(self, name, value):
	print('trying to set cfg_I_CurrentImbalanceWarningLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_CurrentImbalanceWarningLevel', int(value))

def ipp_cfgijaminhibittime(self, name, value):
	print('trying to set cfg_I_JamInhibitTime to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_JamInhibitTime', int(value))

def ipp_cfgijamtripdelay(self, name, value):
	print('trying to set cfg_I_JamTripDelay to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_JamTripDelay', int(value))

def ipp_cfgijamwarninglevel(self, name, value):
	print('trying to set cfg_I_JamWarningLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_JamWarningLevel', int(value))

def ipp_cfgilinelossinhibittime(self, name, value):
	print('trying to set cfg_I_LineLossInhibitTime to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_LineLossInhibitTime', int(value))

def ipp_cfgilinelosstripdelay(self, name, value):
	print('trying to set cfg_I_LineLossTripDelay to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_LineLossTripDelay', float(value))

def ipp_cfgiovercurrentinhibittime(self, name, value):
	print('trying to set cfg_I_OvercurrentInhibitTime to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_OvercurrentInhibitTime', int(value))

def ipp_cfgiovercurrenttripdelay(self, name, value):
	print('trying to set cfg_I_OvercurrentTripDelay to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_OvercurrentTripDelay', float(value))

def ipp_cfgiovercurrenttriplevel(self, name, value):
	print('trying to set cfg_I_OvercurrentTripLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_OvercurrentTripLevel', int(value))

def ipp_cfgiovercurrentwarninglevel(self, name, value):
	print('trying to set cfg_I_OvercurrentWarningLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_OvercurrentWarningLevel', int(value))

def ipp_cfgistallenabledtime(self, name, value):
	print('trying to set cfg_I_StallEnabledTime to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_StallEnabledTime', int(value))

def ipp_cfgistalltriplevel(self, name, value):
	print('trying to set cfg_I_StallTripLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_StallTripLevel', int(value))

def ipp_cfgiundercurrentinhibittime(self, name, value):
	print('trying to set cfg_I_UndercurrentInhibitTime to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_UndercurrentInhibitTime', int(value))

def ipp_cfgiundercurrenttripdelay(self, name, value):
	print('trying to set cfg_I_UndercurrentTripDelay to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_UndercurrentTripDelay', float(value))

def ipp_cfgiundercurrenttriplevel(self, name, value):
	print('trying to set cfg_I_UndercurrentTripLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_UndercurrentTripLevel', int(value))

def ipp_cfgiundercurrentwarninglevel(self, name, value):
	print('trying to set cfg_I_UndercurrentWarningLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_UndercurrentWarningLevel', int(value))

def ipp_cfgiunderloadinhibittime(self, name, value):
	print('trying to set cfg_I_UnderloadInhibitTime to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_UnderloadInhibitTime', int(value))

def ipp_cfgiunderloadtripdelay(self, name, value):
	print('trying to set cfg_I_UnderloadTripDelay to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_UnderloadTripDelay', float(value))

def ipp_cfgiunderloadtriplevel(self, name, value):
	print('trying to set cfg_I_UnderloadTripLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_UnderloadTripLevel', int(value))

def ipp_cfgiunderloadwarninglevel(self, name, value):
	print('trying to set cfg_I_UnderloadWarningLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_I_UnderloadWarningLevel', int(value))

def ipp_cfgoverloadtripcountlimit(self, name, value):
	print('trying to set cfg_OverloadTripCountLimit to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_OverloadTripCountLimit', int(value))

def ipp_cfgplphaselossinhibittime(self, name, value):
	print('trying to set cfg_PL_PhaseLossInhibitTime to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_PL_PhaseLossInhibitTime', int(value))

def ipp_cfgplphaselosstripdelay(self, name, value):
	print('trying to set cfg_PL_PhaseLossTripDelay to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_PL_PhaseLossTripDelay', float(value))

def ipp_cfgread(self, name, value):
	print('trying to set cfg_READ to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_READ', int(value))

def ipp_cfgspecificgravity(self, name, value):
	print('trying to set cfg_SpecificGravity to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_SpecificGravity', float(value))

def ipp_cfgtcutripclass(self, name, value):
	print('trying to set cfg_TCU_TripClass to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_TCU_TripClass', int(value))

def ipp_cfgtimermodeenabled(self, name, value):
	print('trying to set cfg_TimerModeEnabled to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_TimerModeEnabled', int(value))

def ipp_cfgtimerruntime(self, name, value):
	print('trying to set cfg_TimerRunTime to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_TimerRunTime', int(value))

def ipp_cfgtimerwaittime(self, name, value):
	print('trying to set cfg_TimerWaitTime to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_TimerWaitTime', int(value))

def ipp_cfgtripcountlimit(self, name, value):
	print('trying to set cfg_TripCountLimit to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_TripCountLimit', int(value))

def ipp_cfgvoverfrequencyinhibittime(self, name, value):
	print('trying to set cfg_V_OverfrequencyInhibitTime to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_OverfrequencyInhibitTime', int(value))

def ipp_cfgvoverfrequencytripdelay(self, name, value):
	print('trying to set cfg_V_OverfrequencyTripDelay to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_OverfrequencyTripDelay', float(value))

def ipp_cfgvoverfrequencytriplevel(self, name, value):
	print('trying to set cfg_V_OverfrequencyTripLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_OverfrequencyTripLevel', int(value))

def ipp_cfgvoverfrequencywarninglevel(self, name, value):
	print('trying to set cfg_V_OverfrequencyWarningLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_OverfrequencyWarningLevel', int(value))

def ipp_cfgvovervoltageinhibittime(self, name, value):
	print('trying to set cfg_V_OvervoltageInhibitTime to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_OvervoltageInhibitTime', int(value))

def ipp_cfgvovervoltagetripdelay(self, name, value):
	print('trying to set cfg_V_OvervoltageTripDelay to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_OvervoltageTripDelay', float(value))

def ipp_cfgvovervoltagetriplevel(self, name, value):
	print('trying to set cfg_V_OvervoltageTripLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_OvervoltageTripLevel', float(value))

def ipp_cfgvovervoltagewarninglevel(self, name, value):
	print('trying to set cfg_V_OvervoltageWarningLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_OvervoltageWarningLevel', float(value))

def ipp_cfgvphaserotationinhibittime(self, name, value):
	print('trying to set cfg_V_PhaseRotationInhibitTime to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_PhaseRotationInhibitTime', int(value))

def ipp_cfgvphaserotationtriptype(self, name, value):
	print('trying to set cfg_V_PhaseRotationTripType to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_PhaseRotationTripType', int(value))

def ipp_cfgvptprimary(self, name, value):
	print('trying to set cfg_V_PTPrimary to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_PTPrimary', int(value))

def ipp_cfgvptsecondary(self, name, value):
	print('trying to set cfg_V_PTSecondary to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_PTSecondary', int(value))

def ipp_cfgvunderfrequencyinhibittime(self, name, value):
	print('trying to set cfg_V_UnderfrequencyInhibitTime to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_UnderfrequencyInhibitTime', int(value))

def ipp_cfgvunderfrequencytripdelay(self, name, value):
	print('trying to set cfg_V_UnderfrequencyTripDelay to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_UnderfrequencyTripDelay', float(value))

def ipp_cfgvunderfrequencytriplevel(self, name, value):
	print('trying to set cfg_V_UnderfrequencyTripLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_UnderfrequencyTripLevel', int(value))

def ipp_cfgvunderfrequencywarninglevel(self, name, value):
	print('trying to set cfg_V_UnderfrequencyWarningLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_UnderfrequencyWarningLevel', int(value))

def ipp_cfgvundervoltageinhibittime(self, name, value):
	print('trying to set cfg_V_UndervoltageInhibitTime to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_UndervoltageInhibitTime', int(value))

def ipp_cfgvundervoltagetripdelay(self, name, value):
	print('trying to set cfg_V_UndervoltageTripDelay to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_UndervoltageTripDelay', float(value))

def ipp_cfgvundervoltagetriplevel(self, name, value):
	print('trying to set cfg_V_UndervoltageTripLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_UndervoltageTripLevel', float(value))

def ipp_cfgvundervoltagewarninglevel(self, name, value):
	print('trying to set cfg_V_UndervoltageWarningLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_UndervoltageWarningLevel', float(value))

def ipp_cfgvvoltageimbalanceinhibittim(self, name, value):
	print('trying to set cfg_V_VoltageImbalanceInhibitTime to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_VoltageImbalanceInhibitTime', int(value))

def ipp_cfgvvoltageimbalancetripdelay(self, name, value):
	print('trying to set cfg_V_VoltageImbalanceTripDelay to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_VoltageImbalanceTripDelay', float(value))

def ipp_cfgvvoltageimbalancetriplevel(self, name, value):
	print('trying to set cfg_V_VoltageImbalanceTripLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_VoltageImbalanceTripLevel', int(value))

def ipp_cfgvvoltageimbalancewarninglev(self, name, value):
	print('trying to set cfg_V_VoltageImbalanceWarningLevel to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_VoltageImbalanceWarningLevel', int(value))

def ipp_cfgvvoltagemode(self, name, value):
	print('trying to set cfg_V_VoltageMode to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_V_VoltageMode', int(value))

def ipp_cfgwrite(self, name, value):
	print('trying to set cfg_WRITE to {}'.format(value))
	return u800.writeMicroTag(addr, 'cfg_WRITE', int(value))

def ipp_downtimetimeparameter(self, name, value):
	print('trying to set Downtime_Time_Parameter to {}'.format(value))
	return u800.writeMicroTag(addr, 'Downtime_Time_Parameter', int(value))

def ipp_downtimetimeparameterol(self, name, value):
	print('trying to set Downtime_Time_Parameter_OL to {}'.format(value))
	return u800.writeMicroTag(addr, 'Downtime_Time_Parameter_OL', int(value))

def ipp_pressurealarmdelay(self, name, value):
	print('trying to set Pressure_Alarm_Delay to {}'.format(value))
	return u800.writeMicroTag(addr, 'Pressure_Alarm_Delay', int(value))

def ipp_pressurealarmstartupdelay(self, name, value):
	print('trying to set Pressure_Alarm_Startup_Delay to {}'.format(value))
	return u800.writeMicroTag(addr, 'Pressure_Alarm_Startup_Delay', int(value))

def ipp_pressureeumax(self, name, value):
	print('trying to set Pressure_EU_Max to {}'.format(value))
	return u800.writeMicroTag(addr, 'Pressure_EU_Max', float(value))

def ipp_pressureeumin(self, name, value):
	print('trying to set Pressure_EU_Min to {}'.format(value))
	return u800.writeMicroTag(addr, 'Pressure_EU_Min', float(value))

def ipp_pressurehisp(self, name, value):
	print('trying to set Pressure_Hi_SP to {}'.format(value))
	return u800.writeMicroTag(addr, 'Pressure_Hi_SP', float(value))

def ipp_pressurelosp(self, name, value):
	print('trying to set Pressure_Lo_SP to {}'.format(value))
	return u800.writeMicroTag(addr, 'Pressure_Lo_SP', float(value))

def ipp_pressureshutdown(self, name, value):
	print('trying to set Pressure_Shutdown to {}'.format(value))
	return u800.writeMicroTag(addr, 'Pressure_Shutdown', float(value))

def ipp_pressureshutdownenabled(self, name, value):
	print('trying to set Pressure_Shutdown_Enabled to {}'.format(value))
	return u800.writeMicroTag(addr, 'Pressure_Shutdown_Enabled', int(value))

def ipp_pressurestartup(self, name, value):
	print('trying to set Pressure_Startup to {}'.format(value))
	return u800.writeMicroTag(addr, 'Pressure_Startup', float(value))

def ipp_pressurestartupenabled(self, name, value):
	print('trying to set Pressure_Startup_Enabled to {}'.format(value))
	return u800.writeMicroTag(addr, 'Pressure_Startup_Enabled', int(value))

def ipp_pressureswitchenabled(self, name, value):
	print('trying to set Pressure_Switch_Enabled to {}'.format(value))
	return u800.writeMicroTag(addr, 'Pressure_Switch_Enabled', int(value))

def ipp_pressuretransducerenabled(self, name, value):
	print('trying to set Pressure_Transducer_Enabled to {}'.format(value))
	return u800.writeMicroTag(addr, 'Pressure_Transducer_Enabled', int(value))

def ipp_startcommand(self, name, value):
	print('trying to set Start_Command to {}'.format(value))
	return u800.writeMicroTag(addr, 'Start_Command', int(value))

def ipp_stopcommand(self, name, value):
	print('trying to set Stop_Command to {}'.format(value))
	return u800.writeMicroTag(addr, 'Stop_Command', int(value))

def ipp_tempshutdown(self, name, value):
	print('trying to set Temp_Shutdown to {}'.format(value))
	return u800.writeMicroTag(addr, 'Temp_Shutdown', float(value))

def ipp_tempshutdownenabled(self, name, value):
	print('trying to set Temp_Shutdown_Enabled to {}'.format(value))
	return u800.writeMicroTag(addr, 'Temp_Shutdown_Enabled', int(value))

def ipp_tempstartup(self, name, value):
	print('trying to set Temp_Startup to {}'.format(value))
	return u800.writeMicroTag(addr, 'Temp_Startup', float(value))

def ipp_tempstartupenabled(self, name, value):
	print('trying to set Temp_Startup_Enabled to {}'.format(value))
	return u800.writeMicroTag(addr, 'Temp_Startup_Enabled', int(value))

def ipp_tripenabledicurrentimbalance(self, name, value):
	print('trying to set TripEnabled_I_CurrentImbalance to {}'.format(value))
	return u800.writeMicroTag(addr, 'TripEnabled_I_CurrentImbalance', int(value))

def ipp_tripenabledigroundfault(self, name, value):
	print('trying to set TripEnabled_I_GroundFault to {}'.format(value))
	return u800.writeMicroTag(addr, 'TripEnabled_I_GroundFault', int(value))

def ipp_tripenabledijam(self, name, value):
	print('trying to set TripEnabled_I_Jam to {}'.format(value))
	return u800.writeMicroTag(addr, 'TripEnabled_I_Jam', int(value))

def ipp_tripenabledilineloss(self, name, value):
	print('trying to set TripEnabled_I_LineLoss to {}'.format(value))
	return u800.writeMicroTag(addr, 'TripEnabled_I_LineLoss', int(value))

def ipp_tripenablediovercurrent(self, name, value):
	print('trying to set TripEnabled_I_Overcurrent to {}'.format(value))
	return u800.writeMicroTag(addr, 'TripEnabled_I_Overcurrent', int(value))

def ipp_tripenabledioverload(self, name, value):
	print('trying to set TripEnabled_I_Overload to {}'.format(value))
	return u800.writeMicroTag(addr, 'TripEnabled_I_Overload', int(value))

def ipp_tripenablediphaseloss(self, name, value):
	print('trying to set TripEnabled_I_PhaseLoss to {}'.format(value))
	return u800.writeMicroTag(addr, 'TripEnabled_I_PhaseLoss', int(value))

def ipp_tripenabledistall(self, name, value):
	print('trying to set TripEnabled_I_Stall to {}'.format(value))
	return u800.writeMicroTag(addr, 'TripEnabled_I_Stall', int(value))

def ipp_tripenablediundercurrent(self, name, value):
	print('trying to set TripEnabled_I_Undercurrent to {}'.format(value))
	return u800.writeMicroTag(addr, 'TripEnabled_I_Undercurrent', int(value))

def ipp_tripenablediunderload(self, name, value):
	print('trying to set TripEnabled_I_Underload to {}'.format(value))
	return u800.writeMicroTag(addr, 'TripEnabled_I_Underload', int(value))

def ipp_tripenablevoverfrequency(self, name, value):
	print('trying to set TripEnable_V_Overfrequency to {}'.format(value))
	return u800.writeMicroTag(addr, 'TripEnable_V_Overfrequency', int(value))

def ipp_tripenablevovervoltage(self, name, value):
	print('trying to set TripEnable_V_Overvoltage to {}'.format(value))
	return u800.writeMicroTag(addr, 'TripEnable_V_Overvoltage', int(value))

def ipp_tripenablevphaserotation(self, name, value):
	print('trying to set TripEnable_V_PhaseRotation to {}'.format(value))
	return u800.writeMicroTag(addr, 'TripEnable_V_PhaseRotation', int(value))

def ipp_tripenablevunderfrequency(self, name, value):
	print('trying to set TripEnable_V_Underfrequency to {}'.format(value))
	return u800.writeMicroTag(addr, 'TripEnable_V_Underfrequency', int(value))

def ipp_tripenablevundervoltage(self, name, value):
	print('trying to set TripEnable_V_Undervoltage to {}'.format(value))
	return u800.writeMicroTag(addr, 'TripEnable_V_Undervoltage', int(value))

def ipp_tripenablevvoltageunbalance(self, name, value):
	print('trying to set TripEnable_V_VoltageUnbalance to {}'.format(value))
	return u800.writeMicroTag(addr, 'TripEnable_V_VoltageUnbalance', int(value))

def ipp_tripresetcmd(self, name, value):
	print('trying to set TripResetCmd to {}'.format(value))
	return u800.writeMicroTag(addr, 'TripResetCmd', int(value))

def ipp_warningenabledicurrentimbalanc(self, name, value):
	print('trying to set WarningEnabled_I_CurrentImbalance to {}'.format(value))
	return u800.writeMicroTag(addr, 'WarningEnabled_I_CurrentImbalance', int(value))

def ipp_warningenabledigroundfault(self, name, value):
	print('trying to set WarningEnabled_I_GroundFault to {}'.format(value))
	return u800.writeMicroTag(addr, 'WarningEnabled_I_GroundFault', int(value))

def ipp_warningenabledijam(self, name, value):
	print('trying to set WarningEnabled_I_Jam to {}'.format(value))
	return u800.writeMicroTag(addr, 'WarningEnabled_I_Jam', int(value))

def ipp_warningenabledilineloss(self, name, value):
	print('trying to set WarningEnabled_I_LineLoss to {}'.format(value))
	return u800.writeMicroTag(addr, 'WarningEnabled_I_LineLoss', int(value))

def ipp_warningenablediovercurrent(self, name, value):
	print('trying to set WarningEnabled_I_Overcurrent to {}'.format(value))
	return u800.writeMicroTag(addr, 'WarningEnabled_I_Overcurrent', int(value))

def ipp_warningenabledioverload(self, name, value):
	print('trying to set WarningEnabled_I_Overload to {}'.format(value))
	return u800.writeMicroTag(addr, 'WarningEnabled_I_Overload', int(value))

def ipp_warningenablediphaseloss(self, name, value):
	print('trying to set WarningEnabled_I_PhaseLoss to {}'.format(value))
	return u800.writeMicroTag(addr, 'WarningEnabled_I_PhaseLoss', int(value))

def ipp_warningenabledistall(self, name, value):
	print('trying to set WarningEnabled_I_Stall to {}'.format(value))
	return u800.writeMicroTag(addr, 'WarningEnabled_I_Stall', int(value))

def ipp_warningenablediundercurrent(self, name, value):
	print('trying to set WarningEnabled_I_Undercurrent to {}'.format(value))
	return u800.writeMicroTag(addr, 'WarningEnabled_I_Undercurrent', int(value))

def ipp_warningenablediunderload(self, name, value):
	print('trying to set WarningEnabled_I_Underload to {}'.format(value))
	return u800.writeMicroTag(addr, 'WarningEnabled_I_Underload', int(value))

def ipp_warningenablevoverfrequency(self, name, value):
	print('trying to set WarningEnable_V_Overfrequency to {}'.format(value))
	return u800.writeMicroTag(addr, 'WarningEnable_V_Overfrequency', int(value))

def ipp_warningenablevovervoltage(self, name, value):
	print('trying to set WarningEnable_V_Overvoltage to {}'.format(value))
	return u800.writeMicroTag(addr, 'WarningEnable_V_Overvoltage', int(value))

def ipp_warningenablevphaserotation(self, name, value):
	print('trying to set WarningEnable_V_PhaseRotation to {}'.format(value))
	return u800.writeMicroTag(addr, 'WarningEnable_V_PhaseRotation', int(value))

def ipp_warningenablevunderfrequency(self, name, value):
	print('trying to set WarningEnable_V_Underfrequency to {}'.format(value))
	return u800.writeMicroTag(addr, 'WarningEnable_V_Underfrequency', int(value))

def ipp_warningenablevundervoltage(self, name, value):
	print('trying to set WarningEnable_V_Undervoltage to {}'.format(value))
	return u800.writeMicroTag(addr, 'WarningEnable_V_Undervoltage', int(value))

def ipp_warningenablevvoltageunbalance(self, name, value):
	print('trying to set WarningEnable_V_VoltageUnbalance to {}'.format(value))
	return u800.writeMicroTag(addr, 'WarningEnable_V_VoltageUnbalance', int(value))

