[BEGIN FB INPUTS]
I1=micro820.micro820.e300data/e300_output.prodname_cop.enable,0x460,BOOL
I2=micro820.micro820.e300data/e300_output.prodname_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I3=micro820.micro820.e300data/e300_output.prodname_cop.srcoffset,0x5604,UINT
I4=micro820.micro820.e300data/e300_output.prodname_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I5=micro820.micro820.e300data/e300_output.prodname_cop.destoffset,0x5604,UINT
I6=micro820.micro820.e300data/e300_output.prodname_cop.length,0x5600,UINT
I7=micro820.micro820.e300data/e300_output.prodname_cop.swap,0x461,BOOL
I8=micro820.micro820.e300data/e300_output.prodname_cop.__adi_src,0xFFFFFFFF,UINT
I9=micro820.micro820.e300data/e300_output.prodname_cop.__adi_dest,0xFFFFFFFF,UINT
I10=micro820.micro820.e300data/e300_output.prodname_cop.__dti_src,0xFFFFFFFF,SINT
I11=micro820.micro820.e300data/e300_output.prodname_cop.__dti_dest,0xFFFFFFFF,SINT
I12=micro820.micro820.e300data/e300_readenergy.phase_cop.enable,0x460,BOOL
I13=micro820.micro820.e300data/e300_readenergy.phase_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I14=micro820.micro820.e300data/e300_readenergy.phase_cop.srcoffset,0x55E2,UINT
I15=micro820.micro820.e300data/e300_readenergy.phase_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I16=micro820.micro820.e300data/e300_readenergy.phase_cop.destoffset,0x55E8,UINT
I17=micro820.micro820.e300data/e300_readenergy.phase_cop.length,0x5600,UINT
I18=micro820.micro820.e300data/e300_readenergy.phase_cop.swap,0x460,BOOL
I19=micro820.micro820.e300data/e300_readenergy.phase_cop.__adi_src,0xFFFFFFFF,UINT
I20=micro820.micro820.e300data/e300_readenergy.phase_cop.__adi_dest,0xFFFFFFFF,UINT
I21=micro820.micro820.e300data/e300_readenergy.phase_cop.__dti_src,0xFFFFFFFF,SINT
I22=micro820.micro820.e300data/e300_readenergy.phase_cop.__dti_dest,0xFFFFFFFF,SINT
I23=micro820.micro820.e300data/e300_readenergy.prodname_cop.enable,0x460,BOOL
I24=micro820.micro820.e300data/e300_readenergy.prodname_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I25=micro820.micro820.e300data/e300_readenergy.prodname_cop.srcoffset,0x5604,UINT
I26=micro820.micro820.e300data/e300_readenergy.prodname_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I27=micro820.micro820.e300data/e300_readenergy.prodname_cop.destoffset,0x5604,UINT
I28=micro820.micro820.e300data/e300_readenergy.prodname_cop.length,0x5600,UINT
I29=micro820.micro820.e300data/e300_readenergy.prodname_cop.swap,0x461,BOOL
I30=micro820.micro820.e300data/e300_readenergy.prodname_cop.__adi_src,0xFFFFFFFF,UINT
I31=micro820.micro820.e300data/e300_readenergy.prodname_cop.__adi_dest,0xFFFFFFFF,UINT
I32=micro820.micro820.e300data/e300_readenergy.prodname_cop.__dti_src,0xFFFFFFFF,SINT
I33=micro820.micro820.e300data/e300_readenergy.prodname_cop.__dti_dest,0xFFFFFFFF,SINT
I34=micro820.micro820.e300data/e300_readenergy.real_cop.enable,0x460,BOOL
I35=micro820.micro820.e300data/e300_readenergy.real_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I36=micro820.micro820.e300data/e300_readenergy.real_cop.srcoffset,0x55E6,UINT
I37=micro820.micro820.e300data/e300_readenergy.real_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I38=micro820.micro820.e300data/e300_readenergy.real_cop.destoffset,0x5604,UINT
I39=micro820.micro820.e300data/e300_readenergy.real_cop.length,0x55E4,UINT
I40=micro820.micro820.e300data/e300_readenergy.real_cop.swap,0x460,BOOL
I41=micro820.micro820.e300data/e300_readenergy.real_cop.__adi_src,0xFFFFFFFF,UINT
I42=micro820.micro820.e300data/e300_readenergy.real_cop.__adi_dest,0xFFFFFFFF,UINT
I43=micro820.micro820.e300data/e300_readenergy.real_cop.__dti_src,0xFFFFFFFF,SINT
I44=micro820.micro820.e300data/e300_readenergy.real_cop.__dti_dest,0xFFFFFFFF,SINT
I45=micro820.micro820.e300data/e300_readenergy.int_cop.enable,0x460,BOOL
I46=micro820.micro820.e300data/e300_readenergy.int_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I47=micro820.micro820.e300data/e300_readenergy.int_cop.srcoffset,0x5604,UINT
I48=micro820.micro820.e300data/e300_readenergy.int_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I49=micro820.micro820.e300data/e300_readenergy.int_cop.destoffset,0x5604,UINT
I50=micro820.micro820.e300data/e300_readenergy.int_cop.length,0x55E8,UINT
I51=micro820.micro820.e300data/e300_readenergy.int_cop.swap,0x460,BOOL
I52=micro820.micro820.e300data/e300_readenergy.int_cop.__adi_src,0xFFFFFFFF,UINT
I53=micro820.micro820.e300data/e300_readenergy.int_cop.__adi_dest,0xFFFFFFFF,UINT
I54=micro820.micro820.e300data/e300_readenergy.int_cop.__dti_src,0xFFFFFFFF,SINT
I55=micro820.micro820.e300data/e300_readenergy.int_cop.__dti_dest,0xFFFFFFFF,SINT
I56=micro820.micro820.readdownholedata/modbuscycletimer.in,0x5541,BOOL
I57=micro820.micro820.readdownholedata/modbuscycletimer.pt,0x794,TIME
I58=micro820.micro820.flowtotalizer/ton_totalizer.in,0x5541,BOOL
I59=micro820.micro820.flowtotalizer/ton_totalizer.pt,0x7A64,TIME
I60=micro820.micro820.e300data/writee300configdata.fben,0x460,BOOL
I61=micro820.micro820.e300data/writee300configdata.ipaddress,0x8F8,STRING
I62=micro820.micro820.e300data/writee300configdata.updaterate_ms,0x51A,UINT
I63=micro820.micro820.e300data/writee300configdata.enable,0x460,BOOL
I64=micro820.micro820.e300data/writee300configdata.input,0xFFFFFFFF,____FB_INIT_CONST_00000010
I65=micro820.micro820.e300data/s2u_underpflagtriplevel.inp_int,0x4CA,SINT
I66=micro820.micro820.e300data/s2u_underpflagwarninglevel.inp_int,0x4CB,SINT
I67=micro820.micro820.e300data/s2u_overpflagtriplevel.inp_int,0x4CC,SINT
I68=micro820.micro820.e300data/s2u_overpflagwarninglevel.inp_int,0x5586,SINT
I69=micro820.micro820.e300data/sint_to_dint_flasetting.sint_src_1,0x5594,USINT
I70=micro820.micro820.e300data/sint_to_dint_flasetting.sint_src_2,0x5595,USINT
I71=micro820.micro820.e300data/sint_to_dint_flasetting.sint_src_3,0x5596,USINT
I72=micro820.micro820.e300data/sint_to_dint_flasetting.sint_src_4,0x5597,USINT
I73=micro820.micro820.e300data/e300_output.fben,0x4B5,BOOL
I74=micro820.micro820.e300data/e300_output.ipaddress,0x8F8,STRING
I75=micro820.micro820.e300data/e300_output.outputnumber,0x4CE,USINT
I76=micro820.micro820.e300data/e300_output.outputsetting,0x464,BOOL
I77=micro820.micro820.currenttimertc.rtc_read_enabled,0x460,BOOL
I78=micro820.micro820.e300data/d2s_flasetting.inp_dint,0x5D80,UDINT
I79=micro820.micro820.e300data/writee300configdata.fben_ftrig.clk,0x5551,BOOL
I80=micro820.micro820.e300data/e300_output.outputsetting_ftrig.clk,0x5551,BOOL
I81=micro820.micro820.e300data/e300_output.fben_ftrig.clk,0x5551,BOOL
I82=micro820.micro820.e300data/e300_readenergy.fben_ftrig.clk,0x5551,BOOL
I83=micro820.micro820.e300data/e300_read_digitalinput0.fben_ftrig.clk,0x5551,BOOL
I84=micro820.micro820.e300data/reade300configdata.fben_ftrig.clk,0x5551,BOOL
I85=micro820.micro820.e300data/e300_tripstatuscurrent.fben_ftrig.clk,0x5551,BOOL
I86=micro820.micro820.e300data/e300_write_tripreset.fben_ftrig.clk,0x5551,BOOL
I87=micro820.micro820.e300data/e300_read_digitalinput1.fben_ftrig.clk,0x5551,BOOL
I88=micro820.micro820.e300data/e300_tripstatusvoltage.fben_ftrig.clk,0x5551,BOOL
I89=micro820.micro820.e300data/e300_read_digitalinput2.fben_ftrig.clk,0x5551,BOOL
I90=micro820.micro820.e300data/e300_tripstatuspower.fben_ftrig.clk,0x5551,BOOL
I91=micro820.micro820.e300data/e300_read_digitalinput3.fben_ftrig.clk,0x5551,BOOL
I92=micro820.micro820.e300data/e300_tripstatuscontrol.fben_ftrig.clk,0x5551,BOOL
I93=micro820.micro820.e300data/e300_read_digitalinput4.fben_ftrig.clk,0x5551,BOOL
I94=micro820.micro820.e300data/e300_warnstatuscurrent.fben_ftrig.clk,0x5551,BOOL
I95=micro820.micro820.e300data/e300_read_digitalinput5.fben_ftrig.clk,0x5551,BOOL
I96=micro820.micro820.e300data/e300_warnstatusvoltage.fben_ftrig.clk,0x5551,BOOL
I97=micro820.micro820.e300data/e300_warnstatuspower.fben_ftrig.clk,0x5551,BOOL
I98=micro820.micro820.e300data/e300_warnstatuscontrol.fben_ftrig.clk,0x5551,BOOL
I99=micro820.micro820.e300data/e300_readenergy.fben,0x460,BOOL
I100=micro820.micro820.e300data/e300_readenergy.ipaddress,0x8F8,STRING
I101=micro820.micro820.e300data/e300_readenergy.updaterate_ms,0x51A,UINT
I102=micro820.micro820.e300data/sint_to_dint_underrealpowertriplevel.sint_src_1,0x5598,USINT
I103=micro820.micro820.e300data/sint_to_dint_underrealpowertriplevel.sint_src_2,0x5599,USINT
I104=micro820.micro820.e300data/sint_to_dint_underrealpowertriplevel.sint_src_3,0x559A,USINT
I105=micro820.micro820.e300data/sint_to_dint_underrealpowertriplevel.sint_src_4,0x559B,USINT
I106=micro820.micro820.e300data/sint_to_dint_underrealpowerwarninglevel.sint_src_1,0x5598,USINT
I107=micro820.micro820.e300data/sint_to_dint_underrealpowerwarninglevel.sint_src_2,0x5599,USINT
I108=micro820.micro820.e300data/sint_to_dint_underrealpowerwarninglevel.sint_src_3,0x559A,USINT
I109=micro820.micro820.e300data/sint_to_dint_underrealpowerwarninglevel.sint_src_4,0x559B,USINT
I110=micro820.micro820.e300data/sint_to_dint_overrealpowertriplevel.sint_src_1,0x5598,USINT
I111=micro820.micro820.e300data/sint_to_dint_overrealpowertriplevel.sint_src_2,0x5599,USINT
I112=micro820.micro820.e300data/sint_to_dint_overrealpowertriplevel.sint_src_3,0x559A,USINT
I113=micro820.micro820.e300data/sint_to_dint_overrealpowertriplevel.sint_src_4,0x559B,USINT
I114=micro820.micro820.e300data/sint_to_dint_overrealpowerwarninglevel.sint_src_1,0x5598,USINT
I115=micro820.micro820.e300data/sint_to_dint_overrealpowerwarninglevel.sint_src_2,0x5599,USINT
I116=micro820.micro820.e300data/sint_to_dint_overrealpowerwarninglevel.sint_src_3,0x559A,USINT
I117=micro820.micro820.e300data/sint_to_dint_overrealpowerwarninglevel.sint_src_4,0x559B,USINT
I118=micro820.micro820.e300data/sint_to_dint_underreactiveconstriplevel.sint_src_1,0x5598,USINT
I119=micro820.micro820.e300data/sint_to_dint_underreactiveconstriplevel.sint_src_2,0x5599,USINT
I120=micro820.micro820.e300data/sint_to_dint_underreactiveconstriplevel.sint_src_3,0x559A,USINT
I121=micro820.micro820.e300data/sint_to_dint_underreactiveconstriplevel.sint_src_4,0x559B,USINT
I122=micro820.micro820.e300data/sint_to_dint_underreactiveconswlevel.sint_src_1,0x5598,USINT
I123=micro820.micro820.e300data/sint_to_dint_underreactiveconswlevel.sint_src_2,0x5599,USINT
I124=micro820.micro820.e300data/sint_to_dint_underreactiveconswlevel.sint_src_3,0x559A,USINT
I125=micro820.micro820.e300data/sint_to_dint_underreactiveconswlevel.sint_src_4,0x559B,USINT
I126=micro820.micro820.e300data/sint_to_dint_oreactiveconstriplevel.sint_src_1,0x5598,USINT
I127=micro820.micro820.e300data/sint_to_dint_oreactiveconstriplevel.sint_src_2,0x5599,USINT
I128=micro820.micro820.e300data/sint_to_dint_oreactiveconstriplevel.sint_src_3,0x559A,USINT
I129=micro820.micro820.e300data/sint_to_dint_oreactiveconstriplevel.sint_src_4,0x559B,USINT
I130=micro820.micro820.e300data/sint_to_dint_oreactiveconswarninglevel.sint_src_1,0x5598,USINT
I131=micro820.micro820.e300data/sint_to_dint_oreactiveconswarninglevel.sint_src_2,0x5599,USINT
I132=micro820.micro820.e300data/sint_to_dint_oreactiveconswarninglevel.sint_src_3,0x559A,USINT
I133=micro820.micro820.e300data/sint_to_dint_oreactiveconswarninglevel.sint_src_4,0x559B,USINT
I134=micro820.micro820.e300data/sint_to_dint_underreactivegentriplevel.sint_src_1,0x5598,USINT
I135=micro820.micro820.e300data/sint_to_dint_underreactivegentriplevel.sint_src_2,0x5599,USINT
I136=micro820.micro820.e300data/sint_to_dint_underreactivegentriplevel.sint_src_3,0x559A,USINT
I137=micro820.micro820.e300data/sint_to_dint_underreactivegentriplevel.sint_src_4,0x559B,USINT
I138=micro820.micro820.e300data/sint_to_dint_underreactgenwarninglevel.sint_src_1,0x5598,USINT
I139=micro820.micro820.e300data/sint_to_dint_underreactgenwarninglevel.sint_src_2,0x5599,USINT
I140=micro820.micro820.e300data/sint_to_dint_underreactgenwarninglevel.sint_src_3,0x559A,USINT
I141=micro820.micro820.e300data/sint_to_dint_underreactgenwarninglevel.sint_src_4,0x559B,USINT
I142=micro820.micro820.e300data/sint_to_dint_oreactivegentriplevel.sint_src_1,0x5598,USINT
I143=micro820.micro820.e300data/sint_to_dint_oreactivegentriplevel.sint_src_2,0x5599,USINT
I144=micro820.micro820.e300data/sint_to_dint_oreactivegentriplevel.sint_src_3,0x559A,USINT
I145=micro820.micro820.e300data/sint_to_dint_oreactivegentriplevel.sint_src_4,0x559B,USINT
I146=micro820.micro820.e300data/sint_to_dint_oreactivegenwarninglevel.sint_src_1,0x5598,USINT
I147=micro820.micro820.e300data/sint_to_dint_oreactivegenwarninglevel.sint_src_2,0x5599,USINT
I148=micro820.micro820.e300data/sint_to_dint_oreactivegenwarninglevel.sint_src_3,0x559A,USINT
I149=micro820.micro820.e300data/sint_to_dint_oreactivegenwarninglevel.sint_src_4,0x559B,USINT
I150=micro820.micro820.e300data/sint_to_dint_underapparentpowertriplevel.sint_src_1,0x5598,USINT
I151=micro820.micro820.e300data/sint_to_dint_underapparentpowertriplevel.sint_src_2,0x5599,USINT
I152=micro820.micro820.e300data/sint_to_dint_underapparentpowertriplevel.sint_src_3,0x559A,USINT
I153=micro820.micro820.e300data/sint_to_dint_underapparentpowertriplevel.sint_src_4,0x559B,USINT
I154=micro820.micro820.e300data/sint_to_dint_underapparentwarninglevel.sint_src_1,0x5598,USINT
I155=micro820.micro820.e300data/sint_to_dint_underapparentwarninglevel.sint_src_2,0x5599,USINT
I156=micro820.micro820.e300data/sint_to_dint_underapparentwarninglevel.sint_src_3,0x559A,USINT
I157=micro820.micro820.e300data/sint_to_dint_underapparentwarninglevel.sint_src_4,0x559B,USINT
I158=micro820.micro820.e300data/sint_to_dint_overapparenttriplevel.sint_src_1,0x5598,USINT
I159=micro820.micro820.e300data/sint_to_dint_overapparenttriplevel.sint_src_2,0x5599,USINT
I160=micro820.micro820.e300data/sint_to_dint_overapparenttriplevel.sint_src_3,0x559A,USINT
I161=micro820.micro820.e300data/sint_to_dint_overapparenttriplevel.sint_src_4,0x559B,USINT
I162=micro820.micro820.e300data/sint_to_dint_overapparentwarninglevel.sint_src_1,0x5598,USINT
I163=micro820.micro820.e300data/sint_to_dint_overapparentwarninglevel.sint_src_2,0x5599,USINT
I164=micro820.micro820.e300data/sint_to_dint_overapparentwarninglevel.sint_src_3,0x559A,USINT
I165=micro820.micro820.e300data/sint_to_dint_overapparentwarninglevel.sint_src_4,0x559B,USINT
I166=micro820.micro820.control/linearscale_pressure.raw_min,0x5DDC,REAL
I167=micro820.micro820.control/linearscale_pressure.raw_max,0x5DD8,REAL
I168=micro820.micro820.control/linearscale_pressure.eu_min,0x6F0,REAL
I169=micro820.micro820.control/linearscale_pressure.eu_max,0x6F4,REAL
I170=micro820.micro820.control/linearscale_pressure.raw_inp,0x5E04,REAL
I171=micro820.micro820.control/linearscale_flow.raw_min,0x5DDC,REAL
I172=micro820.micro820.control/linearscale_flow.raw_max,0x5DD8,REAL
I173=micro820.micro820.control/linearscale_flow.eu_min,0x704,REAL
I174=micro820.micro820.control/linearscale_flow.eu_max,0x708,REAL
I175=micro820.micro820.control/linearscale_flow.raw_inp,0x5E04,REAL
I176=micro820.micro820.e300data/e300_read_digitalinput0.fben,0x460,BOOL
I177=micro820.micro820.e300data/e300_read_digitalinput0.ipaddress,0x8F8,STRING
I178=micro820.micro820.e300data/e300_read_digitalinput0.updaterate_ms,0x51A,UINT
I179=micro820.micro820.e300data/e300_read_digitalinput0.channelnumber,0x5D78,UDINT
I180=micro820.micro820.e300data/e300_read_digitalinput0.enable,0x46E,BOOL
I181=micro820.micro820.e300data/e300_read_digitalinput1.fben,0x460,BOOL
I182=micro820.micro820.e300data/e300_read_digitalinput1.ipaddress,0x8F8,STRING
I183=micro820.micro820.e300data/e300_read_digitalinput1.updaterate_ms,0x51A,UINT
I184=micro820.micro820.e300data/e300_read_digitalinput1.channelnumber,0x5D74,UDINT
I185=micro820.micro820.e300data/e300_read_digitalinput1.enable,0x46E,BOOL
I186=micro820.micro820.e300data/e300_read_digitalinput2.fben,0x460,BOOL
I187=micro820.micro820.e300data/e300_read_digitalinput2.ipaddress,0x8F8,STRING
I188=micro820.micro820.e300data/e300_read_digitalinput2.updaterate_ms,0x51A,UINT
I189=micro820.micro820.e300data/e300_read_digitalinput2.channelnumber,0x5D70,UDINT
I190=micro820.micro820.e300data/e300_read_digitalinput2.enable,0x46E,BOOL
I191=micro820.micro820.e300data/e300_read_digitalinput3.fben,0x460,BOOL
I192=micro820.micro820.e300data/e300_read_digitalinput3.ipaddress,0x8F8,STRING
I193=micro820.micro820.e300data/e300_read_digitalinput3.updaterate_ms,0x51A,UINT
I194=micro820.micro820.e300data/e300_read_digitalinput3.channelnumber,0x5D6C,UDINT
I195=micro820.micro820.e300data/e300_read_digitalinput3.enable,0x46E,BOOL
I196=micro820.micro820.e300data/e300_read_digitalinput4.fben,0x460,BOOL
I197=micro820.micro820.e300data/e300_read_digitalinput4.ipaddress,0x8F8,STRING
I198=micro820.micro820.e300data/e300_read_digitalinput4.updaterate_ms,0x51A,UINT
I199=micro820.micro820.e300data/e300_read_digitalinput4.channelnumber,0x5D68,UDINT
I200=micro820.micro820.e300data/e300_read_digitalinput4.enable,0x46E,BOOL
I201=micro820.micro820.e300data/e300_read_digitalinput5.fben,0x460,BOOL
I202=micro820.micro820.e300data/e300_read_digitalinput5.ipaddress,0x8F8,STRING
I203=micro820.micro820.e300data/e300_read_digitalinput5.updaterate_ms,0x51A,UINT
I204=micro820.micro820.e300data/e300_read_digitalinput5.channelnumber,0x5D64,UDINT
I205=micro820.micro820.e300data/e300_read_digitalinput5.enable,0x46E,BOOL
I206=micro820.micro820.e300data/u2s_underpflagtriplevel.sint_src_1,0x559C,USINT
I207=micro820.micro820.e300data/u2s_underpflagwarninglevel.sint_src_1,0x559C,USINT
I208=micro820.micro820.e300data/u2s_overpflagtriplevel.sint_src_1,0x559C,USINT
I209=micro820.micro820.e300data/u2s_overpflagwarninglevel.sint_src_1,0x559C,USINT
I210=micro820.micro820.currenttimertc.rtc_read_1.enable,0x557E,BOOL
I211=micro820.micro820.control/rtrig_automode.clk,0x478,BOOL
I212=micro820.micro820.e300data/writee300configdata.msgobjread_q_rtrig.clk,0x554B,BOOL
I213=micro820.micro820.e300data/writee300configdata.fben_rtrig.clk,0x554B,BOOL
I214=micro820.micro820.e300data/writee300configdata.msgobjread_err_rtrig.clk,0x554B,BOOL
I215=micro820.micro820.e300data/e300_output.msgprodname_err_rtrig.clk,0x554B,BOOL
I216=micro820.micro820.e300data/e300_output.msgwriteoutput_err_rtrig.clk,0x554B,BOOL
I217=micro820.micro820.e300data/e300_output.fben_rtrig.clk,0x554B,BOOL
I218=micro820.micro820.e300data/e300_output.msgwriteoutput_q_rtrig.clk,0x554B,BOOL
I219=micro820.micro820.e300data/e300_output.outputsetting_rtrig.clk,0x554B,BOOL
I220=micro820.micro820.e300data/e300_output.msgprodname_q_rtrig.clk,0x554B,BOOL
I221=micro820.micro820.e300data/e300_readenergy.msgprodname_err_rtrig.clk,0x554B,BOOL
I222=micro820.micro820.e300data/e300_readenergy.msgobjread_q_rtrig.clk,0x554B,BOOL
I223=micro820.micro820.e300data/e300_readenergy.fben_rtrig.clk,0x554B,BOOL
I224=micro820.micro820.e300data/e300_readenergy.msgobjread_err_rtrig.clk,0x554B,BOOL
I225=micro820.micro820.e300data/e300_readenergy.msgprodname_q_rtrig.clk,0x554B,BOOL
I226=micro820.micro820.e300data/e300_read_digitalinput0.msgobjread_q_rtrig.clk,0x554B,BOOL
I227=micro820.micro820.e300data/e300_read_digitalinput0.fben_rtrig.clk,0x554B,BOOL
I228=micro820.micro820.e300data/e300_read_digitalinput0.msgobjread_err_rtrig.clk,0x554B,BOOL
I229=micro820.micro820.e300data/reade300configdata.msgobjread_q_rtrig.clk,0x554B,BOOL
I230=micro820.micro820.e300data/reade300configdata.fben_rtrig.clk,0x554B,BOOL
I231=micro820.micro820.e300data/reade300configdata.msgobjread_err_rtrig.clk,0x554B,BOOL
I232=micro820.micro820.e300data/e300_tripstatuscurrent.msgobjread_q_rtrig.clk,0x554B,BOOL
I233=micro820.micro820.e300data/e300_tripstatuscurrent.fben_rtrig.clk,0x554B,BOOL
I234=micro820.micro820.e300data/e300_tripstatuscurrent.msgobjread_err_rtrig.clk,0x554B,BOOL
I235=micro820.micro820.e300data/e300_write_tripreset.msgobjread_q_rtrig.clk,0x554B,BOOL
I236=micro820.micro820.e300data/e300_write_tripreset.fben_rtrig.clk,0x554B,BOOL
I237=micro820.micro820.e300data/e300_write_tripreset.msgobjread_err_rtrig.clk,0x554B,BOOL
I238=micro820.micro820.e300data/e300_read_digitalinput1.msgobjread_q_rtrig.clk,0x554B,BOOL
I239=micro820.micro820.e300data/e300_read_digitalinput1.fben_rtrig.clk,0x554B,BOOL
I240=micro820.micro820.e300data/e300_read_digitalinput1.msgobjread_err_rtrig.clk,0x554B,BOOL
I241=micro820.micro820.e300data/e300_tripstatusvoltage.msgobjread_q_rtrig.clk,0x554B,BOOL
I242=micro820.micro820.e300data/e300_tripstatusvoltage.fben_rtrig.clk,0x554B,BOOL
I243=micro820.micro820.e300data/e300_tripstatusvoltage.msgobjread_err_rtrig.clk,0x554B,BOOL
I244=micro820.micro820.e300data/e300_read_digitalinput2.msgobjread_q_rtrig.clk,0x554B,BOOL
I245=micro820.micro820.e300data/e300_read_digitalinput2.fben_rtrig.clk,0x554B,BOOL
I246=micro820.micro820.e300data/e300_read_digitalinput2.msgobjread_err_rtrig.clk,0x554B,BOOL
I247=micro820.micro820.e300data/e300_tripstatuspower.msgobjread_q_rtrig.clk,0x554B,BOOL
I248=micro820.micro820.e300data/e300_tripstatuspower.fben_rtrig.clk,0x554B,BOOL
I249=micro820.micro820.e300data/e300_tripstatuspower.msgobjread_err_rtrig.clk,0x554B,BOOL
I250=micro820.micro820.e300data/e300_read_digitalinput3.msgobjread_q_rtrig.clk,0x554B,BOOL
I251=micro820.micro820.e300data/e300_read_digitalinput3.fben_rtrig.clk,0x554B,BOOL
I252=micro820.micro820.e300data/e300_read_digitalinput3.msgobjread_err_rtrig.clk,0x554B,BOOL
I253=micro820.micro820.e300data/e300_tripstatuscontrol.msgobjread_q_rtrig.clk,0x554B,BOOL
I254=micro820.micro820.e300data/e300_tripstatuscontrol.fben_rtrig.clk,0x554B,BOOL
I255=micro820.micro820.e300data/e300_tripstatuscontrol.msgobjread_err_rtrig.clk,0x554B,BOOL
I256=micro820.micro820.e300data/e300_read_digitalinput4.msgobjread_q_rtrig.clk,0x554B,BOOL
I257=micro820.micro820.e300data/e300_read_digitalinput4.fben_rtrig.clk,0x554B,BOOL
I258=micro820.micro820.e300data/e300_read_digitalinput4.msgobjread_err_rtrig.clk,0x554B,BOOL
I259=micro820.micro820.e300data/e300_warnstatuscurrent.msgobjread_q_rtrig.clk,0x554B,BOOL
I260=micro820.micro820.e300data/e300_warnstatuscurrent.fben_rtrig.clk,0x554B,BOOL
I261=micro820.micro820.e300data/e300_warnstatuscurrent.msgobjread_err_rtrig.clk,0x554B,BOOL
I262=micro820.micro820.e300data/e300_read_digitalinput5.msgobjread_q_rtrig.clk,0x554B,BOOL
I263=micro820.micro820.e300data/e300_read_digitalinput5.fben_rtrig.clk,0x554B,BOOL
I264=micro820.micro820.e300data/e300_read_digitalinput5.msgobjread_err_rtrig.clk,0x554B,BOOL
I265=micro820.micro820.e300data/e300_warnstatusvoltage.msgobjread_q_rtrig.clk,0x554B,BOOL
I266=micro820.micro820.e300data/e300_warnstatusvoltage.fben_rtrig.clk,0x554B,BOOL
I267=micro820.micro820.e300data/e300_warnstatusvoltage.msgobjread_err_rtrig.clk,0x554B,BOOL
I268=micro820.micro820.e300data/e300_warnstatuspower.msgobjread_q_rtrig.clk,0x554B,BOOL
I269=micro820.micro820.e300data/e300_warnstatuspower.fben_rtrig.clk,0x554B,BOOL
I270=micro820.micro820.e300data/e300_warnstatuspower.msgobjread_err_rtrig.clk,0x554B,BOOL
I271=micro820.micro820.e300data/e300_warnstatuscontrol.msgobjread_q_rtrig.clk,0x554B,BOOL
I272=micro820.micro820.e300data/e300_warnstatuscontrol.fben_rtrig.clk,0x554B,BOOL
I273=micro820.micro820.e300data/e300_warnstatuscontrol.msgobjread_err_rtrig.clk,0x554B,BOOL
I274=micro820.micro820.e300data/i2s_tripenablecurrent.inp_int,0x5608,UINT
I275=micro820.micro820.e300data/i2s_tripenablevoltage.inp_int,0x5608,UINT
I276=micro820.micro820.e300data/i2s_tripenablepower.inp_int,0x5608,UINT
I277=micro820.micro820.e300data/i2s_tripenablecontrol.inp_int,0x5608,UINT
I278=micro820.micro820.e300data/i2s_warningenablecurrent.inp_int,0x5608,UINT
I279=micro820.micro820.e300data/i2s_warningenablevoltage.inp_int,0x5608,UINT
I280=micro820.micro820.e300data/i2s_warningenablepower.inp_int,0x5608,UINT
I281=micro820.micro820.e300data/i2s_warningenablecontrol.inp_int,0x5608,UINT
I282=micro820.micro820.e300data/i2s_groundfaulttriplevel.inp_int,0x5608,UINT
I283=micro820.micro820.e300data/i2s_groundfaultwarninglevel.inp_int,0x5608,UINT
I284=micro820.micro820.e300data/i2s_stalltriplevel.inp_int,0x5608,UINT
I285=micro820.micro820.e300data/i2s_jamtriplevel.inp_int,0x5608,UINT
I286=micro820.micro820.e300data/i2s_jamwarninglevel.inp_int,0x5608,UINT
I287=micro820.micro820.e300data/i2s_ctprimary.inp_int,0x5608,UINT
I288=micro820.micro820.e300data/i2s_ctsecondary.inp_int,0x5608,UINT
I289=micro820.micro820.e300data/i2s_ptprimary.inp_int,0x5608,UINT
I290=micro820.micro820.e300data/i2s_ptsecondary.inp_int,0x5608,UINT
I291=micro820.micro820.e300data/i2s_undervoltagetriplevel.inp_int,0x5608,UINT
I292=micro820.micro820.e300data/i2s_undervoltagewarninglevel.inp_int,0x5608,UINT
I293=micro820.micro820.e300data/i2s_overvoltagetriplevel.inp_int,0x5608,UINT
I294=micro820.micro820.e300data/i2s_overvoltagewarninglevel.inp_int,0x5608,UINT
I295=micro820.micro820.e300data/reade300configdata.fben,0x460,BOOL
I296=micro820.micro820.e300data/reade300configdata.ipaddress,0x8F8,STRING
I297=micro820.micro820.e300data/reade300configdata.updaterate_ms,0x51A,UINT
I298=micro820.micro820.e300data/reade300configdata.enable,0x460,BOOL
I299=micro820.micro820.e300data/s2i_tripstatuscurrent.sint_src_1,0x5590,USINT
I300=micro820.micro820.e300data/s2i_tripstatuscurrent.sint_src_2,0x5591,USINT
I301=micro820.micro820.e300data/s2i_tripstatusvoltage.sint_src_1,0x5590,USINT
I302=micro820.micro820.e300data/s2i_tripstatusvoltage.sint_src_2,0x5591,USINT
I303=micro820.micro820.e300data/s2i_tripstatuspower.sint_src_1,0x5590,USINT
I304=micro820.micro820.e300data/s2i_tripstatuspower.sint_src_2,0x5591,USINT
I305=micro820.micro820.e300data/s2i_tripstatuscontrol.sint_src_1,0x5590,USINT
I306=micro820.micro820.e300data/s2i_tripstatuscontrol.sint_src_2,0x5591,USINT
I307=micro820.micro820.e300data/s2i_warningstatuscurrent.sint_src_1,0x5590,USINT
I308=micro820.micro820.e300data/s2i_warningstatuscurrent.sint_src_2,0x5591,USINT
I309=micro820.micro820.e300data/s2i_warningstatusvoltage.sint_src_1,0x5590,USINT
I310=micro820.micro820.e300data/s2i_warningstatusvoltage.sint_src_2,0x5591,USINT
I311=micro820.micro820.e300data/s2i_warningstatuspower.sint_src_1,0x5590,USINT
I312=micro820.micro820.e300data/s2i_warningstatuspower.sint_src_2,0x5591,USINT
I313=micro820.micro820.e300data/s2i_warningstatuscontrol.sint_src_1,0x5590,USINT
I314=micro820.micro820.e300data/s2i_warningstatuscontrol.sint_src_2,0x5591,USINT
I315=micro820.micro820.e300data/sint_to_int_tripenablecurrent.sint_src_1,0x5590,USINT
I316=micro820.micro820.e300data/sint_to_int_tripenablecurrent.sint_src_2,0x5591,USINT
I317=micro820.micro820.e300data/sint_to_int_tripenablevoltage.sint_src_1,0x5590,USINT
I318=micro820.micro820.e300data/sint_to_int_tripenablevoltage.sint_src_2,0x5591,USINT
I319=micro820.micro820.e300data/sint_to_int_tripenablepower.sint_src_1,0x5590,USINT
I320=micro820.micro820.e300data/sint_to_int_tripenablepower.sint_src_2,0x5591,USINT
I321=micro820.micro820.e300data/sint_to_int_tripenablecontrol.sint_src_1,0x5590,USINT
I322=micro820.micro820.e300data/sint_to_int_tripenablecontrol.sint_src_2,0x5591,USINT
I323=micro820.micro820.e300data/sint_to_int_warningenablecurrent.sint_src_1,0x5590,USINT
I324=micro820.micro820.e300data/sint_to_int_warningenablecurrent.sint_src_2,0x5591,USINT
I325=micro820.micro820.e300data/sint_to_int_warningenablevoltage.sint_src_1,0x5590,USINT
I326=micro820.micro820.e300data/sint_to_int_warningenablevoltage.sint_src_2,0x5591,USINT
I327=micro820.micro820.e300data/sint_to_int_warningenablepower.sint_src_1,0x5590,USINT
I328=micro820.micro820.e300data/sint_to_int_warningenablepower.sint_src_2,0x5591,USINT
I329=micro820.micro820.e300data/sint_to_int_warningenablecontrol.sint_src_1,0x5590,USINT
I330=micro820.micro820.e300data/sint_to_int_warningenablecontrol.sint_src_2,0x5591,USINT
I331=micro820.micro820.e300data/sint_to_int_groundfaulttriplevel.sint_src_1,0x5590,USINT
I332=micro820.micro820.e300data/sint_to_int_groundfaulttriplevel.sint_src_2,0x5591,USINT
I333=micro820.micro820.e300data/sint_to_int_groundfaultwarninglevel.sint_src_1,0x5590,USINT
I334=micro820.micro820.e300data/sint_to_int_groundfaultwarninglevel.sint_src_2,0x5591,USINT
I335=micro820.micro820.e300data/sint_to_int_stalltriplevel.sint_src_1,0x5590,USINT
I336=micro820.micro820.e300data/sint_to_int_stalltriplevel.sint_src_2,0x5591,USINT
I337=micro820.micro820.e300data/sint_to_int_jamtriplevel.sint_src_1,0x5590,USINT
I338=micro820.micro820.e300data/sint_to_int_jamtriplevel.sint_src_2,0x5591,USINT
I339=micro820.micro820.e300data/sint_to_int_jamwarninglevel.sint_src_1,0x5590,USINT
I340=micro820.micro820.e300data/sint_to_int_jamwarninglevel.sint_src_2,0x5591,USINT
I341=micro820.micro820.e300data/sint_to_int_ctprimary.sint_src_1,0x5590,USINT
I342=micro820.micro820.e300data/sint_to_int_ctprimary.sint_src_2,0x5591,USINT
I343=micro820.micro820.e300data/sint_to_int_ctsecondary.sint_src_1,0x5590,USINT
I344=micro820.micro820.e300data/sint_to_int_ctsecondary.sint_src_2,0x5591,USINT
I345=micro820.micro820.e300data/sint_to_int_ptprimary.sint_src_1,0x5590,USINT
I346=micro820.micro820.e300data/sint_to_int_ptprimary.sint_src_2,0x5591,USINT
I347=micro820.micro820.e300data/sint_to_int_ptsecondary.sint_src_1,0x5590,USINT
I348=micro820.micro820.e300data/sint_to_int_ptsecondary.sint_src_2,0x5591,USINT
I349=micro820.micro820.e300data/sint_to_int_undervoltagetriplevel.sint_src_1,0x5590,USINT
I350=micro820.micro820.e300data/sint_to_int_undervoltagetriplevel.sint_src_2,0x5591,USINT
I351=micro820.micro820.e300data/sint_to_int_undervoltagewarninglevel.sint_src_1,0x5590,USINT
I352=micro820.micro820.e300data/sint_to_int_undervoltagewarninglevel.sint_src_2,0x5591,USINT
I353=micro820.micro820.e300data/sint_to_int_overvoltagetriplevel.sint_src_1,0x5590,USINT
I354=micro820.micro820.e300data/sint_to_int_overvoltagetriplevel.sint_src_2,0x5591,USINT
I355=micro820.micro820.e300data/sint_to_int_overvoltagewarninglevel.sint_src_1,0x5590,USINT
I356=micro820.micro820.e300data/sint_to_int_overvoltagewarninglevel.sint_src_2,0x5591,USINT
I357=micro820.micro820.readdownholedata/modbusdata_0.in,0x5542,BOOL
I358=micro820.micro820.readdownholedata/modbusdata_0.cancel,0x4C3,BOOL
I359=micro820.micro820.readdownholedata/modbusdata_0.localcfg,0xFFFFFFFF,MODBUSLOCPARA
I360=micro820.micro820.readdownholedata/modbusdata_0.targetcfg,0xFFFFFFFF,MODBUSTARPARA
I361=micro820.micro820.readdownholedata/modbusdata_0.localaddr,0xFFFFFFFF,MODBUSLOCADDR
I362=micro820.micro820.readdownholedata/modbusdata_0.__adi_localaddr,0xFFFFFFFF,UINT
I363=micro820.micro820.readdownholedata/modbusdata_1000.in,0x5542,BOOL
I364=micro820.micro820.readdownholedata/modbusdata_1000.cancel,0x4C3,BOOL
I365=micro820.micro820.readdownholedata/modbusdata_1000.localcfg,0xFFFFFFFF,MODBUSLOCPARA
I366=micro820.micro820.readdownholedata/modbusdata_1000.targetcfg,0xFFFFFFFF,MODBUSTARPARA
I367=micro820.micro820.readdownholedata/modbusdata_1000.localaddr,0xFFFFFFFF,MODBUSLOCADDR
I368=micro820.micro820.readdownholedata/modbusdata_1000.__adi_localaddr,0xFFFFFFFF,UINT
I369=micro820.micro820.e300data/e300_tripstatuscurrent.fben,0x460,BOOL
I370=micro820.micro820.e300data/e300_tripstatuscurrent.ipaddress,0x8F8,STRING
I371=micro820.micro820.e300data/e300_tripstatuscurrent.updaterate_ms,0x51A,UINT
I372=micro820.micro820.e300data/e300_tripstatuscurrent.enable,0x460,BOOL
I373=micro820.micro820.e300data/e300_tripstatuscurrent.paramnumber,0x5D68,UDINT
I374=micro820.micro820.e300data/e300_tripstatusvoltage.fben,0x460,BOOL
I375=micro820.micro820.e300data/e300_tripstatusvoltage.ipaddress,0x8F8,STRING
I376=micro820.micro820.e300data/e300_tripstatusvoltage.updaterate_ms,0x51A,UINT
I377=micro820.micro820.e300data/e300_tripstatusvoltage.enable,0x460,BOOL
I378=micro820.micro820.e300data/e300_tripstatusvoltage.paramnumber,0x5D64,UDINT
I379=micro820.micro820.e300data/e300_tripstatuspower.fben,0x460,BOOL
I380=micro820.micro820.e300data/e300_tripstatuspower.ipaddress,0x8F8,STRING
I381=micro820.micro820.e300data/e300_tripstatuspower.updaterate_ms,0x51A,UINT
I382=micro820.micro820.e300data/e300_tripstatuspower.enable,0x460,BOOL
I383=micro820.micro820.e300data/e300_tripstatuspower.paramnumber,0x5D60,UDINT
I384=micro820.micro820.e300data/e300_tripstatuscontrol.fben,0x460,BOOL
I385=micro820.micro820.e300data/e300_tripstatuscontrol.ipaddress,0x8F8,STRING
I386=micro820.micro820.e300data/e300_tripstatuscontrol.updaterate_ms,0x51A,UINT
I387=micro820.micro820.e300data/e300_tripstatuscontrol.enable,0x460,BOOL
I388=micro820.micro820.e300data/e300_tripstatuscontrol.paramnumber,0x5D5C,UDINT
I389=micro820.micro820.e300data/e300_warnstatuscurrent.fben,0x460,BOOL
I390=micro820.micro820.e300data/e300_warnstatuscurrent.ipaddress,0x8F8,STRING
I391=micro820.micro820.e300data/e300_warnstatuscurrent.updaterate_ms,0x51A,UINT
I392=micro820.micro820.e300data/e300_warnstatuscurrent.enable,0x460,BOOL
I393=micro820.micro820.e300data/e300_warnstatuscurrent.paramnumber,0x5D58,UDINT
I394=micro820.micro820.e300data/e300_warnstatusvoltage.fben,0x460,BOOL
I395=micro820.micro820.e300data/e300_warnstatusvoltage.ipaddress,0x8F8,STRING
I396=micro820.micro820.e300data/e300_warnstatusvoltage.updaterate_ms,0x51A,UINT
I397=micro820.micro820.e300data/e300_warnstatusvoltage.enable,0x460,BOOL
I398=micro820.micro820.e300data/e300_warnstatusvoltage.paramnumber,0x5D54,UDINT
I399=micro820.micro820.e300data/e300_warnstatuspower.fben,0x460,BOOL
I400=micro820.micro820.e300data/e300_warnstatuspower.ipaddress,0x8F8,STRING
I401=micro820.micro820.e300data/e300_warnstatuspower.updaterate_ms,0x51A,UINT
I402=micro820.micro820.e300data/e300_warnstatuspower.enable,0x460,BOOL
I403=micro820.micro820.e300data/e300_warnstatuspower.paramnumber,0x5D50,UDINT
I404=micro820.micro820.e300data/e300_warnstatuscontrol.fben,0x460,BOOL
I405=micro820.micro820.e300data/e300_warnstatuscontrol.ipaddress,0x8F8,STRING
I406=micro820.micro820.e300data/e300_warnstatuscontrol.updaterate_ms,0x51A,UINT
I407=micro820.micro820.e300data/e300_warnstatuscontrol.enable,0x460,BOOL
I408=micro820.micro820.e300data/e300_warnstatuscontrol.paramnumber,0x5D4C,UDINT
I409=micro820.micro820.e300data/writee300configdata.msgobjread.in,0x555D,BOOL
I410=micro820.micro820.e300data/writee300configdata.msgobjread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I411=micro820.micro820.e300data/writee300configdata.msgobjread.appcfg,0xFFFFFFFF,CIPAPPCFG
I412=micro820.micro820.e300data/writee300configdata.msgobjread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I413=micro820.micro820.e300data/writee300configdata.msgobjread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I414=micro820.micro820.e300data/writee300configdata.msgobjread.reqlength,0x55DA,UINT
I415=micro820.micro820.e300data/writee300configdata.msgobjread.__adi_reqdata,0xFFFFFFFF,UINT
I416=micro820.micro820.e300data/e300_output.msgwriteoutput.in,0x555D,BOOL
I417=micro820.micro820.e300data/e300_output.msgwriteoutput.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I418=micro820.micro820.e300data/e300_output.msgwriteoutput.appcfg,0xFFFFFFFF,CIPAPPCFG
I419=micro820.micro820.e300data/e300_output.msgwriteoutput.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I420=micro820.micro820.e300data/e300_output.msgwriteoutput.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I421=micro820.micro820.e300data/e300_output.msgwriteoutput.reqlength,0x5600,UINT
I422=micro820.micro820.e300data/e300_output.msgwriteoutput.__adi_reqdata,0xFFFFFFFF,UINT
I423=micro820.micro820.e300data/e300_output.msgprodname.in,0x555D,BOOL
I424=micro820.micro820.e300data/e300_output.msgprodname.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I425=micro820.micro820.e300data/e300_output.msgprodname.appcfg,0xFFFFFFFF,CIPAPPCFG
I426=micro820.micro820.e300data/e300_output.msgprodname.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I427=micro820.micro820.e300data/e300_output.msgprodname.reqlength,0x5604,UINT
I428=micro820.micro820.e300data/e300_output.msgprodname.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I429=micro820.micro820.e300data/e300_output.msgprodname.__adi_resdata,0xFFFFFFFF,UINT
I430=micro820.micro820.e300data/e300_readenergy.msgprodname.in,0x555D,BOOL
I431=micro820.micro820.e300data/e300_readenergy.msgprodname.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I432=micro820.micro820.e300data/e300_readenergy.msgprodname.appcfg,0xFFFFFFFF,CIPAPPCFG
I433=micro820.micro820.e300data/e300_readenergy.msgprodname.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I434=micro820.micro820.e300data/e300_readenergy.msgprodname.reqlength,0x5604,UINT
I435=micro820.micro820.e300data/e300_readenergy.msgprodname.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I436=micro820.micro820.e300data/e300_readenergy.msgprodname.__adi_resdata,0xFFFFFFFF,UINT
I437=micro820.micro820.e300data/e300_readenergy.msgobjread.in,0x555D,BOOL
I438=micro820.micro820.e300data/e300_readenergy.msgobjread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I439=micro820.micro820.e300data/e300_readenergy.msgobjread.appcfg,0xFFFFFFFF,CIPAPPCFG
I440=micro820.micro820.e300data/e300_readenergy.msgobjread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I441=micro820.micro820.e300data/e300_readenergy.msgobjread.reqlength,0x5604,UINT
I442=micro820.micro820.e300data/e300_readenergy.msgobjread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I443=micro820.micro820.e300data/e300_readenergy.msgobjread.__adi_resdata,0xFFFFFFFF,UINT
I444=micro820.micro820.e300data/e300_read_digitalinput0.msgobjread.in,0x555D,BOOL
I445=micro820.micro820.e300data/e300_read_digitalinput0.msgobjread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I446=micro820.micro820.e300data/e300_read_digitalinput0.msgobjread.appcfg,0xFFFFFFFF,CIPAPPCFG
I447=micro820.micro820.e300data/e300_read_digitalinput0.msgobjread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I448=micro820.micro820.e300data/e300_read_digitalinput0.msgobjread.reqlength,0x5600,UINT
I449=micro820.micro820.e300data/e300_read_digitalinput0.msgobjread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I450=micro820.micro820.e300data/e300_read_digitalinput0.msgobjread.__adi_resdata,0xFFFFFFFF,UINT
I451=micro820.micro820.e300data/reade300configdata.msgobjread.in,0x555D,BOOL
I452=micro820.micro820.e300data/reade300configdata.msgobjread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I453=micro820.micro820.e300data/reade300configdata.msgobjread.appcfg,0xFFFFFFFF,CIPAPPCFG
I454=micro820.micro820.e300data/reade300configdata.msgobjread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I455=micro820.micro820.e300data/reade300configdata.msgobjread.reqlength,0x5604,UINT
I456=micro820.micro820.e300data/reade300configdata.msgobjread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I457=micro820.micro820.e300data/reade300configdata.msgobjread.__adi_resdata,0xFFFFFFFF,UINT
I458=micro820.micro820.e300data/e300_tripstatuscurrent.msgobjread.in,0x555D,BOOL
I459=micro820.micro820.e300data/e300_tripstatuscurrent.msgobjread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I460=micro820.micro820.e300data/e300_tripstatuscurrent.msgobjread.appcfg,0xFFFFFFFF,CIPAPPCFG
I461=micro820.micro820.e300data/e300_tripstatuscurrent.msgobjread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I462=micro820.micro820.e300data/e300_tripstatuscurrent.msgobjread.reqlength,0x5604,UINT
I463=micro820.micro820.e300data/e300_tripstatuscurrent.msgobjread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I464=micro820.micro820.e300data/e300_tripstatuscurrent.msgobjread.__adi_resdata,0xFFFFFFFF,UINT
I465=micro820.micro820.e300data/e300_write_tripreset.msgobjread.in,0x555D,BOOL
I466=micro820.micro820.e300data/e300_write_tripreset.msgobjread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I467=micro820.micro820.e300data/e300_write_tripreset.msgobjread.appcfg,0xFFFFFFFF,CIPAPPCFG
I468=micro820.micro820.e300data/e300_write_tripreset.msgobjread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I469=micro820.micro820.e300data/e300_write_tripreset.msgobjread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I470=micro820.micro820.e300data/e300_write_tripreset.msgobjread.reqlength,0x5600,UINT
I471=micro820.micro820.e300data/e300_write_tripreset.msgobjread.__adi_reqdata,0xFFFFFFFF,UINT
I472=micro820.micro820.e300data/e300_read_digitalinput1.msgobjread.in,0x555D,BOOL
I473=micro820.micro820.e300data/e300_read_digitalinput1.msgobjread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I474=micro820.micro820.e300data/e300_read_digitalinput1.msgobjread.appcfg,0xFFFFFFFF,CIPAPPCFG
I475=micro820.micro820.e300data/e300_read_digitalinput1.msgobjread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I476=micro820.micro820.e300data/e300_read_digitalinput1.msgobjread.reqlength,0x5600,UINT
I477=micro820.micro820.e300data/e300_read_digitalinput1.msgobjread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I478=micro820.micro820.e300data/e300_read_digitalinput1.msgobjread.__adi_resdata,0xFFFFFFFF,UINT
I479=micro820.micro820.e300data/e300_tripstatusvoltage.msgobjread.in,0x555D,BOOL
I480=micro820.micro820.e300data/e300_tripstatusvoltage.msgobjread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I481=micro820.micro820.e300data/e300_tripstatusvoltage.msgobjread.appcfg,0xFFFFFFFF,CIPAPPCFG
I482=micro820.micro820.e300data/e300_tripstatusvoltage.msgobjread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I483=micro820.micro820.e300data/e300_tripstatusvoltage.msgobjread.reqlength,0x5604,UINT
I484=micro820.micro820.e300data/e300_tripstatusvoltage.msgobjread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I485=micro820.micro820.e300data/e300_tripstatusvoltage.msgobjread.__adi_resdata,0xFFFFFFFF,UINT
I486=micro820.micro820.e300data/e300_read_digitalinput2.msgobjread.in,0x555D,BOOL
I487=micro820.micro820.e300data/e300_read_digitalinput2.msgobjread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I488=micro820.micro820.e300data/e300_read_digitalinput2.msgobjread.appcfg,0xFFFFFFFF,CIPAPPCFG
I489=micro820.micro820.e300data/e300_read_digitalinput2.msgobjread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I490=micro820.micro820.e300data/e300_read_digitalinput2.msgobjread.reqlength,0x5600,UINT
I491=micro820.micro820.e300data/e300_read_digitalinput2.msgobjread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I492=micro820.micro820.e300data/e300_read_digitalinput2.msgobjread.__adi_resdata,0xFFFFFFFF,UINT
I493=micro820.micro820.e300data/e300_tripstatuspower.msgobjread.in,0x555D,BOOL
I494=micro820.micro820.e300data/e300_tripstatuspower.msgobjread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I495=micro820.micro820.e300data/e300_tripstatuspower.msgobjread.appcfg,0xFFFFFFFF,CIPAPPCFG
I496=micro820.micro820.e300data/e300_tripstatuspower.msgobjread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I497=micro820.micro820.e300data/e300_tripstatuspower.msgobjread.reqlength,0x5604,UINT
I498=micro820.micro820.e300data/e300_tripstatuspower.msgobjread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I499=micro820.micro820.e300data/e300_tripstatuspower.msgobjread.__adi_resdata,0xFFFFFFFF,UINT
I500=micro820.micro820.e300data/e300_read_digitalinput3.msgobjread.in,0x555D,BOOL
I501=micro820.micro820.e300data/e300_read_digitalinput3.msgobjread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I502=micro820.micro820.e300data/e300_read_digitalinput3.msgobjread.appcfg,0xFFFFFFFF,CIPAPPCFG
I503=micro820.micro820.e300data/e300_read_digitalinput3.msgobjread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I504=micro820.micro820.e300data/e300_read_digitalinput3.msgobjread.reqlength,0x5600,UINT
I505=micro820.micro820.e300data/e300_read_digitalinput3.msgobjread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I506=micro820.micro820.e300data/e300_read_digitalinput3.msgobjread.__adi_resdata,0xFFFFFFFF,UINT
I507=micro820.micro820.e300data/e300_tripstatuscontrol.msgobjread.in,0x555D,BOOL
I508=micro820.micro820.e300data/e300_tripstatuscontrol.msgobjread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I509=micro820.micro820.e300data/e300_tripstatuscontrol.msgobjread.appcfg,0xFFFFFFFF,CIPAPPCFG
I510=micro820.micro820.e300data/e300_tripstatuscontrol.msgobjread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I511=micro820.micro820.e300data/e300_tripstatuscontrol.msgobjread.reqlength,0x5604,UINT
I512=micro820.micro820.e300data/e300_tripstatuscontrol.msgobjread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I513=micro820.micro820.e300data/e300_tripstatuscontrol.msgobjread.__adi_resdata,0xFFFFFFFF,UINT
I514=micro820.micro820.e300data/e300_read_digitalinput4.msgobjread.in,0x555D,BOOL
I515=micro820.micro820.e300data/e300_read_digitalinput4.msgobjread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I516=micro820.micro820.e300data/e300_read_digitalinput4.msgobjread.appcfg,0xFFFFFFFF,CIPAPPCFG
I517=micro820.micro820.e300data/e300_read_digitalinput4.msgobjread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I518=micro820.micro820.e300data/e300_read_digitalinput4.msgobjread.reqlength,0x5600,UINT
I519=micro820.micro820.e300data/e300_read_digitalinput4.msgobjread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I520=micro820.micro820.e300data/e300_read_digitalinput4.msgobjread.__adi_resdata,0xFFFFFFFF,UINT
I521=micro820.micro820.e300data/e300_warnstatuscurrent.msgobjread.in,0x555D,BOOL
I522=micro820.micro820.e300data/e300_warnstatuscurrent.msgobjread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I523=micro820.micro820.e300data/e300_warnstatuscurrent.msgobjread.appcfg,0xFFFFFFFF,CIPAPPCFG
I524=micro820.micro820.e300data/e300_warnstatuscurrent.msgobjread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I525=micro820.micro820.e300data/e300_warnstatuscurrent.msgobjread.reqlength,0x5604,UINT
I526=micro820.micro820.e300data/e300_warnstatuscurrent.msgobjread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I527=micro820.micro820.e300data/e300_warnstatuscurrent.msgobjread.__adi_resdata,0xFFFFFFFF,UINT
I528=micro820.micro820.e300data/e300_read_digitalinput5.msgobjread.in,0x555D,BOOL
I529=micro820.micro820.e300data/e300_read_digitalinput5.msgobjread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I530=micro820.micro820.e300data/e300_read_digitalinput5.msgobjread.appcfg,0xFFFFFFFF,CIPAPPCFG
I531=micro820.micro820.e300data/e300_read_digitalinput5.msgobjread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I532=micro820.micro820.e300data/e300_read_digitalinput5.msgobjread.reqlength,0x5600,UINT
I533=micro820.micro820.e300data/e300_read_digitalinput5.msgobjread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I534=micro820.micro820.e300data/e300_read_digitalinput5.msgobjread.__adi_resdata,0xFFFFFFFF,UINT
I535=micro820.micro820.e300data/e300_warnstatusvoltage.msgobjread.in,0x555D,BOOL
I536=micro820.micro820.e300data/e300_warnstatusvoltage.msgobjread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I537=micro820.micro820.e300data/e300_warnstatusvoltage.msgobjread.appcfg,0xFFFFFFFF,CIPAPPCFG
I538=micro820.micro820.e300data/e300_warnstatusvoltage.msgobjread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I539=micro820.micro820.e300data/e300_warnstatusvoltage.msgobjread.reqlength,0x5604,UINT
I540=micro820.micro820.e300data/e300_warnstatusvoltage.msgobjread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I541=micro820.micro820.e300data/e300_warnstatusvoltage.msgobjread.__adi_resdata,0xFFFFFFFF,UINT
I542=micro820.micro820.e300data/e300_warnstatuspower.msgobjread.in,0x555D,BOOL
I543=micro820.micro820.e300data/e300_warnstatuspower.msgobjread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I544=micro820.micro820.e300data/e300_warnstatuspower.msgobjread.appcfg,0xFFFFFFFF,CIPAPPCFG
I545=micro820.micro820.e300data/e300_warnstatuspower.msgobjread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I546=micro820.micro820.e300data/e300_warnstatuspower.msgobjread.reqlength,0x5604,UINT
I547=micro820.micro820.e300data/e300_warnstatuspower.msgobjread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I548=micro820.micro820.e300data/e300_warnstatuspower.msgobjread.__adi_resdata,0xFFFFFFFF,UINT
I549=micro820.micro820.e300data/e300_warnstatuscontrol.msgobjread.in,0x555D,BOOL
I550=micro820.micro820.e300data/e300_warnstatuscontrol.msgobjread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I551=micro820.micro820.e300data/e300_warnstatuscontrol.msgobjread.appcfg,0xFFFFFFFF,CIPAPPCFG
I552=micro820.micro820.e300data/e300_warnstatuscontrol.msgobjread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I553=micro820.micro820.e300data/e300_warnstatuscontrol.msgobjread.reqlength,0x5604,UINT
I554=micro820.micro820.e300data/e300_warnstatuscontrol.msgobjread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I555=micro820.micro820.e300data/e300_warnstatuscontrol.msgobjread.__adi_resdata,0xFFFFFFFF,UINT
I556=micro820.micro820.e300data/d2s_underrealpowertriplevel.inp_dint,0x5CE0,DINT
I557=micro820.micro820.e300data/d2s_underrealpowerwarninglevel.inp_dint,0x5CE0,DINT
I558=micro820.micro820.e300data/d2s_overrealpowertriplevel.inp_dint,0x5CE0,DINT
I559=micro820.micro820.e300data/d2s_overrealpowerwarninglevel.inp_dint,0x5CE0,DINT
I560=micro820.micro820.e300data/d2s_underreactiveconsumedpowertriplevel.inp_dint,0x5CE0,DINT
I561=micro820.micro820.e300data/d2s_underreactiveconswarninglevel.inp_dint,0x5CE0,DINT
I562=micro820.micro820.e300data/d2s_overreactiveconsumedpowertriplevel.inp_dint,0x5CE0,DINT
I563=micro820.micro820.e300data/d2s_overreactiveconswarninglevel.inp_dint,0x5CE0,DINT
I564=micro820.micro820.e300data/d2s_underreactivegeneratedpowertriplevel.inp_dint,0x5CE0,DINT
I565=micro820.micro820.e300data/d2s_underreactivegenwarninglevel.inp_dint,0x5CE0,DINT
I566=micro820.micro820.e300data/d2s_overreactivegeneratedpowertriplevel.inp_dint,0x5CE0,DINT
I567=micro820.micro820.e300data/d2s_overreactivegenwarninglevel.inp_dint,0x5CE0,DINT
I568=micro820.micro820.e300data/d2s_underapparentpowertriplevel.inp_dint,0x5CE0,DINT
I569=micro820.micro820.e300data/d2s_underapparentpowerwarninglevel.inp_dint,0x5CE0,DINT
I570=micro820.micro820.e300data/d2s_overapparentpowertriplevel.inp_dint,0x5CE0,DINT
I571=micro820.micro820.e300data/d2s_overapparentpowerwarninglevel.inp_dint,0x5CE0,DINT
I572=micro820.micro820.e300data/e300_write_tripreset.fben,0x460,BOOL
I573=micro820.micro820.e300data/e300_write_tripreset.ipaddress,0x8F8,STRING
I574=micro820.micro820.e300data/e300_write_tripreset.updaterate_ms,0x51A,UINT
I575=micro820.micro820.e300data/e300_write_tripreset.enable,0x460,BOOL
I576=micro820.micro820.e300data/e300_write_tripreset.input,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I577=micro820.micro820.downtime_timer.in,0x7A68,BOOL
I578=micro820.micro820.downtime_timer.pt,0x7A7C,TIME
I579=micro820.micro820.e300data/e300_readenergy.msgobjread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I580=micro820.micro820.e300data/e300_readenergy.msgobjread.__adi_reqdata,0xFFFFFFFF,UINT
I581=micro820.micro820.e300data/e300_readenergy.msgprodname.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I582=micro820.micro820.e300data/e300_readenergy.msgprodname.__adi_reqdata,0xFFFFFFFF,UINT
I583=micro820.micro820.e300data/e300_output.msgwriteoutput.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I584=micro820.micro820.e300data/e300_output.msgwriteoutput.__adi_resdata,0xFFFFFFFF,UINT
I585=micro820.micro820.e300data/e300_output.msgprodname.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I586=micro820.micro820.e300data/e300_output.msgprodname.__adi_reqdata,0xFFFFFFFF,UINT
I587=micro820.micro820.e300data/e300_read_digitalinput0.msgobjread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I588=micro820.micro820.e300data/e300_read_digitalinput0.msgobjread.__adi_reqdata,0xFFFFFFFF,UINT
I589=micro820.micro820.e300data/e300_read_digitalinput0.int_cop.enable,0x7A68,BOOL
I590=micro820.micro820.e300data/e300_read_digitalinput0.int_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I591=micro820.micro820.e300data/e300_read_digitalinput0.int_cop.srcoffset,0x7A6C,UINT
I592=micro820.micro820.e300data/e300_read_digitalinput0.int_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I593=micro820.micro820.e300data/e300_read_digitalinput0.int_cop.destoffset,0x7A6C,UINT
I594=micro820.micro820.e300data/e300_read_digitalinput0.int_cop.length,0x7A6C,UINT
I595=micro820.micro820.e300data/e300_read_digitalinput0.int_cop.swap,0x7A68,BOOL
I596=micro820.micro820.e300data/e300_read_digitalinput0.int_cop.__adi_src,0xFFFFFFFF,UINT
I597=micro820.micro820.e300data/e300_read_digitalinput0.int_cop.__adi_dest,0xFFFFFFFF,UINT
I598=micro820.micro820.e300data/e300_read_digitalinput0.int_cop.__dti_src,0xFFFFFFFF,SINT
I599=micro820.micro820.e300data/e300_read_digitalinput0.int_cop.__dti_dest,0xFFFFFFFF,SINT
I600=micro820.micro820.e300data/e300_read_digitalinput0.real_cop.enable,0x7A68,BOOL
I601=micro820.micro820.e300data/e300_read_digitalinput0.real_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I602=micro820.micro820.e300data/e300_read_digitalinput0.real_cop.srcoffset,0x7A6C,UINT
I603=micro820.micro820.e300data/e300_read_digitalinput0.real_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I604=micro820.micro820.e300data/e300_read_digitalinput0.real_cop.destoffset,0x7A6C,UINT
I605=micro820.micro820.e300data/e300_read_digitalinput0.real_cop.length,0x7A6C,UINT
I606=micro820.micro820.e300data/e300_read_digitalinput0.real_cop.swap,0x7A68,BOOL
I607=micro820.micro820.e300data/e300_read_digitalinput0.real_cop.__adi_src,0xFFFFFFFF,UINT
I608=micro820.micro820.e300data/e300_read_digitalinput0.real_cop.__adi_dest,0xFFFFFFFF,UINT
I609=micro820.micro820.e300data/e300_read_digitalinput0.real_cop.__dti_src,0xFFFFFFFF,SINT
I610=micro820.micro820.e300data/e300_read_digitalinput0.real_cop.__dti_dest,0xFFFFFFFF,SINT
I611=micro820.micro820.e300data/e300_read_digitalinput0.phase_cop.enable,0x7A68,BOOL
I612=micro820.micro820.e300data/e300_read_digitalinput0.phase_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I613=micro820.micro820.e300data/e300_read_digitalinput0.phase_cop.srcoffset,0x7A6C,UINT
I614=micro820.micro820.e300data/e300_read_digitalinput0.phase_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I615=micro820.micro820.e300data/e300_read_digitalinput0.phase_cop.destoffset,0x7A6C,UINT
I616=micro820.micro820.e300data/e300_read_digitalinput0.phase_cop.length,0x7A6C,UINT
I617=micro820.micro820.e300data/e300_read_digitalinput0.phase_cop.swap,0x7A68,BOOL
I618=micro820.micro820.e300data/e300_read_digitalinput0.phase_cop.__adi_src,0xFFFFFFFF,UINT
I619=micro820.micro820.e300data/e300_read_digitalinput0.phase_cop.__adi_dest,0xFFFFFFFF,UINT
I620=micro820.micro820.e300data/e300_read_digitalinput0.phase_cop.__dti_src,0xFFFFFFFF,SINT
I621=micro820.micro820.e300data/e300_read_digitalinput0.phase_cop.__dti_dest,0xFFFFFFFF,SINT
I622=micro820.micro820.e300data/e300_read_digitalinput1.msgobjread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I623=micro820.micro820.e300data/e300_read_digitalinput1.msgobjread.__adi_reqdata,0xFFFFFFFF,UINT
I624=micro820.micro820.e300data/e300_read_digitalinput1.int_cop.enable,0x7A68,BOOL
I625=micro820.micro820.e300data/e300_read_digitalinput1.int_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I626=micro820.micro820.e300data/e300_read_digitalinput1.int_cop.srcoffset,0x7A6C,UINT
I627=micro820.micro820.e300data/e300_read_digitalinput1.int_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I628=micro820.micro820.e300data/e300_read_digitalinput1.int_cop.destoffset,0x7A6C,UINT
I629=micro820.micro820.e300data/e300_read_digitalinput1.int_cop.length,0x7A6C,UINT
I630=micro820.micro820.e300data/e300_read_digitalinput1.int_cop.swap,0x7A68,BOOL
I631=micro820.micro820.e300data/e300_read_digitalinput1.int_cop.__adi_src,0xFFFFFFFF,UINT
I632=micro820.micro820.e300data/e300_read_digitalinput1.int_cop.__adi_dest,0xFFFFFFFF,UINT
I633=micro820.micro820.e300data/e300_read_digitalinput1.int_cop.__dti_src,0xFFFFFFFF,SINT
I634=micro820.micro820.e300data/e300_read_digitalinput1.int_cop.__dti_dest,0xFFFFFFFF,SINT
I635=micro820.micro820.e300data/e300_read_digitalinput1.real_cop.enable,0x7A68,BOOL
I636=micro820.micro820.e300data/e300_read_digitalinput1.real_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I637=micro820.micro820.e300data/e300_read_digitalinput1.real_cop.srcoffset,0x7A6C,UINT
I638=micro820.micro820.e300data/e300_read_digitalinput1.real_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I639=micro820.micro820.e300data/e300_read_digitalinput1.real_cop.destoffset,0x7A6C,UINT
I640=micro820.micro820.e300data/e300_read_digitalinput1.real_cop.length,0x7A6C,UINT
I641=micro820.micro820.e300data/e300_read_digitalinput1.real_cop.swap,0x7A68,BOOL
I642=micro820.micro820.e300data/e300_read_digitalinput1.real_cop.__adi_src,0xFFFFFFFF,UINT
I643=micro820.micro820.e300data/e300_read_digitalinput1.real_cop.__adi_dest,0xFFFFFFFF,UINT
I644=micro820.micro820.e300data/e300_read_digitalinput1.real_cop.__dti_src,0xFFFFFFFF,SINT
I645=micro820.micro820.e300data/e300_read_digitalinput1.real_cop.__dti_dest,0xFFFFFFFF,SINT
I646=micro820.micro820.e300data/e300_read_digitalinput1.phase_cop.enable,0x7A68,BOOL
I647=micro820.micro820.e300data/e300_read_digitalinput1.phase_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I648=micro820.micro820.e300data/e300_read_digitalinput1.phase_cop.srcoffset,0x7A6C,UINT
I649=micro820.micro820.e300data/e300_read_digitalinput1.phase_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I650=micro820.micro820.e300data/e300_read_digitalinput1.phase_cop.destoffset,0x7A6C,UINT
I651=micro820.micro820.e300data/e300_read_digitalinput1.phase_cop.length,0x7A6C,UINT
I652=micro820.micro820.e300data/e300_read_digitalinput1.phase_cop.swap,0x7A68,BOOL
I653=micro820.micro820.e300data/e300_read_digitalinput1.phase_cop.__adi_src,0xFFFFFFFF,UINT
I654=micro820.micro820.e300data/e300_read_digitalinput1.phase_cop.__adi_dest,0xFFFFFFFF,UINT
I655=micro820.micro820.e300data/e300_read_digitalinput1.phase_cop.__dti_src,0xFFFFFFFF,SINT
I656=micro820.micro820.e300data/e300_read_digitalinput1.phase_cop.__dti_dest,0xFFFFFFFF,SINT
I657=micro820.micro820.e300data/e300_read_digitalinput2.msgobjread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I658=micro820.micro820.e300data/e300_read_digitalinput2.msgobjread.__adi_reqdata,0xFFFFFFFF,UINT
I659=micro820.micro820.e300data/e300_read_digitalinput2.int_cop.enable,0x7A68,BOOL
I660=micro820.micro820.e300data/e300_read_digitalinput2.int_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I661=micro820.micro820.e300data/e300_read_digitalinput2.int_cop.srcoffset,0x7A6C,UINT
I662=micro820.micro820.e300data/e300_read_digitalinput2.int_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I663=micro820.micro820.e300data/e300_read_digitalinput2.int_cop.destoffset,0x7A6C,UINT
I664=micro820.micro820.e300data/e300_read_digitalinput2.int_cop.length,0x7A6C,UINT
I665=micro820.micro820.e300data/e300_read_digitalinput2.int_cop.swap,0x7A68,BOOL
I666=micro820.micro820.e300data/e300_read_digitalinput2.int_cop.__adi_src,0xFFFFFFFF,UINT
I667=micro820.micro820.e300data/e300_read_digitalinput2.int_cop.__adi_dest,0xFFFFFFFF,UINT
I668=micro820.micro820.e300data/e300_read_digitalinput2.int_cop.__dti_src,0xFFFFFFFF,SINT
I669=micro820.micro820.e300data/e300_read_digitalinput2.int_cop.__dti_dest,0xFFFFFFFF,SINT
I670=micro820.micro820.e300data/e300_read_digitalinput2.real_cop.enable,0x7A68,BOOL
I671=micro820.micro820.e300data/e300_read_digitalinput2.real_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I672=micro820.micro820.e300data/e300_read_digitalinput2.real_cop.srcoffset,0x7A6C,UINT
I673=micro820.micro820.e300data/e300_read_digitalinput2.real_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I674=micro820.micro820.e300data/e300_read_digitalinput2.real_cop.destoffset,0x7A6C,UINT
I675=micro820.micro820.e300data/e300_read_digitalinput2.real_cop.length,0x7A6C,UINT
I676=micro820.micro820.e300data/e300_read_digitalinput2.real_cop.swap,0x7A68,BOOL
I677=micro820.micro820.e300data/e300_read_digitalinput2.real_cop.__adi_src,0xFFFFFFFF,UINT
I678=micro820.micro820.e300data/e300_read_digitalinput2.real_cop.__adi_dest,0xFFFFFFFF,UINT
I679=micro820.micro820.e300data/e300_read_digitalinput2.real_cop.__dti_src,0xFFFFFFFF,SINT
I680=micro820.micro820.e300data/e300_read_digitalinput2.real_cop.__dti_dest,0xFFFFFFFF,SINT
I681=micro820.micro820.e300data/e300_read_digitalinput2.phase_cop.enable,0x7A68,BOOL
I682=micro820.micro820.e300data/e300_read_digitalinput2.phase_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I683=micro820.micro820.e300data/e300_read_digitalinput2.phase_cop.srcoffset,0x7A6C,UINT
I684=micro820.micro820.e300data/e300_read_digitalinput2.phase_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I685=micro820.micro820.e300data/e300_read_digitalinput2.phase_cop.destoffset,0x7A6C,UINT
I686=micro820.micro820.e300data/e300_read_digitalinput2.phase_cop.length,0x7A6C,UINT
I687=micro820.micro820.e300data/e300_read_digitalinput2.phase_cop.swap,0x7A68,BOOL
I688=micro820.micro820.e300data/e300_read_digitalinput2.phase_cop.__adi_src,0xFFFFFFFF,UINT
I689=micro820.micro820.e300data/e300_read_digitalinput2.phase_cop.__adi_dest,0xFFFFFFFF,UINT
I690=micro820.micro820.e300data/e300_read_digitalinput2.phase_cop.__dti_src,0xFFFFFFFF,SINT
I691=micro820.micro820.e300data/e300_read_digitalinput2.phase_cop.__dti_dest,0xFFFFFFFF,SINT
I692=micro820.micro820.e300data/e300_read_digitalinput3.msgobjread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I693=micro820.micro820.e300data/e300_read_digitalinput3.msgobjread.__adi_reqdata,0xFFFFFFFF,UINT
I694=micro820.micro820.e300data/e300_read_digitalinput3.int_cop.enable,0x7A68,BOOL
I695=micro820.micro820.e300data/e300_read_digitalinput3.int_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I696=micro820.micro820.e300data/e300_read_digitalinput3.int_cop.srcoffset,0x7A6C,UINT
I697=micro820.micro820.e300data/e300_read_digitalinput3.int_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I698=micro820.micro820.e300data/e300_read_digitalinput3.int_cop.destoffset,0x7A6C,UINT
I699=micro820.micro820.e300data/e300_read_digitalinput3.int_cop.length,0x7A6C,UINT
I700=micro820.micro820.e300data/e300_read_digitalinput3.int_cop.swap,0x7A68,BOOL
I701=micro820.micro820.e300data/e300_read_digitalinput3.int_cop.__adi_src,0xFFFFFFFF,UINT
I702=micro820.micro820.e300data/e300_read_digitalinput3.int_cop.__adi_dest,0xFFFFFFFF,UINT
I703=micro820.micro820.e300data/e300_read_digitalinput3.int_cop.__dti_src,0xFFFFFFFF,SINT
I704=micro820.micro820.e300data/e300_read_digitalinput3.int_cop.__dti_dest,0xFFFFFFFF,SINT
I705=micro820.micro820.e300data/e300_read_digitalinput3.real_cop.enable,0x7A68,BOOL
I706=micro820.micro820.e300data/e300_read_digitalinput3.real_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I707=micro820.micro820.e300data/e300_read_digitalinput3.real_cop.srcoffset,0x7A6C,UINT
I708=micro820.micro820.e300data/e300_read_digitalinput3.real_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I709=micro820.micro820.e300data/e300_read_digitalinput3.real_cop.destoffset,0x7A6C,UINT
I710=micro820.micro820.e300data/e300_read_digitalinput3.real_cop.length,0x7A6C,UINT
I711=micro820.micro820.e300data/e300_read_digitalinput3.real_cop.swap,0x7A68,BOOL
I712=micro820.micro820.e300data/e300_read_digitalinput3.real_cop.__adi_src,0xFFFFFFFF,UINT
I713=micro820.micro820.e300data/e300_read_digitalinput3.real_cop.__adi_dest,0xFFFFFFFF,UINT
I714=micro820.micro820.e300data/e300_read_digitalinput3.real_cop.__dti_src,0xFFFFFFFF,SINT
I715=micro820.micro820.e300data/e300_read_digitalinput3.real_cop.__dti_dest,0xFFFFFFFF,SINT
I716=micro820.micro820.e300data/e300_read_digitalinput3.phase_cop.enable,0x7A68,BOOL
I717=micro820.micro820.e300data/e300_read_digitalinput3.phase_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I718=micro820.micro820.e300data/e300_read_digitalinput3.phase_cop.srcoffset,0x7A6C,UINT
I719=micro820.micro820.e300data/e300_read_digitalinput3.phase_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I720=micro820.micro820.e300data/e300_read_digitalinput3.phase_cop.destoffset,0x7A6C,UINT
I721=micro820.micro820.e300data/e300_read_digitalinput3.phase_cop.length,0x7A6C,UINT
I722=micro820.micro820.e300data/e300_read_digitalinput3.phase_cop.swap,0x7A68,BOOL
I723=micro820.micro820.e300data/e300_read_digitalinput3.phase_cop.__adi_src,0xFFFFFFFF,UINT
I724=micro820.micro820.e300data/e300_read_digitalinput3.phase_cop.__adi_dest,0xFFFFFFFF,UINT
I725=micro820.micro820.e300data/e300_read_digitalinput3.phase_cop.__dti_src,0xFFFFFFFF,SINT
I726=micro820.micro820.e300data/e300_read_digitalinput3.phase_cop.__dti_dest,0xFFFFFFFF,SINT
I727=micro820.micro820.e300data/e300_read_digitalinput4.msgobjread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I728=micro820.micro820.e300data/e300_read_digitalinput4.msgobjread.__adi_reqdata,0xFFFFFFFF,UINT
I729=micro820.micro820.e300data/e300_read_digitalinput4.int_cop.enable,0x7A68,BOOL
I730=micro820.micro820.e300data/e300_read_digitalinput4.int_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I731=micro820.micro820.e300data/e300_read_digitalinput4.int_cop.srcoffset,0x7A6C,UINT
I732=micro820.micro820.e300data/e300_read_digitalinput4.int_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I733=micro820.micro820.e300data/e300_read_digitalinput4.int_cop.destoffset,0x7A6C,UINT
I734=micro820.micro820.e300data/e300_read_digitalinput4.int_cop.length,0x7A6C,UINT
I735=micro820.micro820.e300data/e300_read_digitalinput4.int_cop.swap,0x7A68,BOOL
I736=micro820.micro820.e300data/e300_read_digitalinput4.int_cop.__adi_src,0xFFFFFFFF,UINT
I737=micro820.micro820.e300data/e300_read_digitalinput4.int_cop.__adi_dest,0xFFFFFFFF,UINT
I738=micro820.micro820.e300data/e300_read_digitalinput4.int_cop.__dti_src,0xFFFFFFFF,SINT
I739=micro820.micro820.e300data/e300_read_digitalinput4.int_cop.__dti_dest,0xFFFFFFFF,SINT
I740=micro820.micro820.e300data/e300_read_digitalinput4.real_cop.enable,0x7A68,BOOL
I741=micro820.micro820.e300data/e300_read_digitalinput4.real_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I742=micro820.micro820.e300data/e300_read_digitalinput4.real_cop.srcoffset,0x7A6C,UINT
I743=micro820.micro820.e300data/e300_read_digitalinput4.real_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I744=micro820.micro820.e300data/e300_read_digitalinput4.real_cop.destoffset,0x7A6C,UINT
I745=micro820.micro820.e300data/e300_read_digitalinput4.real_cop.length,0x7A6C,UINT
I746=micro820.micro820.e300data/e300_read_digitalinput4.real_cop.swap,0x7A68,BOOL
I747=micro820.micro820.e300data/e300_read_digitalinput4.real_cop.__adi_src,0xFFFFFFFF,UINT
I748=micro820.micro820.e300data/e300_read_digitalinput4.real_cop.__adi_dest,0xFFFFFFFF,UINT
I749=micro820.micro820.e300data/e300_read_digitalinput4.real_cop.__dti_src,0xFFFFFFFF,SINT
I750=micro820.micro820.e300data/e300_read_digitalinput4.real_cop.__dti_dest,0xFFFFFFFF,SINT
I751=micro820.micro820.e300data/e300_read_digitalinput4.phase_cop.enable,0x7A68,BOOL
I752=micro820.micro820.e300data/e300_read_digitalinput4.phase_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I753=micro820.micro820.e300data/e300_read_digitalinput4.phase_cop.srcoffset,0x7A6C,UINT
I754=micro820.micro820.e300data/e300_read_digitalinput4.phase_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I755=micro820.micro820.e300data/e300_read_digitalinput4.phase_cop.destoffset,0x7A6C,UINT
I756=micro820.micro820.e300data/e300_read_digitalinput4.phase_cop.length,0x7A6C,UINT
I757=micro820.micro820.e300data/e300_read_digitalinput4.phase_cop.swap,0x7A68,BOOL
I758=micro820.micro820.e300data/e300_read_digitalinput4.phase_cop.__adi_src,0xFFFFFFFF,UINT
I759=micro820.micro820.e300data/e300_read_digitalinput4.phase_cop.__adi_dest,0xFFFFFFFF,UINT
I760=micro820.micro820.e300data/e300_read_digitalinput4.phase_cop.__dti_src,0xFFFFFFFF,SINT
I761=micro820.micro820.e300data/e300_read_digitalinput4.phase_cop.__dti_dest,0xFFFFFFFF,SINT
I762=micro820.micro820.e300data/e300_read_digitalinput5.msgobjread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I763=micro820.micro820.e300data/e300_read_digitalinput5.msgobjread.__adi_reqdata,0xFFFFFFFF,UINT
I764=micro820.micro820.e300data/e300_read_digitalinput5.int_cop.enable,0x7A68,BOOL
I765=micro820.micro820.e300data/e300_read_digitalinput5.int_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I766=micro820.micro820.e300data/e300_read_digitalinput5.int_cop.srcoffset,0x7A6C,UINT
I767=micro820.micro820.e300data/e300_read_digitalinput5.int_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I768=micro820.micro820.e300data/e300_read_digitalinput5.int_cop.destoffset,0x7A6C,UINT
I769=micro820.micro820.e300data/e300_read_digitalinput5.int_cop.length,0x7A6C,UINT
I770=micro820.micro820.e300data/e300_read_digitalinput5.int_cop.swap,0x7A68,BOOL
I771=micro820.micro820.e300data/e300_read_digitalinput5.int_cop.__adi_src,0xFFFFFFFF,UINT
I772=micro820.micro820.e300data/e300_read_digitalinput5.int_cop.__adi_dest,0xFFFFFFFF,UINT
I773=micro820.micro820.e300data/e300_read_digitalinput5.int_cop.__dti_src,0xFFFFFFFF,SINT
I774=micro820.micro820.e300data/e300_read_digitalinput5.int_cop.__dti_dest,0xFFFFFFFF,SINT
I775=micro820.micro820.e300data/e300_read_digitalinput5.real_cop.enable,0x7A68,BOOL
I776=micro820.micro820.e300data/e300_read_digitalinput5.real_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I777=micro820.micro820.e300data/e300_read_digitalinput5.real_cop.srcoffset,0x7A6C,UINT
I778=micro820.micro820.e300data/e300_read_digitalinput5.real_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I779=micro820.micro820.e300data/e300_read_digitalinput5.real_cop.destoffset,0x7A6C,UINT
I780=micro820.micro820.e300data/e300_read_digitalinput5.real_cop.length,0x7A6C,UINT
I781=micro820.micro820.e300data/e300_read_digitalinput5.real_cop.swap,0x7A68,BOOL
I782=micro820.micro820.e300data/e300_read_digitalinput5.real_cop.__adi_src,0xFFFFFFFF,UINT
I783=micro820.micro820.e300data/e300_read_digitalinput5.real_cop.__adi_dest,0xFFFFFFFF,UINT
I784=micro820.micro820.e300data/e300_read_digitalinput5.real_cop.__dti_src,0xFFFFFFFF,SINT
I785=micro820.micro820.e300data/e300_read_digitalinput5.real_cop.__dti_dest,0xFFFFFFFF,SINT
I786=micro820.micro820.e300data/e300_read_digitalinput5.phase_cop.enable,0x7A68,BOOL
I787=micro820.micro820.e300data/e300_read_digitalinput5.phase_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I788=micro820.micro820.e300data/e300_read_digitalinput5.phase_cop.srcoffset,0x7A6C,UINT
I789=micro820.micro820.e300data/e300_read_digitalinput5.phase_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I790=micro820.micro820.e300data/e300_read_digitalinput5.phase_cop.destoffset,0x7A6C,UINT
I791=micro820.micro820.e300data/e300_read_digitalinput5.phase_cop.length,0x7A6C,UINT
I792=micro820.micro820.e300data/e300_read_digitalinput5.phase_cop.swap,0x7A68,BOOL
I793=micro820.micro820.e300data/e300_read_digitalinput5.phase_cop.__adi_src,0xFFFFFFFF,UINT
I794=micro820.micro820.e300data/e300_read_digitalinput5.phase_cop.__adi_dest,0xFFFFFFFF,UINT
I795=micro820.micro820.e300data/e300_read_digitalinput5.phase_cop.__dti_src,0xFFFFFFFF,SINT
I796=micro820.micro820.e300data/e300_read_digitalinput5.phase_cop.__dti_dest,0xFFFFFFFF,SINT
I797=micro820.micro820.e300data/reade300configdata.msgobjread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I798=micro820.micro820.e300data/reade300configdata.msgobjread.__adi_reqdata,0xFFFFFFFF,UINT
I799=micro820.micro820.e300data/reade300configdata.int_cop.enable,0x7A68,BOOL
I800=micro820.micro820.e300data/reade300configdata.int_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I801=micro820.micro820.e300data/reade300configdata.int_cop.srcoffset,0x7A6C,UINT
I802=micro820.micro820.e300data/reade300configdata.int_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I803=micro820.micro820.e300data/reade300configdata.int_cop.destoffset,0x7A6C,UINT
I804=micro820.micro820.e300data/reade300configdata.int_cop.length,0x7A6C,UINT
I805=micro820.micro820.e300data/reade300configdata.int_cop.swap,0x7A68,BOOL
I806=micro820.micro820.e300data/reade300configdata.int_cop.__adi_src,0xFFFFFFFF,UINT
I807=micro820.micro820.e300data/reade300configdata.int_cop.__adi_dest,0xFFFFFFFF,UINT
I808=micro820.micro820.e300data/reade300configdata.int_cop.__dti_src,0xFFFFFFFF,SINT
I809=micro820.micro820.e300data/reade300configdata.int_cop.__dti_dest,0xFFFFFFFF,SINT
I810=micro820.micro820.e300data/reade300configdata.real_cop.enable,0x7A68,BOOL
I811=micro820.micro820.e300data/reade300configdata.real_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I812=micro820.micro820.e300data/reade300configdata.real_cop.srcoffset,0x7A6C,UINT
I813=micro820.micro820.e300data/reade300configdata.real_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I814=micro820.micro820.e300data/reade300configdata.real_cop.destoffset,0x7A6C,UINT
I815=micro820.micro820.e300data/reade300configdata.real_cop.length,0x7A6C,UINT
I816=micro820.micro820.e300data/reade300configdata.real_cop.swap,0x7A68,BOOL
I817=micro820.micro820.e300data/reade300configdata.real_cop.__adi_src,0xFFFFFFFF,UINT
I818=micro820.micro820.e300data/reade300configdata.real_cop.__adi_dest,0xFFFFFFFF,UINT
I819=micro820.micro820.e300data/reade300configdata.real_cop.__dti_src,0xFFFFFFFF,SINT
I820=micro820.micro820.e300data/reade300configdata.real_cop.__dti_dest,0xFFFFFFFF,SINT
I821=micro820.micro820.e300data/reade300configdata.phase_cop.enable,0x7A68,BOOL
I822=micro820.micro820.e300data/reade300configdata.phase_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I823=micro820.micro820.e300data/reade300configdata.phase_cop.srcoffset,0x7A6C,UINT
I824=micro820.micro820.e300data/reade300configdata.phase_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I825=micro820.micro820.e300data/reade300configdata.phase_cop.destoffset,0x7A6C,UINT
I826=micro820.micro820.e300data/reade300configdata.phase_cop.length,0x7A6C,UINT
I827=micro820.micro820.e300data/reade300configdata.phase_cop.swap,0x7A68,BOOL
I828=micro820.micro820.e300data/reade300configdata.phase_cop.__adi_src,0xFFFFFFFF,UINT
I829=micro820.micro820.e300data/reade300configdata.phase_cop.__adi_dest,0xFFFFFFFF,UINT
I830=micro820.micro820.e300data/reade300configdata.phase_cop.__dti_src,0xFFFFFFFF,SINT
I831=micro820.micro820.e300data/reade300configdata.phase_cop.__dti_dest,0xFFFFFFFF,SINT
I832=micro820.micro820.e300data/d_2_s_flasetting.inp_dint,0x7A74,UDINT
I833=micro820.micro820.e300data/writee300configdata.msgobjread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I834=micro820.micro820.e300data/writee300configdata.msgobjread.__adi_resdata,0xFFFFFFFF,UINT
I835=micro820.micro820.e300data/writee300configdata.int_cop.enable,0x7A68,BOOL
I836=micro820.micro820.e300data/writee300configdata.int_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I837=micro820.micro820.e300data/writee300configdata.int_cop.srcoffset,0x7A6C,UINT
I838=micro820.micro820.e300data/writee300configdata.int_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I839=micro820.micro820.e300data/writee300configdata.int_cop.destoffset,0x7A6C,UINT
I840=micro820.micro820.e300data/writee300configdata.int_cop.length,0x7A6C,UINT
I841=micro820.micro820.e300data/writee300configdata.int_cop.swap,0x7A68,BOOL
I842=micro820.micro820.e300data/writee300configdata.int_cop.__adi_src,0xFFFFFFFF,UINT
I843=micro820.micro820.e300data/writee300configdata.int_cop.__adi_dest,0xFFFFFFFF,UINT
I844=micro820.micro820.e300data/writee300configdata.int_cop.__dti_src,0xFFFFFFFF,SINT
I845=micro820.micro820.e300data/writee300configdata.int_cop.__dti_dest,0xFFFFFFFF,SINT
I846=micro820.micro820.e300data/writee300configdata.real_cop.enable,0x7A68,BOOL
I847=micro820.micro820.e300data/writee300configdata.real_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I848=micro820.micro820.e300data/writee300configdata.real_cop.srcoffset,0x7A6C,UINT
I849=micro820.micro820.e300data/writee300configdata.real_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I850=micro820.micro820.e300data/writee300configdata.real_cop.destoffset,0x7A6C,UINT
I851=micro820.micro820.e300data/writee300configdata.real_cop.length,0x7A6C,UINT
I852=micro820.micro820.e300data/writee300configdata.real_cop.swap,0x7A68,BOOL
I853=micro820.micro820.e300data/writee300configdata.real_cop.__adi_src,0xFFFFFFFF,UINT
I854=micro820.micro820.e300data/writee300configdata.real_cop.__adi_dest,0xFFFFFFFF,UINT
I855=micro820.micro820.e300data/writee300configdata.real_cop.__dti_src,0xFFFFFFFF,SINT
I856=micro820.micro820.e300data/writee300configdata.real_cop.__dti_dest,0xFFFFFFFF,SINT
I857=micro820.micro820.e300data/writee300configdata.phase_cop.enable,0x7A68,BOOL
I858=micro820.micro820.e300data/writee300configdata.phase_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I859=micro820.micro820.e300data/writee300configdata.phase_cop.srcoffset,0x7A6C,UINT
I860=micro820.micro820.e300data/writee300configdata.phase_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I861=micro820.micro820.e300data/writee300configdata.phase_cop.destoffset,0x7A6C,UINT
I862=micro820.micro820.e300data/writee300configdata.phase_cop.length,0x7A6C,UINT
I863=micro820.micro820.e300data/writee300configdata.phase_cop.swap,0x7A68,BOOL
I864=micro820.micro820.e300data/writee300configdata.phase_cop.__adi_src,0xFFFFFFFF,UINT
I865=micro820.micro820.e300data/writee300configdata.phase_cop.__adi_dest,0xFFFFFFFF,UINT
I866=micro820.micro820.e300data/writee300configdata.phase_cop.__dti_src,0xFFFFFFFF,SINT
I867=micro820.micro820.e300data/writee300configdata.phase_cop.__dti_dest,0xFFFFFFFF,SINT
I868=micro820.micro820.e300data/e300_write_tripreset.msgobjread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I869=micro820.micro820.e300data/e300_write_tripreset.msgobjread.__adi_resdata,0xFFFFFFFF,UINT
I870=micro820.micro820.e300data/e300_write_tripreset.int_cop.enable,0x7A68,BOOL
I871=micro820.micro820.e300data/e300_write_tripreset.int_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I872=micro820.micro820.e300data/e300_write_tripreset.int_cop.srcoffset,0x7A6C,UINT
I873=micro820.micro820.e300data/e300_write_tripreset.int_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I874=micro820.micro820.e300data/e300_write_tripreset.int_cop.destoffset,0x7A6C,UINT
I875=micro820.micro820.e300data/e300_write_tripreset.int_cop.length,0x7A6C,UINT
I876=micro820.micro820.e300data/e300_write_tripreset.int_cop.swap,0x7A68,BOOL
I877=micro820.micro820.e300data/e300_write_tripreset.int_cop.__adi_src,0xFFFFFFFF,UINT
I878=micro820.micro820.e300data/e300_write_tripreset.int_cop.__adi_dest,0xFFFFFFFF,UINT
I879=micro820.micro820.e300data/e300_write_tripreset.int_cop.__dti_src,0xFFFFFFFF,SINT
I880=micro820.micro820.e300data/e300_write_tripreset.int_cop.__dti_dest,0xFFFFFFFF,SINT
I881=micro820.micro820.e300data/e300_write_tripreset.real_cop.enable,0x7A68,BOOL
I882=micro820.micro820.e300data/e300_write_tripreset.real_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I883=micro820.micro820.e300data/e300_write_tripreset.real_cop.srcoffset,0x7A6C,UINT
I884=micro820.micro820.e300data/e300_write_tripreset.real_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I885=micro820.micro820.e300data/e300_write_tripreset.real_cop.destoffset,0x7A6C,UINT
I886=micro820.micro820.e300data/e300_write_tripreset.real_cop.length,0x7A6C,UINT
I887=micro820.micro820.e300data/e300_write_tripreset.real_cop.swap,0x7A68,BOOL
I888=micro820.micro820.e300data/e300_write_tripreset.real_cop.__adi_src,0xFFFFFFFF,UINT
I889=micro820.micro820.e300data/e300_write_tripreset.real_cop.__adi_dest,0xFFFFFFFF,UINT
I890=micro820.micro820.e300data/e300_write_tripreset.real_cop.__dti_src,0xFFFFFFFF,SINT
I891=micro820.micro820.e300data/e300_write_tripreset.real_cop.__dti_dest,0xFFFFFFFF,SINT
I892=micro820.micro820.e300data/e300_write_tripreset.phase_cop.enable,0x7A68,BOOL
I893=micro820.micro820.e300data/e300_write_tripreset.phase_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I894=micro820.micro820.e300data/e300_write_tripreset.phase_cop.srcoffset,0x7A6C,UINT
I895=micro820.micro820.e300data/e300_write_tripreset.phase_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I896=micro820.micro820.e300data/e300_write_tripreset.phase_cop.destoffset,0x7A6C,UINT
I897=micro820.micro820.e300data/e300_write_tripreset.phase_cop.length,0x7A6C,UINT
I898=micro820.micro820.e300data/e300_write_tripreset.phase_cop.swap,0x7A68,BOOL
I899=micro820.micro820.e300data/e300_write_tripreset.phase_cop.__adi_src,0xFFFFFFFF,UINT
I900=micro820.micro820.e300data/e300_write_tripreset.phase_cop.__adi_dest,0xFFFFFFFF,UINT
I901=micro820.micro820.e300data/e300_write_tripreset.phase_cop.__dti_src,0xFFFFFFFF,SINT
I902=micro820.micro820.e300data/e300_write_tripreset.phase_cop.__dti_dest,0xFFFFFFFF,SINT
I903=micro820.micro820.e300data/e300_read_param.fben,0x7A68,BOOL
I904=micro820.micro820.e300data/e300_read_param.ipaddress,0x7A80,STRING
I905=micro820.micro820.e300data/e300_read_param.updaterate_ms,0x7A6C,UINT
I906=micro820.micro820.e300data/e300_read_param.enable,0x7A68,BOOL
I907=micro820.micro820.e300data/e300_read_param.paramnumber,0x7A74,UDINT
I908=micro820.micro820.e300data/e300_read_param.msgobjread.in,0x7A68,BOOL
I909=micro820.micro820.e300data/e300_read_param.msgobjread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I910=micro820.micro820.e300data/e300_read_param.msgobjread.appcfg,0xFFFFFFFF,CIPAPPCFG
I911=micro820.micro820.e300data/e300_read_param.msgobjread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I912=micro820.micro820.e300data/e300_read_param.msgobjread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I913=micro820.micro820.e300data/e300_read_param.msgobjread.reqlength,0x7A6C,UINT
I914=micro820.micro820.e300data/e300_read_param.msgobjread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I915=micro820.micro820.e300data/e300_read_param.msgobjread.__adi_reqdata,0xFFFFFFFF,UINT
I916=micro820.micro820.e300data/e300_read_param.msgobjread.__adi_resdata,0xFFFFFFFF,UINT
I917=micro820.micro820.e300data/e300_read_param.fben_rtrig.clk,0x7A68,BOOL
I918=micro820.micro820.e300data/e300_read_param.msgobjread_q_rtrig.clk,0x7A68,BOOL
I919=micro820.micro820.e300data/e300_read_param.msgobjread_err_rtrig.clk,0x7A68,BOOL
I920=micro820.micro820.e300data/e300_read_param.int_cop.enable,0x7A68,BOOL
I921=micro820.micro820.e300data/e300_read_param.int_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I922=micro820.micro820.e300data/e300_read_param.int_cop.srcoffset,0x7A6C,UINT
I923=micro820.micro820.e300data/e300_read_param.int_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I924=micro820.micro820.e300data/e300_read_param.int_cop.destoffset,0x7A6C,UINT
I925=micro820.micro820.e300data/e300_read_param.int_cop.length,0x7A6C,UINT
I926=micro820.micro820.e300data/e300_read_param.int_cop.swap,0x7A68,BOOL
I927=micro820.micro820.e300data/e300_read_param.int_cop.__adi_src,0xFFFFFFFF,UINT
I928=micro820.micro820.e300data/e300_read_param.int_cop.__adi_dest,0xFFFFFFFF,UINT
I929=micro820.micro820.e300data/e300_read_param.int_cop.__dti_src,0xFFFFFFFF,SINT
I930=micro820.micro820.e300data/e300_read_param.int_cop.__dti_dest,0xFFFFFFFF,SINT
I931=micro820.micro820.e300data/e300_read_param.real_cop.enable,0x7A68,BOOL
I932=micro820.micro820.e300data/e300_read_param.real_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I933=micro820.micro820.e300data/e300_read_param.real_cop.srcoffset,0x7A6C,UINT
I934=micro820.micro820.e300data/e300_read_param.real_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I935=micro820.micro820.e300data/e300_read_param.real_cop.destoffset,0x7A6C,UINT
I936=micro820.micro820.e300data/e300_read_param.real_cop.length,0x7A6C,UINT
I937=micro820.micro820.e300data/e300_read_param.real_cop.swap,0x7A68,BOOL
I938=micro820.micro820.e300data/e300_read_param.real_cop.__adi_src,0xFFFFFFFF,UINT
I939=micro820.micro820.e300data/e300_read_param.real_cop.__adi_dest,0xFFFFFFFF,UINT
I940=micro820.micro820.e300data/e300_read_param.real_cop.__dti_src,0xFFFFFFFF,SINT
I941=micro820.micro820.e300data/e300_read_param.real_cop.__dti_dest,0xFFFFFFFF,SINT
I942=micro820.micro820.e300data/e300_read_param.phase_cop.enable,0x7A68,BOOL
I943=micro820.micro820.e300data/e300_read_param.phase_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I944=micro820.micro820.e300data/e300_read_param.phase_cop.srcoffset,0x7A6C,UINT
I945=micro820.micro820.e300data/e300_read_param.phase_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I946=micro820.micro820.e300data/e300_read_param.phase_cop.destoffset,0x7A6C,UINT
I947=micro820.micro820.e300data/e300_read_param.phase_cop.length,0x7A6C,UINT
I948=micro820.micro820.e300data/e300_read_param.phase_cop.swap,0x7A68,BOOL
I949=micro820.micro820.e300data/e300_read_param.phase_cop.__adi_src,0xFFFFFFFF,UINT
I950=micro820.micro820.e300data/e300_read_param.phase_cop.__adi_dest,0xFFFFFFFF,UINT
I951=micro820.micro820.e300data/e300_read_param.phase_cop.__dti_src,0xFFFFFFFF,SINT
I952=micro820.micro820.e300data/e300_read_param.phase_cop.__dti_dest,0xFFFFFFFF,SINT
I953=micro820.micro820.e300data/e300_read_param.fben_ftrig.clk,0x7A68,BOOL
I954=micro820.micro820.e300data/e300_tripstatuscurrent.msgobjread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I955=micro820.micro820.e300data/e300_tripstatuscurrent.msgobjread.__adi_reqdata,0xFFFFFFFF,UINT
I956=micro820.micro820.e300data/e300_tripstatuscurrent.int_cop.enable,0x7A68,BOOL
I957=micro820.micro820.e300data/e300_tripstatuscurrent.int_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I958=micro820.micro820.e300data/e300_tripstatuscurrent.int_cop.srcoffset,0x7A6C,UINT
I959=micro820.micro820.e300data/e300_tripstatuscurrent.int_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I960=micro820.micro820.e300data/e300_tripstatuscurrent.int_cop.destoffset,0x7A6C,UINT
I961=micro820.micro820.e300data/e300_tripstatuscurrent.int_cop.length,0x7A6C,UINT
I962=micro820.micro820.e300data/e300_tripstatuscurrent.int_cop.swap,0x7A68,BOOL
I963=micro820.micro820.e300data/e300_tripstatuscurrent.int_cop.__adi_src,0xFFFFFFFF,UINT
I964=micro820.micro820.e300data/e300_tripstatuscurrent.int_cop.__adi_dest,0xFFFFFFFF,UINT
I965=micro820.micro820.e300data/e300_tripstatuscurrent.int_cop.__dti_src,0xFFFFFFFF,SINT
I966=micro820.micro820.e300data/e300_tripstatuscurrent.int_cop.__dti_dest,0xFFFFFFFF,SINT
I967=micro820.micro820.e300data/e300_tripstatuscurrent.real_cop.enable,0x7A68,BOOL
I968=micro820.micro820.e300data/e300_tripstatuscurrent.real_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I969=micro820.micro820.e300data/e300_tripstatuscurrent.real_cop.srcoffset,0x7A6C,UINT
I970=micro820.micro820.e300data/e300_tripstatuscurrent.real_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I971=micro820.micro820.e300data/e300_tripstatuscurrent.real_cop.destoffset,0x7A6C,UINT
I972=micro820.micro820.e300data/e300_tripstatuscurrent.real_cop.length,0x7A6C,UINT
I973=micro820.micro820.e300data/e300_tripstatuscurrent.real_cop.swap,0x7A68,BOOL
I974=micro820.micro820.e300data/e300_tripstatuscurrent.real_cop.__adi_src,0xFFFFFFFF,UINT
I975=micro820.micro820.e300data/e300_tripstatuscurrent.real_cop.__adi_dest,0xFFFFFFFF,UINT
I976=micro820.micro820.e300data/e300_tripstatuscurrent.real_cop.__dti_src,0xFFFFFFFF,SINT
I977=micro820.micro820.e300data/e300_tripstatuscurrent.real_cop.__dti_dest,0xFFFFFFFF,SINT
I978=micro820.micro820.e300data/e300_tripstatuscurrent.phase_cop.enable,0x7A68,BOOL
I979=micro820.micro820.e300data/e300_tripstatuscurrent.phase_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I980=micro820.micro820.e300data/e300_tripstatuscurrent.phase_cop.srcoffset,0x7A6C,UINT
I981=micro820.micro820.e300data/e300_tripstatuscurrent.phase_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I982=micro820.micro820.e300data/e300_tripstatuscurrent.phase_cop.destoffset,0x7A6C,UINT
I983=micro820.micro820.e300data/e300_tripstatuscurrent.phase_cop.length,0x7A6C,UINT
I984=micro820.micro820.e300data/e300_tripstatuscurrent.phase_cop.swap,0x7A68,BOOL
I985=micro820.micro820.e300data/e300_tripstatuscurrent.phase_cop.__adi_src,0xFFFFFFFF,UINT
I986=micro820.micro820.e300data/e300_tripstatuscurrent.phase_cop.__adi_dest,0xFFFFFFFF,UINT
I987=micro820.micro820.e300data/e300_tripstatuscurrent.phase_cop.__dti_src,0xFFFFFFFF,SINT
I988=micro820.micro820.e300data/e300_tripstatuscurrent.phase_cop.__dti_dest,0xFFFFFFFF,SINT
I989=micro820.micro820.e300data/e300_tripstatusvoltage.msgobjread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I990=micro820.micro820.e300data/e300_tripstatusvoltage.msgobjread.__adi_reqdata,0xFFFFFFFF,UINT
I991=micro820.micro820.e300data/e300_tripstatusvoltage.int_cop.enable,0x7A68,BOOL
I992=micro820.micro820.e300data/e300_tripstatusvoltage.int_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I993=micro820.micro820.e300data/e300_tripstatusvoltage.int_cop.srcoffset,0x7A6C,UINT
I994=micro820.micro820.e300data/e300_tripstatusvoltage.int_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I995=micro820.micro820.e300data/e300_tripstatusvoltage.int_cop.destoffset,0x7A6C,UINT
I996=micro820.micro820.e300data/e300_tripstatusvoltage.int_cop.length,0x7A6C,UINT
I997=micro820.micro820.e300data/e300_tripstatusvoltage.int_cop.swap,0x7A68,BOOL
I998=micro820.micro820.e300data/e300_tripstatusvoltage.int_cop.__adi_src,0xFFFFFFFF,UINT
I999=micro820.micro820.e300data/e300_tripstatusvoltage.int_cop.__adi_dest,0xFFFFFFFF,UINT
I1000=micro820.micro820.e300data/e300_tripstatusvoltage.int_cop.__dti_src,0xFFFFFFFF,SINT
I1001=micro820.micro820.e300data/e300_tripstatusvoltage.int_cop.__dti_dest,0xFFFFFFFF,SINT
I1002=micro820.micro820.e300data/e300_tripstatusvoltage.real_cop.enable,0x7A68,BOOL
I1003=micro820.micro820.e300data/e300_tripstatusvoltage.real_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1004=micro820.micro820.e300data/e300_tripstatusvoltage.real_cop.srcoffset,0x7A6C,UINT
I1005=micro820.micro820.e300data/e300_tripstatusvoltage.real_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1006=micro820.micro820.e300data/e300_tripstatusvoltage.real_cop.destoffset,0x7A6C,UINT
I1007=micro820.micro820.e300data/e300_tripstatusvoltage.real_cop.length,0x7A6C,UINT
I1008=micro820.micro820.e300data/e300_tripstatusvoltage.real_cop.swap,0x7A68,BOOL
I1009=micro820.micro820.e300data/e300_tripstatusvoltage.real_cop.__adi_src,0xFFFFFFFF,UINT
I1010=micro820.micro820.e300data/e300_tripstatusvoltage.real_cop.__adi_dest,0xFFFFFFFF,UINT
I1011=micro820.micro820.e300data/e300_tripstatusvoltage.real_cop.__dti_src,0xFFFFFFFF,SINT
I1012=micro820.micro820.e300data/e300_tripstatusvoltage.real_cop.__dti_dest,0xFFFFFFFF,SINT
I1013=micro820.micro820.e300data/e300_tripstatusvoltage.phase_cop.enable,0x7A68,BOOL
I1014=micro820.micro820.e300data/e300_tripstatusvoltage.phase_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1015=micro820.micro820.e300data/e300_tripstatusvoltage.phase_cop.srcoffset,0x7A6C,UINT
I1016=micro820.micro820.e300data/e300_tripstatusvoltage.phase_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1017=micro820.micro820.e300data/e300_tripstatusvoltage.phase_cop.destoffset,0x7A6C,UINT
I1018=micro820.micro820.e300data/e300_tripstatusvoltage.phase_cop.length,0x7A6C,UINT
I1019=micro820.micro820.e300data/e300_tripstatusvoltage.phase_cop.swap,0x7A68,BOOL
I1020=micro820.micro820.e300data/e300_tripstatusvoltage.phase_cop.__adi_src,0xFFFFFFFF,UINT
I1021=micro820.micro820.e300data/e300_tripstatusvoltage.phase_cop.__adi_dest,0xFFFFFFFF,UINT
I1022=micro820.micro820.e300data/e300_tripstatusvoltage.phase_cop.__dti_src,0xFFFFFFFF,SINT
I1023=micro820.micro820.e300data/e300_tripstatusvoltage.phase_cop.__dti_dest,0xFFFFFFFF,SINT
I1024=micro820.micro820.e300data/e300_tripstatuspower.msgobjread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I1025=micro820.micro820.e300data/e300_tripstatuspower.msgobjread.__adi_reqdata,0xFFFFFFFF,UINT
I1026=micro820.micro820.e300data/e300_tripstatuspower.int_cop.enable,0x7A68,BOOL
I1027=micro820.micro820.e300data/e300_tripstatuspower.int_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1028=micro820.micro820.e300data/e300_tripstatuspower.int_cop.srcoffset,0x7A6C,UINT
I1029=micro820.micro820.e300data/e300_tripstatuspower.int_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1030=micro820.micro820.e300data/e300_tripstatuspower.int_cop.destoffset,0x7A6C,UINT
I1031=micro820.micro820.e300data/e300_tripstatuspower.int_cop.length,0x7A6C,UINT
I1032=micro820.micro820.e300data/e300_tripstatuspower.int_cop.swap,0x7A68,BOOL
I1033=micro820.micro820.e300data/e300_tripstatuspower.int_cop.__adi_src,0xFFFFFFFF,UINT
I1034=micro820.micro820.e300data/e300_tripstatuspower.int_cop.__adi_dest,0xFFFFFFFF,UINT
I1035=micro820.micro820.e300data/e300_tripstatuspower.int_cop.__dti_src,0xFFFFFFFF,SINT
I1036=micro820.micro820.e300data/e300_tripstatuspower.int_cop.__dti_dest,0xFFFFFFFF,SINT
I1037=micro820.micro820.e300data/e300_tripstatuspower.real_cop.enable,0x7A68,BOOL
I1038=micro820.micro820.e300data/e300_tripstatuspower.real_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1039=micro820.micro820.e300data/e300_tripstatuspower.real_cop.srcoffset,0x7A6C,UINT
I1040=micro820.micro820.e300data/e300_tripstatuspower.real_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1041=micro820.micro820.e300data/e300_tripstatuspower.real_cop.destoffset,0x7A6C,UINT
I1042=micro820.micro820.e300data/e300_tripstatuspower.real_cop.length,0x7A6C,UINT
I1043=micro820.micro820.e300data/e300_tripstatuspower.real_cop.swap,0x7A68,BOOL
I1044=micro820.micro820.e300data/e300_tripstatuspower.real_cop.__adi_src,0xFFFFFFFF,UINT
I1045=micro820.micro820.e300data/e300_tripstatuspower.real_cop.__adi_dest,0xFFFFFFFF,UINT
I1046=micro820.micro820.e300data/e300_tripstatuspower.real_cop.__dti_src,0xFFFFFFFF,SINT
I1047=micro820.micro820.e300data/e300_tripstatuspower.real_cop.__dti_dest,0xFFFFFFFF,SINT
I1048=micro820.micro820.e300data/e300_tripstatuspower.phase_cop.enable,0x7A68,BOOL
I1049=micro820.micro820.e300data/e300_tripstatuspower.phase_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1050=micro820.micro820.e300data/e300_tripstatuspower.phase_cop.srcoffset,0x7A6C,UINT
I1051=micro820.micro820.e300data/e300_tripstatuspower.phase_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1052=micro820.micro820.e300data/e300_tripstatuspower.phase_cop.destoffset,0x7A6C,UINT
I1053=micro820.micro820.e300data/e300_tripstatuspower.phase_cop.length,0x7A6C,UINT
I1054=micro820.micro820.e300data/e300_tripstatuspower.phase_cop.swap,0x7A68,BOOL
I1055=micro820.micro820.e300data/e300_tripstatuspower.phase_cop.__adi_src,0xFFFFFFFF,UINT
I1056=micro820.micro820.e300data/e300_tripstatuspower.phase_cop.__adi_dest,0xFFFFFFFF,UINT
I1057=micro820.micro820.e300data/e300_tripstatuspower.phase_cop.__dti_src,0xFFFFFFFF,SINT
I1058=micro820.micro820.e300data/e300_tripstatuspower.phase_cop.__dti_dest,0xFFFFFFFF,SINT
I1059=micro820.micro820.e300data/e300_tripstatuscontrol.msgobjread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I1060=micro820.micro820.e300data/e300_tripstatuscontrol.msgobjread.__adi_reqdata,0xFFFFFFFF,UINT
I1061=micro820.micro820.e300data/e300_tripstatuscontrol.int_cop.enable,0x7A68,BOOL
I1062=micro820.micro820.e300data/e300_tripstatuscontrol.int_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1063=micro820.micro820.e300data/e300_tripstatuscontrol.int_cop.srcoffset,0x7A6C,UINT
I1064=micro820.micro820.e300data/e300_tripstatuscontrol.int_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1065=micro820.micro820.e300data/e300_tripstatuscontrol.int_cop.destoffset,0x7A6C,UINT
I1066=micro820.micro820.e300data/e300_tripstatuscontrol.int_cop.length,0x7A6C,UINT
I1067=micro820.micro820.e300data/e300_tripstatuscontrol.int_cop.swap,0x7A68,BOOL
I1068=micro820.micro820.e300data/e300_tripstatuscontrol.int_cop.__adi_src,0xFFFFFFFF,UINT
I1069=micro820.micro820.e300data/e300_tripstatuscontrol.int_cop.__adi_dest,0xFFFFFFFF,UINT
I1070=micro820.micro820.e300data/e300_tripstatuscontrol.int_cop.__dti_src,0xFFFFFFFF,SINT
I1071=micro820.micro820.e300data/e300_tripstatuscontrol.int_cop.__dti_dest,0xFFFFFFFF,SINT
I1072=micro820.micro820.e300data/e300_tripstatuscontrol.real_cop.enable,0x7A68,BOOL
I1073=micro820.micro820.e300data/e300_tripstatuscontrol.real_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1074=micro820.micro820.e300data/e300_tripstatuscontrol.real_cop.srcoffset,0x7A6C,UINT
I1075=micro820.micro820.e300data/e300_tripstatuscontrol.real_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1076=micro820.micro820.e300data/e300_tripstatuscontrol.real_cop.destoffset,0x7A6C,UINT
I1077=micro820.micro820.e300data/e300_tripstatuscontrol.real_cop.length,0x7A6C,UINT
I1078=micro820.micro820.e300data/e300_tripstatuscontrol.real_cop.swap,0x7A68,BOOL
I1079=micro820.micro820.e300data/e300_tripstatuscontrol.real_cop.__adi_src,0xFFFFFFFF,UINT
I1080=micro820.micro820.e300data/e300_tripstatuscontrol.real_cop.__adi_dest,0xFFFFFFFF,UINT
I1081=micro820.micro820.e300data/e300_tripstatuscontrol.real_cop.__dti_src,0xFFFFFFFF,SINT
I1082=micro820.micro820.e300data/e300_tripstatuscontrol.real_cop.__dti_dest,0xFFFFFFFF,SINT
I1083=micro820.micro820.e300data/e300_tripstatuscontrol.phase_cop.enable,0x7A68,BOOL
I1084=micro820.micro820.e300data/e300_tripstatuscontrol.phase_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1085=micro820.micro820.e300data/e300_tripstatuscontrol.phase_cop.srcoffset,0x7A6C,UINT
I1086=micro820.micro820.e300data/e300_tripstatuscontrol.phase_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1087=micro820.micro820.e300data/e300_tripstatuscontrol.phase_cop.destoffset,0x7A6C,UINT
I1088=micro820.micro820.e300data/e300_tripstatuscontrol.phase_cop.length,0x7A6C,UINT
I1089=micro820.micro820.e300data/e300_tripstatuscontrol.phase_cop.swap,0x7A68,BOOL
I1090=micro820.micro820.e300data/e300_tripstatuscontrol.phase_cop.__adi_src,0xFFFFFFFF,UINT
I1091=micro820.micro820.e300data/e300_tripstatuscontrol.phase_cop.__adi_dest,0xFFFFFFFF,UINT
I1092=micro820.micro820.e300data/e300_tripstatuscontrol.phase_cop.__dti_src,0xFFFFFFFF,SINT
I1093=micro820.micro820.e300data/e300_tripstatuscontrol.phase_cop.__dti_dest,0xFFFFFFFF,SINT
I1094=micro820.micro820.e300data/e300_warnstatuscurrent.msgobjread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I1095=micro820.micro820.e300data/e300_warnstatuscurrent.msgobjread.__adi_reqdata,0xFFFFFFFF,UINT
I1096=micro820.micro820.e300data/e300_warnstatuscurrent.int_cop.enable,0x7A68,BOOL
I1097=micro820.micro820.e300data/e300_warnstatuscurrent.int_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1098=micro820.micro820.e300data/e300_warnstatuscurrent.int_cop.srcoffset,0x7A6C,UINT
I1099=micro820.micro820.e300data/e300_warnstatuscurrent.int_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1100=micro820.micro820.e300data/e300_warnstatuscurrent.int_cop.destoffset,0x7A6C,UINT
I1101=micro820.micro820.e300data/e300_warnstatuscurrent.int_cop.length,0x7A6C,UINT
I1102=micro820.micro820.e300data/e300_warnstatuscurrent.int_cop.swap,0x7A68,BOOL
I1103=micro820.micro820.e300data/e300_warnstatuscurrent.int_cop.__adi_src,0xFFFFFFFF,UINT
I1104=micro820.micro820.e300data/e300_warnstatuscurrent.int_cop.__adi_dest,0xFFFFFFFF,UINT
I1105=micro820.micro820.e300data/e300_warnstatuscurrent.int_cop.__dti_src,0xFFFFFFFF,SINT
I1106=micro820.micro820.e300data/e300_warnstatuscurrent.int_cop.__dti_dest,0xFFFFFFFF,SINT
I1107=micro820.micro820.e300data/e300_warnstatuscurrent.real_cop.enable,0x7A68,BOOL
I1108=micro820.micro820.e300data/e300_warnstatuscurrent.real_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1109=micro820.micro820.e300data/e300_warnstatuscurrent.real_cop.srcoffset,0x7A6C,UINT
I1110=micro820.micro820.e300data/e300_warnstatuscurrent.real_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1111=micro820.micro820.e300data/e300_warnstatuscurrent.real_cop.destoffset,0x7A6C,UINT
I1112=micro820.micro820.e300data/e300_warnstatuscurrent.real_cop.length,0x7A6C,UINT
I1113=micro820.micro820.e300data/e300_warnstatuscurrent.real_cop.swap,0x7A68,BOOL
I1114=micro820.micro820.e300data/e300_warnstatuscurrent.real_cop.__adi_src,0xFFFFFFFF,UINT
I1115=micro820.micro820.e300data/e300_warnstatuscurrent.real_cop.__adi_dest,0xFFFFFFFF,UINT
I1116=micro820.micro820.e300data/e300_warnstatuscurrent.real_cop.__dti_src,0xFFFFFFFF,SINT
I1117=micro820.micro820.e300data/e300_warnstatuscurrent.real_cop.__dti_dest,0xFFFFFFFF,SINT
I1118=micro820.micro820.e300data/e300_warnstatuscurrent.phase_cop.enable,0x7A68,BOOL
I1119=micro820.micro820.e300data/e300_warnstatuscurrent.phase_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1120=micro820.micro820.e300data/e300_warnstatuscurrent.phase_cop.srcoffset,0x7A6C,UINT
I1121=micro820.micro820.e300data/e300_warnstatuscurrent.phase_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1122=micro820.micro820.e300data/e300_warnstatuscurrent.phase_cop.destoffset,0x7A6C,UINT
I1123=micro820.micro820.e300data/e300_warnstatuscurrent.phase_cop.length,0x7A6C,UINT
I1124=micro820.micro820.e300data/e300_warnstatuscurrent.phase_cop.swap,0x7A68,BOOL
I1125=micro820.micro820.e300data/e300_warnstatuscurrent.phase_cop.__adi_src,0xFFFFFFFF,UINT
I1126=micro820.micro820.e300data/e300_warnstatuscurrent.phase_cop.__adi_dest,0xFFFFFFFF,UINT
I1127=micro820.micro820.e300data/e300_warnstatuscurrent.phase_cop.__dti_src,0xFFFFFFFF,SINT
I1128=micro820.micro820.e300data/e300_warnstatuscurrent.phase_cop.__dti_dest,0xFFFFFFFF,SINT
I1129=micro820.micro820.e300data/e300_warnstatusvoltage.msgobjread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I1130=micro820.micro820.e300data/e300_warnstatusvoltage.msgobjread.__adi_reqdata,0xFFFFFFFF,UINT
I1131=micro820.micro820.e300data/e300_warnstatusvoltage.int_cop.enable,0x7A68,BOOL
I1132=micro820.micro820.e300data/e300_warnstatusvoltage.int_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1133=micro820.micro820.e300data/e300_warnstatusvoltage.int_cop.srcoffset,0x7A6C,UINT
I1134=micro820.micro820.e300data/e300_warnstatusvoltage.int_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1135=micro820.micro820.e300data/e300_warnstatusvoltage.int_cop.destoffset,0x7A6C,UINT
I1136=micro820.micro820.e300data/e300_warnstatusvoltage.int_cop.length,0x7A6C,UINT
I1137=micro820.micro820.e300data/e300_warnstatusvoltage.int_cop.swap,0x7A68,BOOL
I1138=micro820.micro820.e300data/e300_warnstatusvoltage.int_cop.__adi_src,0xFFFFFFFF,UINT
I1139=micro820.micro820.e300data/e300_warnstatusvoltage.int_cop.__adi_dest,0xFFFFFFFF,UINT
I1140=micro820.micro820.e300data/e300_warnstatusvoltage.int_cop.__dti_src,0xFFFFFFFF,SINT
I1141=micro820.micro820.e300data/e300_warnstatusvoltage.int_cop.__dti_dest,0xFFFFFFFF,SINT
I1142=micro820.micro820.e300data/e300_warnstatusvoltage.real_cop.enable,0x7A68,BOOL
I1143=micro820.micro820.e300data/e300_warnstatusvoltage.real_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1144=micro820.micro820.e300data/e300_warnstatusvoltage.real_cop.srcoffset,0x7A6C,UINT
I1145=micro820.micro820.e300data/e300_warnstatusvoltage.real_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1146=micro820.micro820.e300data/e300_warnstatusvoltage.real_cop.destoffset,0x7A6C,UINT
I1147=micro820.micro820.e300data/e300_warnstatusvoltage.real_cop.length,0x7A6C,UINT
I1148=micro820.micro820.e300data/e300_warnstatusvoltage.real_cop.swap,0x7A68,BOOL
I1149=micro820.micro820.e300data/e300_warnstatusvoltage.real_cop.__adi_src,0xFFFFFFFF,UINT
I1150=micro820.micro820.e300data/e300_warnstatusvoltage.real_cop.__adi_dest,0xFFFFFFFF,UINT
I1151=micro820.micro820.e300data/e300_warnstatusvoltage.real_cop.__dti_src,0xFFFFFFFF,SINT
I1152=micro820.micro820.e300data/e300_warnstatusvoltage.real_cop.__dti_dest,0xFFFFFFFF,SINT
I1153=micro820.micro820.e300data/e300_warnstatusvoltage.phase_cop.enable,0x7A68,BOOL
I1154=micro820.micro820.e300data/e300_warnstatusvoltage.phase_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1155=micro820.micro820.e300data/e300_warnstatusvoltage.phase_cop.srcoffset,0x7A6C,UINT
I1156=micro820.micro820.e300data/e300_warnstatusvoltage.phase_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1157=micro820.micro820.e300data/e300_warnstatusvoltage.phase_cop.destoffset,0x7A6C,UINT
I1158=micro820.micro820.e300data/e300_warnstatusvoltage.phase_cop.length,0x7A6C,UINT
I1159=micro820.micro820.e300data/e300_warnstatusvoltage.phase_cop.swap,0x7A68,BOOL
I1160=micro820.micro820.e300data/e300_warnstatusvoltage.phase_cop.__adi_src,0xFFFFFFFF,UINT
I1161=micro820.micro820.e300data/e300_warnstatusvoltage.phase_cop.__adi_dest,0xFFFFFFFF,UINT
I1162=micro820.micro820.e300data/e300_warnstatusvoltage.phase_cop.__dti_src,0xFFFFFFFF,SINT
I1163=micro820.micro820.e300data/e300_warnstatusvoltage.phase_cop.__dti_dest,0xFFFFFFFF,SINT
I1164=micro820.micro820.e300data/e300_warnstatuspower.msgobjread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I1165=micro820.micro820.e300data/e300_warnstatuspower.msgobjread.__adi_reqdata,0xFFFFFFFF,UINT
I1166=micro820.micro820.e300data/e300_warnstatuspower.int_cop.enable,0x7A68,BOOL
I1167=micro820.micro820.e300data/e300_warnstatuspower.int_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1168=micro820.micro820.e300data/e300_warnstatuspower.int_cop.srcoffset,0x7A6C,UINT
I1169=micro820.micro820.e300data/e300_warnstatuspower.int_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1170=micro820.micro820.e300data/e300_warnstatuspower.int_cop.destoffset,0x7A6C,UINT
I1171=micro820.micro820.e300data/e300_warnstatuspower.int_cop.length,0x7A6C,UINT
I1172=micro820.micro820.e300data/e300_warnstatuspower.int_cop.swap,0x7A68,BOOL
I1173=micro820.micro820.e300data/e300_warnstatuspower.int_cop.__adi_src,0xFFFFFFFF,UINT
I1174=micro820.micro820.e300data/e300_warnstatuspower.int_cop.__adi_dest,0xFFFFFFFF,UINT
I1175=micro820.micro820.e300data/e300_warnstatuspower.int_cop.__dti_src,0xFFFFFFFF,SINT
I1176=micro820.micro820.e300data/e300_warnstatuspower.int_cop.__dti_dest,0xFFFFFFFF,SINT
I1177=micro820.micro820.e300data/e300_warnstatuspower.real_cop.enable,0x7A68,BOOL
I1178=micro820.micro820.e300data/e300_warnstatuspower.real_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1179=micro820.micro820.e300data/e300_warnstatuspower.real_cop.srcoffset,0x7A6C,UINT
I1180=micro820.micro820.e300data/e300_warnstatuspower.real_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1181=micro820.micro820.e300data/e300_warnstatuspower.real_cop.destoffset,0x7A6C,UINT
I1182=micro820.micro820.e300data/e300_warnstatuspower.real_cop.length,0x7A6C,UINT
I1183=micro820.micro820.e300data/e300_warnstatuspower.real_cop.swap,0x7A68,BOOL
I1184=micro820.micro820.e300data/e300_warnstatuspower.real_cop.__adi_src,0xFFFFFFFF,UINT
I1185=micro820.micro820.e300data/e300_warnstatuspower.real_cop.__adi_dest,0xFFFFFFFF,UINT
I1186=micro820.micro820.e300data/e300_warnstatuspower.real_cop.__dti_src,0xFFFFFFFF,SINT
I1187=micro820.micro820.e300data/e300_warnstatuspower.real_cop.__dti_dest,0xFFFFFFFF,SINT
I1188=micro820.micro820.e300data/e300_warnstatuspower.phase_cop.enable,0x7A68,BOOL
I1189=micro820.micro820.e300data/e300_warnstatuspower.phase_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1190=micro820.micro820.e300data/e300_warnstatuspower.phase_cop.srcoffset,0x7A6C,UINT
I1191=micro820.micro820.e300data/e300_warnstatuspower.phase_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1192=micro820.micro820.e300data/e300_warnstatuspower.phase_cop.destoffset,0x7A6C,UINT
I1193=micro820.micro820.e300data/e300_warnstatuspower.phase_cop.length,0x7A6C,UINT
I1194=micro820.micro820.e300data/e300_warnstatuspower.phase_cop.swap,0x7A68,BOOL
I1195=micro820.micro820.e300data/e300_warnstatuspower.phase_cop.__adi_src,0xFFFFFFFF,UINT
I1196=micro820.micro820.e300data/e300_warnstatuspower.phase_cop.__adi_dest,0xFFFFFFFF,UINT
I1197=micro820.micro820.e300data/e300_warnstatuspower.phase_cop.__dti_src,0xFFFFFFFF,SINT
I1198=micro820.micro820.e300data/e300_warnstatuspower.phase_cop.__dti_dest,0xFFFFFFFF,SINT
I1199=micro820.micro820.e300data/e300_warnstatuscontrol.msgobjread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000B
I1200=micro820.micro820.e300data/e300_warnstatuscontrol.msgobjread.__adi_reqdata,0xFFFFFFFF,UINT
I1201=micro820.micro820.e300data/e300_warnstatuscontrol.int_cop.enable,0x7A68,BOOL
I1202=micro820.micro820.e300data/e300_warnstatuscontrol.int_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1203=micro820.micro820.e300data/e300_warnstatuscontrol.int_cop.srcoffset,0x7A6C,UINT
I1204=micro820.micro820.e300data/e300_warnstatuscontrol.int_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1205=micro820.micro820.e300data/e300_warnstatuscontrol.int_cop.destoffset,0x7A6C,UINT
I1206=micro820.micro820.e300data/e300_warnstatuscontrol.int_cop.length,0x7A6C,UINT
I1207=micro820.micro820.e300data/e300_warnstatuscontrol.int_cop.swap,0x7A68,BOOL
I1208=micro820.micro820.e300data/e300_warnstatuscontrol.int_cop.__adi_src,0xFFFFFFFF,UINT
I1209=micro820.micro820.e300data/e300_warnstatuscontrol.int_cop.__adi_dest,0xFFFFFFFF,UINT
I1210=micro820.micro820.e300data/e300_warnstatuscontrol.int_cop.__dti_src,0xFFFFFFFF,SINT
I1211=micro820.micro820.e300data/e300_warnstatuscontrol.int_cop.__dti_dest,0xFFFFFFFF,SINT
I1212=micro820.micro820.e300data/e300_warnstatuscontrol.real_cop.enable,0x7A68,BOOL
I1213=micro820.micro820.e300data/e300_warnstatuscontrol.real_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1214=micro820.micro820.e300data/e300_warnstatuscontrol.real_cop.srcoffset,0x7A6C,UINT
I1215=micro820.micro820.e300data/e300_warnstatuscontrol.real_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1216=micro820.micro820.e300data/e300_warnstatuscontrol.real_cop.destoffset,0x7A6C,UINT
I1217=micro820.micro820.e300data/e300_warnstatuscontrol.real_cop.length,0x7A6C,UINT
I1218=micro820.micro820.e300data/e300_warnstatuscontrol.real_cop.swap,0x7A68,BOOL
I1219=micro820.micro820.e300data/e300_warnstatuscontrol.real_cop.__adi_src,0xFFFFFFFF,UINT
I1220=micro820.micro820.e300data/e300_warnstatuscontrol.real_cop.__adi_dest,0xFFFFFFFF,UINT
I1221=micro820.micro820.e300data/e300_warnstatuscontrol.real_cop.__dti_src,0xFFFFFFFF,SINT
I1222=micro820.micro820.e300data/e300_warnstatuscontrol.real_cop.__dti_dest,0xFFFFFFFF,SINT
I1223=micro820.micro820.e300data/e300_warnstatuscontrol.phase_cop.enable,0x7A68,BOOL
I1224=micro820.micro820.e300data/e300_warnstatuscontrol.phase_cop.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1225=micro820.micro820.e300data/e300_warnstatuscontrol.phase_cop.srcoffset,0x7A6C,UINT
I1226=micro820.micro820.e300data/e300_warnstatuscontrol.phase_cop.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1227=micro820.micro820.e300data/e300_warnstatuscontrol.phase_cop.destoffset,0x7A6C,UINT
I1228=micro820.micro820.e300data/e300_warnstatuscontrol.phase_cop.length,0x7A6C,UINT
I1229=micro820.micro820.e300data/e300_warnstatuscontrol.phase_cop.swap,0x7A68,BOOL
I1230=micro820.micro820.e300data/e300_warnstatuscontrol.phase_cop.__adi_src,0xFFFFFFFF,UINT
I1231=micro820.micro820.e300data/e300_warnstatuscontrol.phase_cop.__adi_dest,0xFFFFFFFF,UINT
I1232=micro820.micro820.e300data/e300_warnstatuscontrol.phase_cop.__dti_src,0xFFFFFFFF,SINT
I1233=micro820.micro820.e300data/e300_warnstatuscontrol.phase_cop.__dti_dest,0xFFFFFFFF,SINT
I1234=micro820.micro820.flowtotalizer/cop_1.enable,0x7A68,BOOL
I1235=micro820.micro820.flowtotalizer/cop_1.src,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1236=micro820.micro820.flowtotalizer/cop_1.srcoffset,0x7A6C,UINT
I1237=micro820.micro820.flowtotalizer/cop_1.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I1238=micro820.micro820.flowtotalizer/cop_1.destoffset,0x7A6C,UINT
I1239=micro820.micro820.flowtotalizer/cop_1.length,0x7A6C,UINT
I1240=micro820.micro820.flowtotalizer/cop_1.swap,0x7A68,BOOL
I1241=micro820.micro820.flowtotalizer/cop_1.__adi_src,0xFFFFFFFF,UINT
I1242=micro820.micro820.flowtotalizer/cop_1.__adi_dest,0xFFFFFFFF,UINT
I1243=micro820.micro820.flowtotalizer/cop_1.__dti_src,0xFFFFFFFF,SINT
I1244=micro820.micro820.flowtotalizer/cop_1.__dti_dest,0xFFFFFFFF,SINT
[END]
