# SCADA Tags

| TYPE  | CATEGORY         | NAME                               | DESCRIPTION                                                              | DATATYPE |
|-------|------------------|------------------------------------|--------------------------------------------------------------------------|----------|
| TAG   | Command          | cfg_READ                           | Read configuration from Energy Monitor                                   | BOOL     |
| TAG   | Command          | cfg_WRITE                          | Write configuration to Energy Monitor                                    | BOOL     |
| TAG   | Command          | SCADA_ALM_RESET                    | Reset All Alarms                                                         | BOOL     |
| TAG   | Command          | SCADA_START_PUMP_BIT               | Start from SCADA                                                         | BOOL     |
| TAG   | Command          | SCADA_STOP_PUMP_BIT                | Stop from SCADA                                                          | BOOL     |
| TAG   | Command          | Set_Default_E300_Configuration     | Set E300 to Default Configurations                                       | BOOL     |
| TAG   | Command          | Set_PLC_Time                       | Command to set PLC time                                                  | BOOL     |
| TAG   | Command          | Start_Command                      | Start Command                                                            | BOOL     |
| TAG   | Command          | Stop_Command                       | Stop Command                                                             | BOOL     |
| ALIAS | Command          | TripResetCmd                       | Trip Reset Command                                                       | BOOL     |
| TAG   | Device Config    | cfg_DHSensorDistToIntake           | Feet from Sensor to Pump Intake                                          | REAL     |
| TAG   | Device Config    | cfg_E300_Disabled                  | Energy Monitor is Disabled                                               | BOOL     |
| TAG   | Device Config    | cfg_SpecificGravity                | Fluid Specific Gravity                                                   | REAL     |
| TAG   | Device Config    | DH_Pressure_Shutdown               |                                                                          | REAL     |
| TAG   | Device Config    | DH_Pressure_Shutdown_Enabled       |                                                                          | BOOL     |
| TAG   | Device Config    | DH_Pressure_Startup                |                                                                          | REAL     |
| TAG   | Device Config    | DH_Pressure_Startup_Enabled        |                                                                          | BOOL     |
| TAG   | Device Config    | DH_Temp_Shutdown                   |                                                                          | REAL     |
| TAG   | Device Config    | DH_Temp_Shutdown_Enabled           |                                                                          | BOOL     |
| TAG   | Device Config    | DH_Temp_Startup                    |                                                                          | REAL     |
| TAG   | Device Config    | DH_Temp_Startup_Enabled            |                                                                          | BOOL     |
| TAG   | Device Config    | Downtime_Time_Parameter            | Seconds to wait while tripped for any reason other than Overload         | DINT     |
| TAG   | Device Config    | Downtime_Time_Parameter_OL         | Seconds to wait while tripped for Overload                               | DINT     |
| TAG   | Device Config    | HI_PSI_ALM_SETPOINT                | High Tubing Pressure Alarm Setpoint                                      | REAL     |
| TAG   | Device Config    | Input_DateTime.Day                 | Datetime for setting PLC Datetime from SCADA                             | DINT     |
| TAG   | Device Config    | Input_DateTime.Hour                | Datetime for setting PLC Datetime from SCADA                             | DINT     |
| TAG   | Device Config    | Input_DateTime.Microsecond         | Datetime for setting PLC Datetime from SCADA                             | DINT     |
| TAG   | Device Config    | Input_DateTime.Minute              | Datetime for setting PLC Datetime from SCADA                             | DINT     |
| TAG   | Device Config    | Input_DateTime.Month               | Datetime for setting PLC Datetime from SCADA                             | DINT     |
| TAG   | Device Config    | Input_DateTime.Second              | Datetime for setting PLC Datetime from SCADA                             | DINT     |
| TAG   | Device Config    | Input_DateTime.Year                | Datetime for setting PLC Datetime from SCADA                             | DINT     |
| TAG   | Device Config    | LO_FLOW_ALM_SETPOINT               | Low Flow Alarm Setpoint                                                  | REAL     |
| TAG   | Device Config    | LO_PSI_ALM_SETPOINT                | Low Tubing Pressure Alarm Setpoint                                       | REAL     |
| TAG   | Device Status    | Auto_Mode                          | Auto Mode                                                                | BOOL     |
| TAG   | Device Status    | Contactor_Status                   | Contactor Status                                                         | BOOL     |
| TAG   | Device Status    | DATETIME.Day                       | Current Controller Datetime                                              | DINT     |
| TAG   | Device Status    | DATETIME.Hour                      | Current Controller Datetime                                              | DINT     |
| TAG   | Device Status    | DATETIME.Microsecond               | Current Controller Datetime                                              | DINT     |
| TAG   | Device Status    | DATETIME.Minute                    | Current Controller Datetime                                              | DINT     |
| TAG   | Device Status    | DATETIME.Month                     | Current Controller Datetime                                              | DINT     |
| TAG   | Device Status    | DATETIME.Second                    | Current Controller Datetime                                              | DINT     |
| TAG   | Device Status    | DATETIME.Year                      | Current Controller Datetime                                              | DINT     |
| TAG   | Device Status    | Device_Status                      | Device Status String                                                     | STRING   |
| TAG   | Device Status    | Device_Status_INT                  | Integer for Device Status Indication                                     | DINT     |
| TAG   | Device Status    | DH_DownholeStatus                  | Downhole Monitor Status                                                  | STRING   |
| TAG   | Device Status    | DH_DownholeStatus_INT              | Integer for Downhole Monitor Status                                      | INT      |
| TAG   | Device Status    | Downhole_Tool_Enabled              | Downhole Monitor is Enabled                                              | BOOL     |
| ALIAS | Device Status    | E300_Auto_Mode_Switch              | Auto Mode Switch Input 02 on E300                                        | BOOL     |
| ALIAS | Device Status    | E300_Contactor_Input               | Contactor Status Input 00 on E300                                        | BOOL     |
| ALIAS | Device Status    | E300_Hand_Mode_Switch              | Hand Mode Switch Input 03 on E300                                        | BOOL     |
| ALIAS | Device Status    | E300_Start_Button                  | Start Button Input 01 on E300                                            | BOOL     |
| TAG   | Device Status    | Hand_Mode                          | Hand Mode                                                                | BOOL     |
| TAG   | Device Status    | HI_PSI_SHUTDOWN_ALM                | High Tubing Pressure Alarm Active                                        | BOOL     |
| ALIAS | Device Status    | High_Pressure_Switch               | High Pressure Switch, Fail-Low, (1 = OK)                                 | BOOL     |
| TAG   | Device Status    | HOA_Status                         | HOA position (0 = Auto, 1 = Hand, 2 = Off)                               | BOOL     |
| TAG   | Device Status    | Lightning_Arrestor_Tripped         | Lighning Arrestor is Tripped                                             | BOOL     |
| TAG   | Device Status    | LO_FLOW_ALM                        | Low Flow Alarm Active                                                    | BOOL     |
| TAG   | Device Status    | LO_PSI_SHUTDOWN_ALM                | Low Tubing Pressure Alarm Active                                         | BOOL     |
| TAG   | Device Status    | Off_Mode                           | Off Mode                                                                 | BOOL     |
| TAG   | Device Status    | Overall_Trip_Status                | Overall Trip Status (Mapped from Overall_Trip_Status_INT)                | STRING   |
| TAG   | Device Status    | Overall_Trip_Status_INT            | Overall Trip Status Integer                                              | DINT     |
| TAG   | Device Status    | Overall_Trip_Status_Timestamp      | Overall Trip Status Timestamp                                            | STRING   |
| TAG   | Device Status    | Overall_Warning_Status             | Overall Warning Status (Mapped from Overall_Warning_Status)              | STRING   |
| TAG   | Device Status    | Overall_Warning_Status_INT         | Overall Warning Status Integer                                           | DINT     |
| TAG   | Device Status    | Time_Until_Startup                 | Seconds until device startup                                             | DINT     |
| TAG   | Device Status    | TubingPressure                     | Scaled Tubing Pressure Measurment                                        | REAL     |
| ALIAS | Device Status    | UPS_Buffering                      | UPS is Buffering.                                                        | BOOL     |
| ALIAS | Device Status    | UPS_Ready                          | UPS is Ready                                                             | BOOL     |
| ALIAS | Device Status    | UPS_ReplaceBattery                 | UPS Battery needs Replacing                                              | BOOL     |
| TAG   | Device Status    | UPS_Status_INT                     | UPS Status Integer                                                       | DINT     |
| TAG   | Device Status    | UPS_Status                         | UPS Status String (mapped from UPS_Status_INT)                           | STRING   |
| TAG   | Downhole Monitor | DH_Fluid_Level                     | Fluid Level above the Pump Intake                                        | REAL     |
| TAG   | Downhole Monitor | DH_IntakePressure                  | Pump Intake Pressure (measured at sensor)                                | REAL     |
| TAG   | Downhole Monitor | DH_IntakeTemperature               | Pump Intake Temperature                                                  | REAL     |
| TAG   | Downhole Monitor | DH_Pressure_Offset                 | Ambient Pressure Offset                                                  | REAL     |
| TAG   | Downhole Monitor | DH_PSIRating                       | PSI Rating of Instrument (/1000)                                         | DINT     |
| TAG   | Energy Config    | cfg_GF_GroundFaultInhibitTime      | Ground Fault Inhibit Time                                                | SINT     |
| TAG   | Energy Config    | cfg_GF_GroundFaultTripDelay        | Ground Fault Trip Delay                                                  | REAL     |
| TAG   | Energy Config    | cfg_GF_GroundFaultTripLevel        | Ground Fault Trip Level                                                  | REAL     |
| TAG   | Energy Config    | cfg_GF_GroundFaultWarningDelay     | Ground Fault Warning Delay                                               | REAL     |
| TAG   | Energy Config    | cfg_GF_GroundFaultWarningLevel     | Ground Fault Warning Level                                               | REAL     |
| TAG   | Energy Config    | cfg_I_CTPrimary                    | Current Transformer Primary Ratio                                        | INT      |
| TAG   | Energy Config    | cfg_I_CTSecondary                  | Current Transformer Secondary Ratio                                      | INT      |
| TAG   | Energy Config    | cfg_I_CurrentImbalanceInhibitTime  | Current Imbalance Inhibit Time                                           | SINT     |
| TAG   | Energy Config    | cfg_I_CurrentImbalanceTripDelay    | Current Imbalance Trip Delay                                             | REAL     |
| TAG   | Energy Config    | cfg_I_CurrentImbalanceTripLevel    | Current Imbalance Trip Level                                             | SINT     |
| TAG   | Energy Config    | cfg_I_CurrentImbalanceWarningLevel | Current Imbalance Warning Level                                          | SINT     |
| TAG   | Energy Config    | cfg_I_FLASetting                   | Motor FLA                                                                | REAL     |
| TAG   | Energy Config    | cfg_I_JamInhibitTime               | Jam Inhibit Time                                                         | SINT     |
| TAG   | Energy Config    | cfg_I_JamTripDelay                 | Jam Trip Delay                                                           | REAL     |
| TAG   | Energy Config    | cfg_I_JamTripLevel                 | Jam Trip Level                                                           | INT      |
| TAG   | Energy Config    | cfg_I_JamWarningLevel              | Jam Warning Level                                                        | INT      |
| TAG   | Energy Config    | cfg_I_LineLossInhibitTime          | Line Loss Inhibit Time                                                   | SINT     |
| TAG   | Energy Config    | cfg_I_LineLossTripDelay            | Line Loss Trip Delay                                                     | REAL     |
| TAG   | Energy Config    | cfg_I_OvercurrentInhibitTime       | Overcurrent Inhibit Time                                                 | SINT     |
| TAG   | Energy Config    | cfg_I_OvercurrentTripDelay         | Overcurrent Trip Delay                                                   | REAL     |
| TAG   | Energy Config    | cfg_I_OvercurrentTripLevel         | Overcurrent Trip Level                                                   | SINT     |
| TAG   | Energy Config    | cfg_I_OvercurrentWarningLevel      | Overcurrent Warning Level                                                | SINT     |
| TAG   | Energy Config    | cfg_I_StallEnabledTime             | Stall Enabled Time                                                       | SINT     |
| TAG   | Energy Config    | cfg_I_StallTripLevel               | Stall Trip Level                                                         | INT      |
| TAG   | Energy Config    | cfg_I_UndercurrentInhibitTime      | Undercurrent Inhibit Time                                                | SINT     |
| TAG   | Energy Config    | cfg_I_UndercurrentTripDelay        | Undercurrent Trip Delay                                                  | REAL     |
| TAG   | Energy Config    | cfg_I_UndercurrentTripLevel        | Undercurrent Trip Level                                                  | SINT     |
| TAG   | Energy Config    | cfg_I_UndercurrentWarningLevel     | Undercurrent Warning Level                                               | SINT     |
| TAG   | Energy Config    | cfg_I_UnderloadInhibitTime         | Underload Inhibit Time                                                   | SINT     |
| TAG   | Energy Config    | cfg_I_UnderloadTripDelay           | Underload Trip Delay                                                     | REAL     |
| TAG   | Energy Config    | cfg_I_UnderloadTripLevel           | Underload Trip Level                                                     | SINT     |
| TAG   | Energy Config    | cfg_I_UnderloadWarningLevel        | Underload Warning Level                                                  | SINT     |
| TAG   | Energy Config    | cfg_PL_PhaseLossInhibitTime        | Phase Loss Inhibit Time                                                  | SINT     |
| TAG   | Energy Config    | cfg_PL_PhaseLossTripDelay          | Phase Loss Trip Delay                                                    | REAL     |
| TAG   | Device Config    | cfg_PressureSwitchDisabled         | High Pressure Switch is Disabled                                         | BOOL     |
| TAG   | Energy Config    | cfg_TCU_OLResetLevel               | Thermal Capacity Utilization Overload Reset Level                        | SINT     |
| TAG   | Energy Config    | cfg_TCU_OLWarningLevel             | Thermal Capacity Utilization Overload Warning Level                      | SINT     |
| TAG   | Energy Config    | cfg_TCU_TripClass                  | Thermal Capacity Utilization Trip Class                                  | SINT     |
| TAG   | Energy Config    | cfg_V_OverfrequencyInhibitTime     | Overfrequency Inhibit Time                                               | SINT     |
| TAG   | Energy Config    | cfg_V_OverfrequencyTripDelay       | Overfrequency Trip Delay                                                 | REAL     |
| TAG   | Energy Config    | cfg_V_OverfrequencyTripLevel       | Overfrequency Trip Level                                                 | SINT     |
| TAG   | Energy Config    | cfg_V_OverfrequencyWarningLevel    | Overfrequency Warning Level                                              | SINT     |
| TAG   | Energy Config    | cfg_V_OvervoltageInhibitTime       | Overvoltage Inhibit Time                                                 | SINT     |
| TAG   | Energy Config    | cfg_V_OvervoltageTripDelay         | Overvoltage Trip Delay                                                   | REAL     |
| TAG   | Energy Config    | cfg_V_OvervoltageTripLevel         | Overvoltage Trip Level                                                   | REAL     |
| TAG   | Energy Config    | cfg_V_OvervoltageWarningLevel      | Overvoltage Warning Level                                                | REAL     |
| TAG   | Energy Config    | cfg_V_PhaseRotationInhibitTime     | Phase Rotation Inhibit Time                                              | SINT     |
| TAG   | Energy Config    | cfg_V_PhaseRotationTripType        | Phase Rotation Trip Type (0 = ABC, 1 = ACB)                              | SINT     |
| TAG   | Energy Config    | cfg_V_PTPrimary                    | Potential Transformer Primary Ratio                                      | INT      |
| TAG   | Energy Config    | cfg_V_PTSecondary                  | Potential Transformer Secondary Ratio                                    | INT      |
| TAG   | Energy Config    | cfg_V_UnderfrequencyInhibitTime    | Underfrequency Inhibit Time                                              | SINT     |
| TAG   | Energy Config    | cfg_V_UnderfrequencyTripDelay      | Underfrequency Trip Delay                                                | REAL     |
| TAG   | Energy Config    | cfg_V_UnderfrequencyTripLevel      | Underfrequency Trip Level                                                | SINT     |
| TAG   | Energy Config    | cfg_V_UnderfrequencyWarningLevel   | Underfrequency Warning Level                                             | SINT     |
| TAG   | Energy Config    | cfg_V_UndervoltageInhibitTime      | Undervoltage Inhibit Time                                                | SINT     |
| TAG   | Energy Config    | cfg_V_UndervoltageTripDelay        | Undervoltage Trip Delay                                                  | REAL     |
| TAG   | Energy Config    | cfg_V_UndervoltageTripLevel        | Undervoltage Trip Level                                                  | REAL     |
| TAG   | Energy Config    | cfg_V_UndervoltageWarningLevel     | Undervoltage Warning Level                                               | REAL     |
| TAG   | Energy Config    | cfg_V_VoltageImbalanceInhibitTime  | Voltage Imbalance Inhibit Time                                           | SINT     |
| TAG   | Energy Config    | cfg_V_VoltageImbalanceTripDelay    | Voltage Imbalance Trip Delay                                             | REAL     |
| TAG   | Energy Config    | cfg_V_VoltageImbalanceTripLevel    | Voltage Imbalance Trip Level                                             | SINT     |
| TAG   | Energy Config    | cfg_V_VoltageImbalanceWarningLevel | Voltage Imalance Warning Level                                           | SINT     |
| TAG   | Energy Config    | cfg_V_VoltageMode                  | Voltage Mode ( )                                                         | SINT     |
| TAG   | Energy Config    | TripEnable_I_CurrentImbalance      | Current Imbalance Trip Enabled                                           | BOOL     |
| TAG   | Energy Config    | TripEnable_I_GroundFault           | Ground Fault Trip Enabled                                                | BOOL     |
| TAG   | Energy Config    | TripEnable_I_Jam                   | Jam Trip Enabled                                                         | BOOL     |
| TAG   | Energy Config    | TripEnable_I_LineLoss              | Line Loss Trip Enabled                                                   | BOOL     |
| TAG   | Energy Config    | TripEnable_I_Overcurrent           | Overcurrent Trip Enabled                                                 | BOOL     |
| TAG   | Energy Config    | TripEnable_I_Overload              | Overload Trip Enabled                                                    | BOOL     |
| TAG   | Energy Config    | TripEnable_I_PhaseLoss             | Phase Loss Trip Enabled                                                  | BOOL     |
| TAG   | Energy Config    | TripEnable_I_Stall                 | Stall Trip Enabled                                                       | BOOL     |
| TAG   | Energy Config    | TripEnable_I_Undercurrent          | Undercurrent Trip Enabled                                                | BOOL     |
| TAG   | Energy Config    | TripEnable_I_Underload             | Underload Trip Enabled                                                   | BOOL     |
| TAG   | Energy Config    | TripEnable_V_Overfrequency         | Overfrequency Trip Enabled                                               | BOOL     |
| TAG   | Energy Config    | TripEnable_V_Overvoltage           | Overvoltage Trip Enabled                                                 | BOOL     |
| TAG   | Energy Config    | TripEnable_V_PhaseRotation         | Phase Rotation Trip Enabled                                              | BOOL     |
| TAG   | Energy Config    | TripEnable_V_Underfrequency        | Underfrequency Trip Enabled                                              | BOOL     |
| TAG   | Energy Config    | TripEnable_V_Undervoltage          | Undervoltage Trip Enabled                                                | BOOL     |
| TAG   | Energy Config    | TripEnable_V_VoltageUnbalance      | Voltage Imbalance Trip Enabled                                           | BOOL     |
| TAG   | Energy Config    | WarningEnable_I_CurrentImbalance   | Current Imbalance Warning Enabled                                        | BOOL     |
| TAG   | Energy Config    | WarningEnable_I_GroundFault        | Ground Fault Warning Enabled                                             | BOOL     |
| TAG   | Energy Config    | WarningEnable_I_Jam                | Jam Warning Enabled                                                      | BOOL     |
| TAG   | Energy Config    | WarningEnable_I_LineLoss           | Line Loss Warning Enabled                                                | BOOL     |
| TAG   | Energy Config    | WarningEnable_I_Overcurrent        | Overcurrent Warning Enabled                                              | BOOL     |
| TAG   | Energy Config    | WarningEnable_I_Overload           | Overload Warning Enabled                                                 | BOOL     |
| TAG   | Energy Config    | WarningEnable_I_Undercurrent       | Undercurrent Warning Enabled                                             | BOOL     |
| TAG   | Energy Config    | WarningEnable_I_Underload          | Underload Warning Enabled                                                | BOOL     |
| TAG   | Energy Config    | WarningEnable_V_Overfrequency      | Overfrequency Wanring Enabled                                            | BOOL     |
| TAG   | Energy Config    | WarningEnable_V_Overvoltage        | Overvoltage Warning Enabled                                              | BOOL     |
| TAG   | Energy Config    | WarningEnable_V_PhaseRotation      | Phase Rotation Warning Enabled                                           | BOOL     |
| TAG   | Energy Config    | WarningEnable_V_Underfrequency     | Underfrequency Warning Enabled                                           | BOOL     |
| TAG   | Energy Config    | WarningEnable_V_Undervoltage       | Undervoltage Warning Enabled                                             | BOOL     |
| TAG   | Energy Config    | WarningEnable_V_VoltageUnbalance   | Voltage Imbalance Warning Enabled                                        | BOOL     |
| TAG   | Energy Status    | E300_AverageCurrent                | Average Current                                                          | REAL     |
| TAG   | Energy Status    | E300_AverageLLVoltage              | Average Line-to-Line Voltage                                             | REAL     |
| TAG   | Energy Status    | E300_ControlTripBit                | Control Trip Status Integer (-1 = No Trip)                               | DINT     |
| TAG   | Energy Status    | E300_ControlTripStatus             | Control Trip Status                                                      | STRING   |
| TAG   | Energy Status    | E300_ControlWarningBit             | Control Warning Status Integer (-1 = No Warning)                         | DINT     |
| TAG   | Energy Status    | E300_ControlWarningStatus          | Control Warning Status                                                   | STRING   |
| TAG   | Energy Status    | E300_CurrentTripBit                | Current Trip Status Integers (-1 = No Trip)                              | DINT     |
| TAG   | Energy Status    | E300_CurrentTripStatus             | Current Trip Status                                                      | STRING   |
| TAG   | Energy Status    | E300_CurrentWarningBit             | Current Warning Status Integer (-1= No Warning)                          | DINT     |
| TAG   | Energy Status    | E300_CurrentWarningStatus          | Current Warning Status                                                   | STRING   |
| TAG   | Energy Status    | E300_L1Current                     | L1 Current                                                               | REAL     |
| TAG   | Energy Status    | E300_L1L2Voltage                   | L1-L2 Voltage                                                            | REAL     |
| TAG   | Energy Status    | E300_L2Current                     | L2 Current                                                               | REAL     |
| TAG   | Energy Status    | E300_L2L3Voltage                   | L2-L3 Voltage                                                            | REAL     |
| TAG   | Energy Status    | E300_L3Current                     | L3 Current                                                               | REAL     |
| TAG   | Energy Status    | E300_L3L1Voltage                   | L3-L1 Voltage                                                            | REAL     |
| TAG   | Energy Status    | E300_LineFrequency                 | Line Frequency                                                           | REAL     |
| TAG   | Energy Status    | E300_PercentCurrentUnbalance       | Percent Current Imbalance                                                | REAL     |
| TAG   | Energy Status    | E300_PercentVoltageUnbalance       | Percent Voltage Imbalance                                                | REAL     |
| TAG   | Energy Status    | E300_PhaseRotation                 | Phase Rotation (String)                                                  | STRING   |
| TAG   | Energy Status    | E300_PhaseRotation_INT             | Phase Rotation Integer                                                   | DINT     |
| TAG   | Energy Status    | E300_PowerTripBit                  | Power Trip Status Integer (-1 = No Trip)                                 | DINT     |
| TAG   | Energy Status    | E300_PowerTripStatus               | Power Trip Status                                                        | STRING   |
| TAG   | Energy Status    | E300_PowerWarningBit               | Power Warning Status Integer (-1 = No Warning)                           | DINT     |
| TAG   | Energy Status    | E300_PowerWarningStatus            | Power Warning Status                                                     | STRING   |
| TAG   | Energy Status    | E300_ThreePhaseTruePowerFactor     | True 3-Phase Power Factor                                                | REAL     |
| TAG   | Energy Status    | E300_TotalApparentPower            | Total Apparent Power (kVA)                                               | REAL     |
| TAG   | Energy Status    | E300_TotalReactivePower            | Total Reactive Power (kVAR)                                              | REAL     |
| TAG   | Energy Status    | E300_TotalRealPower                | Total Real Power (kW)                                                    | REAL     |
| TAG   | Energy Status    | E300_VoltageTripBit                | Voltage Trip Status Integer (-1 = No Trip)                               | DINT     |
| TAG   | Energy Status    | E300_VoltageTripStatus             | Voltage Trip Status                                                      | STRING   |
| TAG   | Energy Status    | E300_VoltageWarningBit             | Voltage Warning Status Integer (-1 = No Warning)                         | DINT     |
| TAG   | Energy Status    | E300_VoltageWarningStatus          | Voltage Warning Status                                                   | STRING   |
| ALIAS | Energy Status    | TripStatus                         | Trip Present                                                             | BOOL     |
| TAG   | Energy Status    | VoltageOK                          | Voltage is within the tolerable Limits                                   | BOOL     |
| TAG   | Flow             | FlowRate                           | Scaled Flow Rate                                                         | REAL     |
| ALIAS | Flow             | Flowmeter_HART_Failure             | Communication Failure between HART card and Flowmeter                    | BOOL     |
| TAG   | Flow             | LASTMONTH_TOTAL_BBL                | Last Month Total BBL                                                     | REAL     |
| TAG   | Flow             | LASTMONTH_TOTAL_RUN_TIME_HOURS     | Last Month Total Runtime Hours                                           | REAL     |
| TAG   | Flow             | THISMONTH_TOTAL_BBL                | This Month Total BBL                                                     | REAL     |
| TAG   | Flow             | THISMONTH_TOTAL_RUN_TIME_HOURS     | This Month Total Runtime Hours                                           | REAL     |
| TAG   | Flow             | TODAY_TOTAL_BBL                    | Today's Total BBL                                                        | REAL     |
| TAG   | Flow             | TODAY_TOTAL_RUN_TIME_HOURS         | Today's Total Runtime Hours                                              | REAL     |
| TAG   | Flow             | YESTERDAY_TOTAL_BBL                | Yesterday's Total BBL                                                    | REAL     |
| TAG   | Flow             | YESTERDAY_TOTAL_RUN_TIME_HOURS     | Testerday's Total Runtime Hours                                          | REAL     |
| TAG   | Permissive       | RP_Flow                            | Run not prevented by Flow                                                | BOOL     |
| TAG   | Permissive       | RP_Mode                            | Run not prevented by Mode                                                | BOOL     |
| TAG   | Permissive       | RP_Pressure                        | Run not prevented by Downhole Pressure                                   | BOOL     |
| TAG   | Permissive       | RP_Remote                          | Run not prevented by Remote Trip                                         | BOOL     |
| TAG   | Permissive       | RP_Temperature                     | Run not prevented by Downhole Temperature                                | BOOL     |
| TAG   | Permissive       | RP_Trip                            | Run not prevented by Energy Trip                                         | BOOL     |
| TAG   | Permissive       | RP_TubingPressure                  | Run not prevented by Tubing Pressure                                     | BOOL     |
| TAG   | Permissive       | Run_Permissive                     | Run not prevented                                                        | BOOL     |
| TAG   | Permissive       | SP_Mode                            | Startup not prevented by Mode                                            | BOOL     |
| TAG   | Permissive       | SP_Pressure                        | Startup not prevented by Downhole Pressure                               | BOOL     |
| TAG   | Permissive       | SP_Remote                          | Startup not prevented by Remote Trip                                     | BOOL     |
| TAG   | Permissive       | SP_Temperature                     | Startup not prevented by Downhole Temperature                            | BOOL     |
| TAG   | Permissive       | SP_Trip                            | Startup not prevented by Energy Trip                                     | BOOL     |
| TAG   | Permissive       | SP_Voltage                         | Startup not prevented by Voltage                                         | BOOL     |
| TAG   | Permissive       | Start_Permissive                   | Startup not prevented                                                    | BOOL     |
| TAG   | Watchdog         | datalogger_watchdog                | DataLogger Handshake: Datalogger will write 1 to this tag when it sees 0 | BOOL     |
| TAG   | Watchdog         | Datalogger_Watchdog_Timeout        | The datalogger is not communicating with the PLC                         | BOOL     |
