+---------------------------------------------------------------+
| Configuration listing for channel 1                          |
+---------------------------------------------------------------+
| COMPANY = Woodhead Software & Electronics
| DATE    = Tuesday, March 14, 2017 At 10:01
| VERSION = v1.0.0
| CONFIGURATION NAME = HP_DOWNHOLE_SENSOR_STD
| BOARD LOCATION = The configuration type has been modified. You must restart all the applications communicating with the %s cards.
+---------------------------------------------------------------+
-----------------------------------------------------------------
Master Information
-----------------------------------------------------------------
  
  >> Serial Port Configuration :
     Network format                     = RS485/RS422                        
     Baud Rate                          = 38400 bits/s                       
     Parity Control                     = NONE                               
     Stop bit(s)                        = 1 Bit                              
  
  >> Protocol Configuration :
     Inter-frames Silence               = 0                        ms        
     Mode                               = RTU                                
     Request Time-out                   = 10                       s         
     Max. Request                       = 1                                  
-----------------------------------------------------------------
Equipment 0
-----------------------------------------------------------------
  Broadcast Reserved Address
-----------------------------------------------------------------
Equipment 1
-----------------------------------------------------------------
  Modbus Generic
  
  >> applicom information :
     Topic Name                         = DHSENSOR                           
     Comment                            =                                    
  
  >> Network Configuration :
     Time-out                           = 1000                     ms        
     Nb of Repetitions on CRC, Time-out = 2                                  
     Nb of Repetitions on Error 4       = 0                                  
     Slave number                       = 234                                
  
  >> Messaging Configuration :
     Maximum Number of simultaneus Reque= 1                                  
     Maximum Bits Reading               = 2040                               
     Maximum Bits Writing               = 2040                               
     Maximum Words Reading              = 127                                
     Maximum Words Writing              = 127                                
     Double/floating word format        = Little Endian (Intel)              
     Single Word Writing Support        = Yes                                
     Single Bit Writing Support         = Yes                                
