+---------------------------------------------------------------+
| Configuration listing for channel 0                          |
+---------------------------------------------------------------+
| COMPANY = Woodhead Software & Electronics
| DATE    = Monday, September 12, 2016 At 23:47
| VERSION = v1.0.0
| CONFIGURATION NAME = HP_DOWNHOLE_SENSOR_STD
| BOARD LOCATION = The configuration type has been modified. You must restart all the applications communicating with the %s cards.
+---------------------------------------------------------------+
-----------------------------------------------------------------
Channel Information
-----------------------------------------------------------------
  
  >> General :
     Request Time-out                   = 10                       s         
     Max. Request                       = 4                                  
     Server Mode Turnaround Time        = 2                        x10 ms    
     Client Equipment Access Indicator S= Inactive                           
     Access Indicator Address           = 0                                  
     Client Equipment Access Status Stor= Inactive                           
     Access Status Address              = 0                                  
  
  >> Ethernet :
     Connection Type                    = RJ45                               
     Baud Rate                          = Auto 10/100 Mb                     
     Frame format                       = Ethernet II                        
     Connection Lifetime                = 3                        Minutes   
     Automatic Address Calculation      = Automatic Address                  
     Ethernet Address                   = 00-A0-91-XX-XX-XX                  
