# Multi-Sensor

Connect up to 8 analog signals to be monitored by POCloud!

## Configuration

All configuration can be done via the POCloud interface.

### Scaling Parameters

Scaling defaults to EU values of 4.0 to 20.0

### Pond Configuration

To configure the input to be a pond, click the Pond Enable button. Strapping table measurements can be input below the scaling parameters.

