[BEGIN FB INPUTS]
I1=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.enable,0x458,BOOL
I2=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.src,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I3=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.srcoffset,0x44B2,UINT
I4=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I5=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.destoffset,0x44BA,UINT
I6=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.length,0x44BC,UINT
I7=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.swap,0x458,BOOL
I8=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.__adi_src,0xFFFFFFFF,UINT
I9=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.__adi_dest,0xFFFFFFFF,UINT
I10=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.__dti_src,0xFFFFFFFF,SINT
I11=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.__dti_dest,0xFFFFFFFF,SINT
I12=micro820.micro820.vfd_messaging/vfd.cop_drvtype.enable,0x458,BOOL
I13=micro820.micro820.vfd_messaging/vfd.cop_drvtype.src,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I14=micro820.micro820.vfd_messaging/vfd.cop_drvtype.srcoffset,0x44BA,UINT
I15=micro820.micro820.vfd_messaging/vfd.cop_drvtype.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I16=micro820.micro820.vfd_messaging/vfd.cop_drvtype.destoffset,0x44BA,UINT
I17=micro820.micro820.vfd_messaging/vfd.cop_drvtype.length,0x44BC,UINT
I18=micro820.micro820.vfd_messaging/vfd.cop_drvtype.swap,0x459,BOOL
I19=micro820.micro820.vfd_messaging/vfd.cop_drvtype.__adi_src,0xFFFFFFFF,UINT
I20=micro820.micro820.vfd_messaging/vfd.cop_drvtype.__adi_dest,0xFFFFFFFF,UINT
I21=micro820.micro820.vfd_messaging/vfd.cop_drvtype.__dti_src,0xFFFFFFFF,SINT
I22=micro820.micro820.vfd_messaging/vfd.cop_drvtype.__dti_dest,0xFFFFFFFF,SINT
I23=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.enable,0x458,BOOL
I24=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.src,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I25=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.srcoffset,0x44A6,UINT
I26=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I27=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.destoffset,0x44BA,UINT
I28=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.length,0x44BC,UINT
I29=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.swap,0x458,BOOL
I30=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.__adi_src,0xFFFFFFFF,UINT
I31=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.__adi_dest,0xFFFFFFFF,UINT
I32=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.__dti_src,0xFFFFFFFF,SINT
I33=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.__dti_dest,0xFFFFFFFF,SINT
I34=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.enable,0x458,BOOL
I35=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.src,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I36=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.srcoffset,0x44A2,UINT
I37=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I38=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.destoffset,0x44BA,UINT
I39=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.length,0x44BC,UINT
I40=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.swap,0x458,BOOL
I41=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.__adi_src,0xFFFFFFFF,UINT
I42=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.__adi_dest,0xFFFFFFFF,UINT
I43=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.__dti_src,0xFFFFFFFF,SINT
I44=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.__dti_dest,0xFFFFFFFF,SINT
I45=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.enable,0x458,BOOL
I46=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.src,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I47=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.srcoffset,0x44B2,UINT
I48=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I49=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.destoffset,0x44BA,UINT
I50=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.length,0x44BC,UINT
I51=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.swap,0x458,BOOL
I52=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.__adi_src,0xFFFFFFFF,UINT
I53=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.__adi_dest,0xFFFFFFFF,UINT
I54=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.__dti_src,0xFFFFFFFF,SINT
I55=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.__dti_dest,0xFFFFFFFF,SINT
I56=micro820.micro820.vfd_messaging/vfd.cop_speedref.enable,0x458,BOOL
I57=micro820.micro820.vfd_messaging/vfd.cop_speedref.src,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I58=micro820.micro820.vfd_messaging/vfd.cop_speedref.srcoffset,0x44BA,UINT
I59=micro820.micro820.vfd_messaging/vfd.cop_speedref.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I60=micro820.micro820.vfd_messaging/vfd.cop_speedref.destoffset,0x44BA,UINT
I61=micro820.micro820.vfd_messaging/vfd.cop_speedref.length,0x44B2,UINT
I62=micro820.micro820.vfd_messaging/vfd.cop_speedref.swap,0x458,BOOL
I63=micro820.micro820.vfd_messaging/vfd.cop_speedref.__adi_src,0xFFFFFFFF,UINT
I64=micro820.micro820.vfd_messaging/vfd.cop_speedref.__adi_dest,0xFFFFFFFF,UINT
I65=micro820.micro820.vfd_messaging/vfd.cop_speedref.__dti_src,0xFFFFFFFF,SINT
I66=micro820.micro820.vfd_messaging/vfd.cop_speedref.__dti_dest,0xFFFFFFFF,SINT
I67=micro820.micro820.vfd_messaging/vfd.cop_deceltime.enable,0x458,BOOL
I68=micro820.micro820.vfd_messaging/vfd.cop_deceltime.src,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I69=micro820.micro820.vfd_messaging/vfd.cop_deceltime.srcoffset,0x44BA,UINT
I70=micro820.micro820.vfd_messaging/vfd.cop_deceltime.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I71=micro820.micro820.vfd_messaging/vfd.cop_deceltime.destoffset,0x44BA,UINT
I72=micro820.micro820.vfd_messaging/vfd.cop_deceltime.length,0x44B2,UINT
I73=micro820.micro820.vfd_messaging/vfd.cop_deceltime.swap,0x458,BOOL
I74=micro820.micro820.vfd_messaging/vfd.cop_deceltime.__adi_src,0xFFFFFFFF,UINT
I75=micro820.micro820.vfd_messaging/vfd.cop_deceltime.__adi_dest,0xFFFFFFFF,UINT
I76=micro820.micro820.vfd_messaging/vfd.cop_deceltime.__dti_src,0xFFFFFFFF,SINT
I77=micro820.micro820.vfd_messaging/vfd.cop_deceltime.__dti_dest,0xFFFFFFFF,SINT
I78=micro820.micro820.vfd_messaging/vfd.cop_acceltime.enable,0x458,BOOL
I79=micro820.micro820.vfd_messaging/vfd.cop_acceltime.src,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I80=micro820.micro820.vfd_messaging/vfd.cop_acceltime.srcoffset,0x44BA,UINT
I81=micro820.micro820.vfd_messaging/vfd.cop_acceltime.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I82=micro820.micro820.vfd_messaging/vfd.cop_acceltime.destoffset,0x44BA,UINT
I83=micro820.micro820.vfd_messaging/vfd.cop_acceltime.length,0x44B2,UINT
I84=micro820.micro820.vfd_messaging/vfd.cop_acceltime.swap,0x458,BOOL
I85=micro820.micro820.vfd_messaging/vfd.cop_acceltime.__adi_src,0xFFFFFFFF,UINT
I86=micro820.micro820.vfd_messaging/vfd.cop_acceltime.__adi_dest,0xFFFFFFFF,UINT
I87=micro820.micro820.vfd_messaging/vfd.cop_acceltime.__dti_src,0xFFFFFFFF,SINT
I88=micro820.micro820.vfd_messaging/vfd.cop_acceltime.__dti_dest,0xFFFFFFFF,SINT
I89=micro820.micro820.vfd_messaging/vfd.cop_faultcode.enable,0x458,BOOL
I90=micro820.micro820.vfd_messaging/vfd.cop_faultcode.src,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I91=micro820.micro820.vfd_messaging/vfd.cop_faultcode.srcoffset,0x44B6,UINT
I92=micro820.micro820.vfd_messaging/vfd.cop_faultcode.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I93=micro820.micro820.vfd_messaging/vfd.cop_faultcode.destoffset,0x44BA,UINT
I94=micro820.micro820.vfd_messaging/vfd.cop_faultcode.length,0x44BC,UINT
I95=micro820.micro820.vfd_messaging/vfd.cop_faultcode.swap,0x458,BOOL
I96=micro820.micro820.vfd_messaging/vfd.cop_faultcode.__adi_src,0xFFFFFFFF,UINT
I97=micro820.micro820.vfd_messaging/vfd.cop_faultcode.__adi_dest,0xFFFFFFFF,UINT
I98=micro820.micro820.vfd_messaging/vfd.cop_faultcode.__dti_src,0xFFFFFFFF,SINT
I99=micro820.micro820.vfd_messaging/vfd.cop_faultcode.__dti_dest,0xFFFFFFFF,SINT
I100=micro820.micro820.readdownholedata/modbuscycletimer.in,0x4431,BOOL
I101=micro820.micro820.readdownholedata/modbuscycletimer.pt,0x56C,TIME
I102=micro820.micro820.vfd_configmap/vfd_writetimer.in,0x491,BOOL
I103=micro820.micro820.vfd_configmap/vfd_writetimer.pt,0x590,TIME
I104=micro820.micro820.vfd_configmap/vfd_readtimer.in,0x487,BOOL
I105=micro820.micro820.vfd_configmap/vfd_readtimer.pt,0x590,TIME
I106=micro820.micro820.vfd_configmap/vfd_r_nphp.fben,0x487,BOOL
I107=micro820.micro820.vfd_configmap/vfd_r_nphp.ipaddress,0x792,STRING
I108=micro820.micro820.vfd_configmap/vfd_r_nphp.updaterate_ms,0x44D4,UINT
I109=micro820.micro820.vfd_configmap/vfd_r_nphp.parameternumber,0x44D2,UINT
I110=micro820.micro820.vfd_configmap/vfd_r_npfla.fben,0x487,BOOL
I111=micro820.micro820.vfd_configmap/vfd_r_npfla.ipaddress,0x792,STRING
I112=micro820.micro820.vfd_configmap/vfd_r_npfla.updaterate_ms,0x44D4,UINT
I113=micro820.micro820.vfd_configmap/vfd_r_npfla.parameternumber,0x44D0,UINT
I114=micro820.micro820.vfd_configmap/vfd_r_npvolts.fben,0x487,BOOL
I115=micro820.micro820.vfd_configmap/vfd_r_npvolts.ipaddress,0x792,STRING
I116=micro820.micro820.vfd_configmap/vfd_r_npvolts.updaterate_ms,0x44D4,UINT
I117=micro820.micro820.vfd_configmap/vfd_r_npvolts.parameternumber,0x44CE,UINT
I118=micro820.micro820.vfd_configmap/vfd_r_nphz.fben,0x487,BOOL
I119=micro820.micro820.vfd_configmap/vfd_r_nphz.ipaddress,0x792,STRING
I120=micro820.micro820.vfd_configmap/vfd_r_nphz.updaterate_ms,0x44D4,UINT
I121=micro820.micro820.vfd_configmap/vfd_r_nphz.parameternumber,0x44CC,UINT
I122=micro820.micro820.vfd_configmap/vfd_r_nprpm.fben,0x487,BOOL
I123=micro820.micro820.vfd_configmap/vfd_r_nprpm.ipaddress,0x792,STRING
I124=micro820.micro820.vfd_configmap/vfd_r_nprpm.updaterate_ms,0x44D4,UINT
I125=micro820.micro820.vfd_configmap/vfd_r_nprpm.parameternumber,0x44CA,UINT
I126=micro820.micro820.vfd_configmap/vfd_r_npolcurrent.fben,0x487,BOOL
I127=micro820.micro820.vfd_configmap/vfd_r_npolcurrent.ipaddress,0x792,STRING
I128=micro820.micro820.vfd_configmap/vfd_r_npolcurrent.updaterate_ms,0x44D4,UINT
I129=micro820.micro820.vfd_configmap/vfd_r_npolcurrent.parameternumber,0x44C8,UINT
I130=micro820.micro820.vfd_configmap/vfd_r_motorpoles.fben,0x487,BOOL
I131=micro820.micro820.vfd_configmap/vfd_r_motorpoles.ipaddress,0x792,STRING
I132=micro820.micro820.vfd_configmap/vfd_r_motorpoles.updaterate_ms,0x44D4,UINT
I133=micro820.micro820.vfd_configmap/vfd_r_motorpoles.parameternumber,0x44C6,UINT
I134=micro820.micro820.vfd_configmap/vfd_r_maxfreq.fben,0x487,BOOL
I135=micro820.micro820.vfd_configmap/vfd_r_maxfreq.ipaddress,0x792,STRING
I136=micro820.micro820.vfd_configmap/vfd_r_maxfreq.updaterate_ms,0x44D4,UINT
I137=micro820.micro820.vfd_configmap/vfd_r_maxfreq.parameternumber,0x44C4,UINT
I138=micro820.micro820.vfd_configmap/vfd_r_minfreq.fben,0x487,BOOL
I139=micro820.micro820.vfd_configmap/vfd_r_minfreq.ipaddress,0x792,STRING
I140=micro820.micro820.vfd_configmap/vfd_r_minfreq.updaterate_ms,0x44D4,UINT
I141=micro820.micro820.vfd_configmap/vfd_r_minfreq.parameternumber,0x44C2,UINT
I142=micro820.micro820.vfd_configmap/vfd_r_stopmode.fben,0x487,BOOL
I143=micro820.micro820.vfd_configmap/vfd_r_stopmode.ipaddress,0x792,STRING
I144=micro820.micro820.vfd_configmap/vfd_r_stopmode.updaterate_ms,0x44D4,UINT
I145=micro820.micro820.vfd_configmap/vfd_r_stopmode.parameternumber,0x44C0,UINT
I146=micro820.micro820.vfd_configmap/vfd_r_torqueperfmode.fben,0x487,BOOL
I147=micro820.micro820.vfd_configmap/vfd_r_torqueperfmode.ipaddress,0x792,STRING
I148=micro820.micro820.vfd_configmap/vfd_r_torqueperfmode.updaterate_ms,0x44D4,UINT
I149=micro820.micro820.vfd_configmap/vfd_r_torqueperfmode.parameternumber,0x44BE,UINT
I150=micro820.micro820.control/linearscale_pressure.raw_min,0x4BF8,REAL
I151=micro820.micro820.control/linearscale_pressure.raw_max,0x4BF4,REAL
I152=micro820.micro820.control/linearscale_pressure.eu_min,0x508,REAL
I153=micro820.micro820.control/linearscale_pressure.eu_max,0x50C,REAL
I154=micro820.micro820.control/linearscale_pressure.raw_inp,0x4C08,REAL
I155=micro820.micro820.vfd_messaging/vfd.fben,0x4437,BOOL
I156=micro820.micro820.vfd_messaging/vfd.ipaddress,0x792,STRING
I157=micro820.micro820.vfd_messaging/vfd.updaterate_ms,0x44D4,UINT
I158=micro820.micro820.vfd_messaging/vfd.enetctrlto_sec,0x4479,USINT
I159=micro820.micro820.vfd_messaging/vfd.stop,0x47A,BOOL
I160=micro820.micro820.vfd_messaging/vfd.start,0x47B,BOOL
I161=micro820.micro820.vfd_messaging/vfd.jog,0x47C,BOOL
I162=micro820.micro820.vfd_messaging/vfd.clrfault,0x47D,BOOL
I163=micro820.micro820.vfd_messaging/vfd.setfwd,0x458,BOOL
I164=micro820.micro820.vfd_messaging/vfd.setrev,0x459,BOOL
I165=micro820.micro820.vfd_messaging/vfd.speedref,0x514,REAL
I166=micro820.micro820.vfd_messaging/vfd.acceltime1,0x518,REAL
I167=micro820.micro820.vfd_messaging/vfd.deceltime1,0x51C,REAL
I168=micro820.micro820.vfd_configmap/vfd_r_nphp.msgparread_err_rtrig.clk,0x4448,BOOL
I169=micro820.micro820.vfd_configmap/vfd_r_nphp.msgparread_q_rtrig.clk,0x4448,BOOL
I170=micro820.micro820.vfd_configmap/vfd_r_nphp.fben_rtrig.clk,0x4448,BOOL
I171=micro820.micro820.vfd_messaging/vfd.msgtimeout_q_rtrig.clk,0x4448,BOOL
I172=micro820.micro820.vfd_messaging/vfd.msgparread_err_rtrig.clk,0x4448,BOOL
I173=micro820.micro820.vfd_messaging/vfd.msgparwrite_q_rtrig.clk,0x4448,BOOL
I174=micro820.micro820.vfd_messaging/vfd.msgparread_q_rtrig.clk,0x4448,BOOL
I175=micro820.micro820.vfd_messaging/vfd.fben_rtrig.clk,0x4448,BOOL
I176=micro820.micro820.vfd_messaging/vfd.msgtimeout_err_rtrig.clk,0x4448,BOOL
I177=micro820.micro820.vfd_messaging/vfd.msgsts_err_rtrig.clk,0x4448,BOOL
I178=micro820.micro820.vfd_messaging/vfd.msgcmd_err_rtrig.clk,0x4448,BOOL
I179=micro820.micro820.vfd_messaging/vfd.msgdrvtype_q_rtrig.clk,0x4448,BOOL
I180=micro820.micro820.vfd_messaging/vfd.msgdrvtype_err_rtrig.clk,0x4448,BOOL
I181=micro820.micro820.vfd_messaging/vfd.msgsts_q_rtrig.clk,0x4448,BOOL
I182=micro820.micro820.vfd_messaging/vfd.msgparwrite_err_rtrig.clk,0x4448,BOOL
I183=micro820.micro820.vfd_messaging/vfd.msgcmd_q_rtrig.clk,0x4448,BOOL
I184=micro820.micro820.vfd_configmap/vfd_w_nphp.msgtimeout_q_rtrig.clk,0x4448,BOOL
I185=micro820.micro820.vfd_configmap/vfd_w_nphp.msgparwrite_q_rtrig.clk,0x4448,BOOL
I186=micro820.micro820.vfd_configmap/vfd_w_nphp.fben_rtrig.clk,0x4448,BOOL
I187=micro820.micro820.vfd_configmap/vfd_w_nphp.msgtimeout_err_rtrig.clk,0x4448,BOOL
I188=micro820.micro820.vfd_configmap/vfd_w_nphp.msgparwrite_err_rtrig.clk,0x4448,BOOL
I189=micro820.micro820.vfd_configmap/vfd_r_npfla.msgparread_err_rtrig.clk,0x4448,BOOL
I190=micro820.micro820.vfd_configmap/vfd_r_npfla.msgparread_q_rtrig.clk,0x4448,BOOL
I191=micro820.micro820.vfd_configmap/vfd_r_npfla.fben_rtrig.clk,0x4448,BOOL
I192=micro820.micro820.vfd_configmap/vfd_w_npfla.msgtimeout_q_rtrig.clk,0x4448,BOOL
I193=micro820.micro820.vfd_configmap/vfd_w_npfla.msgparwrite_q_rtrig.clk,0x4448,BOOL
I194=micro820.micro820.vfd_configmap/vfd_w_npfla.fben_rtrig.clk,0x4448,BOOL
I195=micro820.micro820.vfd_configmap/vfd_w_npfla.msgtimeout_err_rtrig.clk,0x4448,BOOL
I196=micro820.micro820.vfd_configmap/vfd_w_npfla.msgparwrite_err_rtrig.clk,0x4448,BOOL
I197=micro820.micro820.vfd_configmap/vfd_r_npvolts.msgparread_err_rtrig.clk,0x4448,BOOL
I198=micro820.micro820.vfd_configmap/vfd_r_npvolts.msgparread_q_rtrig.clk,0x4448,BOOL
I199=micro820.micro820.vfd_configmap/vfd_r_npvolts.fben_rtrig.clk,0x4448,BOOL
I200=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgtimeout_q_rtrig.clk,0x4448,BOOL
I201=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgparwrite_q_rtrig.clk,0x4448,BOOL
I202=micro820.micro820.vfd_configmap/vfd_w_npvolts.fben_rtrig.clk,0x4448,BOOL
I203=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgtimeout_err_rtrig.clk,0x4448,BOOL
I204=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgparwrite_err_rtrig.clk,0x4448,BOOL
I205=micro820.micro820.vfd_configmap/vfd_r_nphz.msgparread_err_rtrig.clk,0x4448,BOOL
I206=micro820.micro820.vfd_configmap/vfd_r_nphz.msgparread_q_rtrig.clk,0x4448,BOOL
I207=micro820.micro820.vfd_configmap/vfd_r_nphz.fben_rtrig.clk,0x4448,BOOL
I208=micro820.micro820.vfd_configmap/vfd_w_nphz.msgtimeout_q_rtrig.clk,0x4448,BOOL
I209=micro820.micro820.vfd_configmap/vfd_w_nphz.msgparwrite_q_rtrig.clk,0x4448,BOOL
I210=micro820.micro820.vfd_configmap/vfd_w_nphz.fben_rtrig.clk,0x4448,BOOL
I211=micro820.micro820.vfd_configmap/vfd_w_nphz.msgtimeout_err_rtrig.clk,0x4448,BOOL
I212=micro820.micro820.vfd_configmap/vfd_w_nphz.msgparwrite_err_rtrig.clk,0x4448,BOOL
I213=micro820.micro820.vfd_configmap/vfd_r_nprpm.msgparread_err_rtrig.clk,0x4448,BOOL
I214=micro820.micro820.vfd_configmap/vfd_r_nprpm.msgparread_q_rtrig.clk,0x4448,BOOL
I215=micro820.micro820.vfd_configmap/vfd_r_nprpm.fben_rtrig.clk,0x4448,BOOL
I216=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgtimeout_q_rtrig.clk,0x4448,BOOL
I217=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgparwrite_q_rtrig.clk,0x4448,BOOL
I218=micro820.micro820.vfd_configmap/vfd_w_nprpm.fben_rtrig.clk,0x4448,BOOL
I219=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgtimeout_err_rtrig.clk,0x4448,BOOL
I220=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgparwrite_err_rtrig.clk,0x4448,BOOL
I221=micro820.micro820.vfd_configmap/vfd_r_npolcurrent.msgparread_err_rtrig.clk,0x4448,BOOL
I222=micro820.micro820.vfd_configmap/vfd_r_npolcurrent.msgparread_q_rtrig.clk,0x4448,BOOL
I223=micro820.micro820.vfd_configmap/vfd_r_npolcurrent.fben_rtrig.clk,0x4448,BOOL
I224=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgtimeout_q_rtrig.clk,0x4448,BOOL
I225=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgparwrite_q_rtrig.clk,0x4448,BOOL
I226=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.fben_rtrig.clk,0x4448,BOOL
I227=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgtimeout_err_rtrig.clk,0x4448,BOOL
I228=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgparwrite_err_rtrig.clk,0x4448,BOOL
I229=micro820.micro820.vfd_configmap/vfd_r_motorpoles.msgparread_err_rtrig.clk,0x4448,BOOL
I230=micro820.micro820.vfd_configmap/vfd_r_motorpoles.msgparread_q_rtrig.clk,0x4448,BOOL
I231=micro820.micro820.vfd_configmap/vfd_r_motorpoles.fben_rtrig.clk,0x4448,BOOL
I232=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgtimeout_q_rtrig.clk,0x4448,BOOL
I233=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgparwrite_q_rtrig.clk,0x4448,BOOL
I234=micro820.micro820.vfd_configmap/vfd_w_motorpoles.fben_rtrig.clk,0x4448,BOOL
I235=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgtimeout_err_rtrig.clk,0x4448,BOOL
I236=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgparwrite_err_rtrig.clk,0x4448,BOOL
I237=micro820.micro820.vfd_configmap/vfd_r_maxfreq.msgparread_err_rtrig.clk,0x4448,BOOL
I238=micro820.micro820.vfd_configmap/vfd_r_maxfreq.msgparread_q_rtrig.clk,0x4448,BOOL
I239=micro820.micro820.vfd_configmap/vfd_r_maxfreq.fben_rtrig.clk,0x4448,BOOL
I240=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgtimeout_q_rtrig.clk,0x4448,BOOL
I241=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgparwrite_q_rtrig.clk,0x4448,BOOL
I242=micro820.micro820.vfd_configmap/vfd_w_maxfreq.fben_rtrig.clk,0x4448,BOOL
I243=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgtimeout_err_rtrig.clk,0x4448,BOOL
I244=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgparwrite_err_rtrig.clk,0x4448,BOOL
I245=micro820.micro820.vfd_configmap/vfd_r_minfreq.msgparread_err_rtrig.clk,0x4448,BOOL
I246=micro820.micro820.vfd_configmap/vfd_r_minfreq.msgparread_q_rtrig.clk,0x4448,BOOL
I247=micro820.micro820.vfd_configmap/vfd_r_minfreq.fben_rtrig.clk,0x4448,BOOL
I248=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgtimeout_q_rtrig.clk,0x4448,BOOL
I249=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgparwrite_q_rtrig.clk,0x4448,BOOL
I250=micro820.micro820.vfd_configmap/vfd_w_minfreq.fben_rtrig.clk,0x4448,BOOL
I251=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgtimeout_err_rtrig.clk,0x4448,BOOL
I252=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgparwrite_err_rtrig.clk,0x4448,BOOL
I253=micro820.micro820.vfd_configmap/vfd_r_stopmode.msgparread_err_rtrig.clk,0x4448,BOOL
I254=micro820.micro820.vfd_configmap/vfd_r_stopmode.msgparread_q_rtrig.clk,0x4448,BOOL
I255=micro820.micro820.vfd_configmap/vfd_r_stopmode.fben_rtrig.clk,0x4448,BOOL
I256=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgtimeout_q_rtrig.clk,0x4448,BOOL
I257=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgparwrite_q_rtrig.clk,0x4448,BOOL
I258=micro820.micro820.vfd_configmap/vfd_w_stopmode.fben_rtrig.clk,0x4448,BOOL
I259=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgtimeout_err_rtrig.clk,0x4448,BOOL
I260=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgparwrite_err_rtrig.clk,0x4448,BOOL
I261=micro820.micro820.vfd_configmap/vfd_r_torqueperfmode.msgparread_err_rtrig.clk,0x4448,BOOL
I262=micro820.micro820.vfd_configmap/vfd_r_torqueperfmode.msgparread_q_rtrig.clk,0x4448,BOOL
I263=micro820.micro820.vfd_configmap/vfd_r_torqueperfmode.fben_rtrig.clk,0x4448,BOOL
I264=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgtimeout_q_rtrig.clk,0x4448,BOOL
I265=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgparwrite_q_rtrig.clk,0x4448,BOOL
I266=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.fben_rtrig.clk,0x4448,BOOL
I267=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgtimeout_err_rtrig.clk,0x4448,BOOL
I268=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgparwrite_err_rtrig.clk,0x4448,BOOL
I269=micro820.micro820.readdownholedata/modbusdata_0.in,0x4432,BOOL
I270=micro820.micro820.readdownholedata/modbusdata_0.cancel,0x49A,BOOL
I271=micro820.micro820.readdownholedata/modbusdata_0.localcfg,0xFFFFFFFF,MODBUSLOCPARA
I272=micro820.micro820.readdownholedata/modbusdata_0.targetcfg,0xFFFFFFFF,MODBUSTARPARA
I273=micro820.micro820.readdownholedata/modbusdata_0.localaddr,0xFFFFFFFF,MODBUSLOCADDR
I274=micro820.micro820.readdownholedata/modbusdata_0.__adi_localaddr,0xFFFFFFFF,UINT
I275=micro820.micro820.readdownholedata/modbusdata_1000.in,0x4432,BOOL
I276=micro820.micro820.readdownholedata/modbusdata_1000.cancel,0x49A,BOOL
I277=micro820.micro820.readdownholedata/modbusdata_1000.localcfg,0xFFFFFFFF,MODBUSLOCPARA
I278=micro820.micro820.readdownholedata/modbusdata_1000.targetcfg,0xFFFFFFFF,MODBUSTARPARA
I279=micro820.micro820.readdownholedata/modbusdata_1000.localaddr,0xFFFFFFFF,MODBUSLOCADDR
I280=micro820.micro820.readdownholedata/modbusdata_1000.__adi_localaddr,0xFFFFFFFF,UINT
I281=micro820.micro820.vfd_configmap/vfd_r_nphp.msgparread.in,0x4452,BOOL
I282=micro820.micro820.vfd_configmap/vfd_r_nphp.msgparread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I283=micro820.micro820.vfd_configmap/vfd_r_nphp.msgparread.appcfg,0xFFFFFFFF,CIPAPPCFG
I284=micro820.micro820.vfd_configmap/vfd_r_nphp.msgparread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I285=micro820.micro820.vfd_configmap/vfd_r_nphp.msgparread.reqlength,0x44BA,UINT
I286=micro820.micro820.vfd_configmap/vfd_r_nphp.msgparread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I287=micro820.micro820.vfd_configmap/vfd_r_nphp.msgparread.__adi_resdata,0xFFFFFFFF,UINT
I288=micro820.micro820.vfd_messaging/vfd.msg_parread.in,0x4452,BOOL
I289=micro820.micro820.vfd_messaging/vfd.msg_parread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I290=micro820.micro820.vfd_messaging/vfd.msg_parread.appcfg,0xFFFFFFFF,CIPAPPCFG
I291=micro820.micro820.vfd_messaging/vfd.msg_parread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I292=micro820.micro820.vfd_messaging/vfd.msg_parread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I293=micro820.micro820.vfd_messaging/vfd.msg_parread.reqlength,0x44E8,UINT
I294=micro820.micro820.vfd_messaging/vfd.msg_parread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I295=micro820.micro820.vfd_messaging/vfd.msg_parread.__adi_reqdata,0xFFFFFFFF,UINT
I296=micro820.micro820.vfd_messaging/vfd.msg_parread.__adi_resdata,0xFFFFFFFF,UINT
I297=micro820.micro820.vfd_messaging/vfd.msg_cmd.in,0x4452,BOOL
I298=micro820.micro820.vfd_messaging/vfd.msg_cmd.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I299=micro820.micro820.vfd_messaging/vfd.msg_cmd.appcfg,0xFFFFFFFF,CIPAPPCFG
I300=micro820.micro820.vfd_messaging/vfd.msg_cmd.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I301=micro820.micro820.vfd_messaging/vfd.msg_cmd.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I302=micro820.micro820.vfd_messaging/vfd.msg_cmd.reqlength,0x44E8,UINT
I303=micro820.micro820.vfd_messaging/vfd.msg_cmd.__adi_reqdata,0xFFFFFFFF,UINT
I304=micro820.micro820.vfd_messaging/vfd.msg_sts.in,0x4452,BOOL
I305=micro820.micro820.vfd_messaging/vfd.msg_sts.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I306=micro820.micro820.vfd_messaging/vfd.msg_sts.appcfg,0xFFFFFFFF,CIPAPPCFG
I307=micro820.micro820.vfd_messaging/vfd.msg_sts.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I308=micro820.micro820.vfd_messaging/vfd.msg_sts.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I309=micro820.micro820.vfd_messaging/vfd.msg_sts.__adi_resdata,0xFFFFFFFF,UINT
I310=micro820.micro820.vfd_messaging/vfd.msg_timeout.in,0x4452,BOOL
I311=micro820.micro820.vfd_messaging/vfd.msg_timeout.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I312=micro820.micro820.vfd_messaging/vfd.msg_timeout.appcfg,0xFFFFFFFF,CIPAPPCFG
I313=micro820.micro820.vfd_messaging/vfd.msg_timeout.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I314=micro820.micro820.vfd_messaging/vfd.msg_timeout.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I315=micro820.micro820.vfd_messaging/vfd.msg_timeout.reqlength,0x44B8,UINT
I316=micro820.micro820.vfd_messaging/vfd.msg_timeout.__adi_reqdata,0xFFFFFFFF,UINT
I317=micro820.micro820.vfd_messaging/vfd.msg_parwrite.in,0x4452,BOOL
I318=micro820.micro820.vfd_messaging/vfd.msg_parwrite.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I319=micro820.micro820.vfd_messaging/vfd.msg_parwrite.appcfg,0xFFFFFFFF,CIPAPPCFG
I320=micro820.micro820.vfd_messaging/vfd.msg_parwrite.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I321=micro820.micro820.vfd_messaging/vfd.msg_parwrite.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I322=micro820.micro820.vfd_messaging/vfd.msg_parwrite.reqlength,0x44E8,UINT
I323=micro820.micro820.vfd_messaging/vfd.msg_parwrite.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I324=micro820.micro820.vfd_messaging/vfd.msg_parwrite.__adi_reqdata,0xFFFFFFFF,UINT
I325=micro820.micro820.vfd_messaging/vfd.msg_parwrite.__adi_resdata,0xFFFFFFFF,UINT
I326=micro820.micro820.vfd_messaging/vfd.msg_drvtype.in,0x4452,BOOL
I327=micro820.micro820.vfd_messaging/vfd.msg_drvtype.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I328=micro820.micro820.vfd_messaging/vfd.msg_drvtype.appcfg,0xFFFFFFFF,CIPAPPCFG
I329=micro820.micro820.vfd_messaging/vfd.msg_drvtype.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I330=micro820.micro820.vfd_messaging/vfd.msg_drvtype.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I331=micro820.micro820.vfd_messaging/vfd.msg_drvtype.__adi_resdata,0xFFFFFFFF,UINT
I332=micro820.micro820.vfd_configmap/vfd_w_nphp.msgparwrite.in,0x4452,BOOL
I333=micro820.micro820.vfd_configmap/vfd_w_nphp.msgparwrite.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I334=micro820.micro820.vfd_configmap/vfd_w_nphp.msgparwrite.appcfg,0xFFFFFFFF,CIPAPPCFG
I335=micro820.micro820.vfd_configmap/vfd_w_nphp.msgparwrite.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I336=micro820.micro820.vfd_configmap/vfd_w_nphp.msgparwrite.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I337=micro820.micro820.vfd_configmap/vfd_w_nphp.msgparwrite.reqlength,0x44B8,UINT
I338=micro820.micro820.vfd_configmap/vfd_w_nphp.msgparwrite.__adi_reqdata,0xFFFFFFFF,UINT
I339=micro820.micro820.vfd_configmap/vfd_w_nphp.msgtimeout.in,0x4452,BOOL
I340=micro820.micro820.vfd_configmap/vfd_w_nphp.msgtimeout.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I341=micro820.micro820.vfd_configmap/vfd_w_nphp.msgtimeout.appcfg,0xFFFFFFFF,CIPAPPCFG
I342=micro820.micro820.vfd_configmap/vfd_w_nphp.msgtimeout.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I343=micro820.micro820.vfd_configmap/vfd_w_nphp.msgtimeout.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I344=micro820.micro820.vfd_configmap/vfd_w_nphp.msgtimeout.reqlength,0x44B8,UINT
I345=micro820.micro820.vfd_configmap/vfd_w_nphp.msgtimeout.__adi_reqdata,0xFFFFFFFF,UINT
I346=micro820.micro820.vfd_configmap/vfd_r_npfla.msgparread.in,0x4452,BOOL
I347=micro820.micro820.vfd_configmap/vfd_r_npfla.msgparread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I348=micro820.micro820.vfd_configmap/vfd_r_npfla.msgparread.appcfg,0xFFFFFFFF,CIPAPPCFG
I349=micro820.micro820.vfd_configmap/vfd_r_npfla.msgparread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I350=micro820.micro820.vfd_configmap/vfd_r_npfla.msgparread.reqlength,0x44BA,UINT
I351=micro820.micro820.vfd_configmap/vfd_r_npfla.msgparread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I352=micro820.micro820.vfd_configmap/vfd_r_npfla.msgparread.__adi_resdata,0xFFFFFFFF,UINT
I353=micro820.micro820.vfd_configmap/vfd_w_npfla.msgparwrite.in,0x4452,BOOL
I354=micro820.micro820.vfd_configmap/vfd_w_npfla.msgparwrite.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I355=micro820.micro820.vfd_configmap/vfd_w_npfla.msgparwrite.appcfg,0xFFFFFFFF,CIPAPPCFG
I356=micro820.micro820.vfd_configmap/vfd_w_npfla.msgparwrite.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I357=micro820.micro820.vfd_configmap/vfd_w_npfla.msgparwrite.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I358=micro820.micro820.vfd_configmap/vfd_w_npfla.msgparwrite.reqlength,0x44B8,UINT
I359=micro820.micro820.vfd_configmap/vfd_w_npfla.msgparwrite.__adi_reqdata,0xFFFFFFFF,UINT
I360=micro820.micro820.vfd_configmap/vfd_w_npfla.msgtimeout.in,0x4452,BOOL
I361=micro820.micro820.vfd_configmap/vfd_w_npfla.msgtimeout.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I362=micro820.micro820.vfd_configmap/vfd_w_npfla.msgtimeout.appcfg,0xFFFFFFFF,CIPAPPCFG
I363=micro820.micro820.vfd_configmap/vfd_w_npfla.msgtimeout.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I364=micro820.micro820.vfd_configmap/vfd_w_npfla.msgtimeout.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I365=micro820.micro820.vfd_configmap/vfd_w_npfla.msgtimeout.reqlength,0x44B8,UINT
I366=micro820.micro820.vfd_configmap/vfd_w_npfla.msgtimeout.__adi_reqdata,0xFFFFFFFF,UINT
I367=micro820.micro820.vfd_configmap/vfd_r_npvolts.msgparread.in,0x4452,BOOL
I368=micro820.micro820.vfd_configmap/vfd_r_npvolts.msgparread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I369=micro820.micro820.vfd_configmap/vfd_r_npvolts.msgparread.appcfg,0xFFFFFFFF,CIPAPPCFG
I370=micro820.micro820.vfd_configmap/vfd_r_npvolts.msgparread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I371=micro820.micro820.vfd_configmap/vfd_r_npvolts.msgparread.reqlength,0x44BA,UINT
I372=micro820.micro820.vfd_configmap/vfd_r_npvolts.msgparread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I373=micro820.micro820.vfd_configmap/vfd_r_npvolts.msgparread.__adi_resdata,0xFFFFFFFF,UINT
I374=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgparwrite.in,0x4452,BOOL
I375=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgparwrite.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I376=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgparwrite.appcfg,0xFFFFFFFF,CIPAPPCFG
I377=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgparwrite.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I378=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgparwrite.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I379=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgparwrite.reqlength,0x44B8,UINT
I380=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgparwrite.__adi_reqdata,0xFFFFFFFF,UINT
I381=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgtimeout.in,0x4452,BOOL
I382=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgtimeout.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I383=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgtimeout.appcfg,0xFFFFFFFF,CIPAPPCFG
I384=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgtimeout.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I385=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgtimeout.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I386=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgtimeout.reqlength,0x44B8,UINT
I387=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgtimeout.__adi_reqdata,0xFFFFFFFF,UINT
I388=micro820.micro820.vfd_configmap/vfd_r_nphz.msgparread.in,0x4452,BOOL
I389=micro820.micro820.vfd_configmap/vfd_r_nphz.msgparread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I390=micro820.micro820.vfd_configmap/vfd_r_nphz.msgparread.appcfg,0xFFFFFFFF,CIPAPPCFG
I391=micro820.micro820.vfd_configmap/vfd_r_nphz.msgparread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I392=micro820.micro820.vfd_configmap/vfd_r_nphz.msgparread.reqlength,0x44BA,UINT
I393=micro820.micro820.vfd_configmap/vfd_r_nphz.msgparread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I394=micro820.micro820.vfd_configmap/vfd_r_nphz.msgparread.__adi_resdata,0xFFFFFFFF,UINT
I395=micro820.micro820.vfd_configmap/vfd_w_nphz.msgparwrite.in,0x4452,BOOL
I396=micro820.micro820.vfd_configmap/vfd_w_nphz.msgparwrite.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I397=micro820.micro820.vfd_configmap/vfd_w_nphz.msgparwrite.appcfg,0xFFFFFFFF,CIPAPPCFG
I398=micro820.micro820.vfd_configmap/vfd_w_nphz.msgparwrite.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I399=micro820.micro820.vfd_configmap/vfd_w_nphz.msgparwrite.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I400=micro820.micro820.vfd_configmap/vfd_w_nphz.msgparwrite.reqlength,0x44B8,UINT
I401=micro820.micro820.vfd_configmap/vfd_w_nphz.msgparwrite.__adi_reqdata,0xFFFFFFFF,UINT
I402=micro820.micro820.vfd_configmap/vfd_w_nphz.msgtimeout.in,0x4452,BOOL
I403=micro820.micro820.vfd_configmap/vfd_w_nphz.msgtimeout.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I404=micro820.micro820.vfd_configmap/vfd_w_nphz.msgtimeout.appcfg,0xFFFFFFFF,CIPAPPCFG
I405=micro820.micro820.vfd_configmap/vfd_w_nphz.msgtimeout.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I406=micro820.micro820.vfd_configmap/vfd_w_nphz.msgtimeout.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I407=micro820.micro820.vfd_configmap/vfd_w_nphz.msgtimeout.reqlength,0x44B8,UINT
I408=micro820.micro820.vfd_configmap/vfd_w_nphz.msgtimeout.__adi_reqdata,0xFFFFFFFF,UINT
I409=micro820.micro820.vfd_configmap/vfd_r_nprpm.msgparread.in,0x4452,BOOL
I410=micro820.micro820.vfd_configmap/vfd_r_nprpm.msgparread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I411=micro820.micro820.vfd_configmap/vfd_r_nprpm.msgparread.appcfg,0xFFFFFFFF,CIPAPPCFG
I412=micro820.micro820.vfd_configmap/vfd_r_nprpm.msgparread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I413=micro820.micro820.vfd_configmap/vfd_r_nprpm.msgparread.reqlength,0x44BA,UINT
I414=micro820.micro820.vfd_configmap/vfd_r_nprpm.msgparread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I415=micro820.micro820.vfd_configmap/vfd_r_nprpm.msgparread.__adi_resdata,0xFFFFFFFF,UINT
I416=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgparwrite.in,0x4452,BOOL
I417=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgparwrite.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I418=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgparwrite.appcfg,0xFFFFFFFF,CIPAPPCFG
I419=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgparwrite.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I420=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgparwrite.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I421=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgparwrite.reqlength,0x44B8,UINT
I422=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgparwrite.__adi_reqdata,0xFFFFFFFF,UINT
I423=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgtimeout.in,0x4452,BOOL
I424=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgtimeout.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I425=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgtimeout.appcfg,0xFFFFFFFF,CIPAPPCFG
I426=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgtimeout.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I427=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgtimeout.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I428=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgtimeout.reqlength,0x44B8,UINT
I429=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgtimeout.__adi_reqdata,0xFFFFFFFF,UINT
I430=micro820.micro820.vfd_configmap/vfd_r_npolcurrent.msgparread.in,0x4452,BOOL
I431=micro820.micro820.vfd_configmap/vfd_r_npolcurrent.msgparread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I432=micro820.micro820.vfd_configmap/vfd_r_npolcurrent.msgparread.appcfg,0xFFFFFFFF,CIPAPPCFG
I433=micro820.micro820.vfd_configmap/vfd_r_npolcurrent.msgparread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I434=micro820.micro820.vfd_configmap/vfd_r_npolcurrent.msgparread.reqlength,0x44BA,UINT
I435=micro820.micro820.vfd_configmap/vfd_r_npolcurrent.msgparread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I436=micro820.micro820.vfd_configmap/vfd_r_npolcurrent.msgparread.__adi_resdata,0xFFFFFFFF,UINT
I437=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgparwrite.in,0x4452,BOOL
I438=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgparwrite.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I439=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgparwrite.appcfg,0xFFFFFFFF,CIPAPPCFG
I440=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgparwrite.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I441=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgparwrite.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I442=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgparwrite.reqlength,0x44B8,UINT
I443=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgparwrite.__adi_reqdata,0xFFFFFFFF,UINT
I444=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgtimeout.in,0x4452,BOOL
I445=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgtimeout.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I446=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgtimeout.appcfg,0xFFFFFFFF,CIPAPPCFG
I447=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgtimeout.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I448=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgtimeout.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I449=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgtimeout.reqlength,0x44B8,UINT
I450=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgtimeout.__adi_reqdata,0xFFFFFFFF,UINT
I451=micro820.micro820.vfd_configmap/vfd_r_motorpoles.msgparread.in,0x4452,BOOL
I452=micro820.micro820.vfd_configmap/vfd_r_motorpoles.msgparread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I453=micro820.micro820.vfd_configmap/vfd_r_motorpoles.msgparread.appcfg,0xFFFFFFFF,CIPAPPCFG
I454=micro820.micro820.vfd_configmap/vfd_r_motorpoles.msgparread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I455=micro820.micro820.vfd_configmap/vfd_r_motorpoles.msgparread.reqlength,0x44BA,UINT
I456=micro820.micro820.vfd_configmap/vfd_r_motorpoles.msgparread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I457=micro820.micro820.vfd_configmap/vfd_r_motorpoles.msgparread.__adi_resdata,0xFFFFFFFF,UINT
I458=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgparwrite.in,0x4452,BOOL
I459=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgparwrite.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I460=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgparwrite.appcfg,0xFFFFFFFF,CIPAPPCFG
I461=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgparwrite.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I462=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgparwrite.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I463=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgparwrite.reqlength,0x44B8,UINT
I464=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgparwrite.__adi_reqdata,0xFFFFFFFF,UINT
I465=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgtimeout.in,0x4452,BOOL
I466=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgtimeout.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I467=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgtimeout.appcfg,0xFFFFFFFF,CIPAPPCFG
I468=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgtimeout.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I469=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgtimeout.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I470=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgtimeout.reqlength,0x44B8,UINT
I471=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgtimeout.__adi_reqdata,0xFFFFFFFF,UINT
I472=micro820.micro820.vfd_configmap/vfd_r_maxfreq.msgparread.in,0x4452,BOOL
I473=micro820.micro820.vfd_configmap/vfd_r_maxfreq.msgparread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I474=micro820.micro820.vfd_configmap/vfd_r_maxfreq.msgparread.appcfg,0xFFFFFFFF,CIPAPPCFG
I475=micro820.micro820.vfd_configmap/vfd_r_maxfreq.msgparread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I476=micro820.micro820.vfd_configmap/vfd_r_maxfreq.msgparread.reqlength,0x44BA,UINT
I477=micro820.micro820.vfd_configmap/vfd_r_maxfreq.msgparread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I478=micro820.micro820.vfd_configmap/vfd_r_maxfreq.msgparread.__adi_resdata,0xFFFFFFFF,UINT
I479=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgparwrite.in,0x4452,BOOL
I480=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgparwrite.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I481=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgparwrite.appcfg,0xFFFFFFFF,CIPAPPCFG
I482=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgparwrite.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I483=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgparwrite.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I484=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgparwrite.reqlength,0x44B8,UINT
I485=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgparwrite.__adi_reqdata,0xFFFFFFFF,UINT
I486=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgtimeout.in,0x4452,BOOL
I487=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgtimeout.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I488=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgtimeout.appcfg,0xFFFFFFFF,CIPAPPCFG
I489=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgtimeout.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I490=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgtimeout.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I491=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgtimeout.reqlength,0x44B8,UINT
I492=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgtimeout.__adi_reqdata,0xFFFFFFFF,UINT
I493=micro820.micro820.vfd_configmap/vfd_r_minfreq.msgparread.in,0x4452,BOOL
I494=micro820.micro820.vfd_configmap/vfd_r_minfreq.msgparread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I495=micro820.micro820.vfd_configmap/vfd_r_minfreq.msgparread.appcfg,0xFFFFFFFF,CIPAPPCFG
I496=micro820.micro820.vfd_configmap/vfd_r_minfreq.msgparread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I497=micro820.micro820.vfd_configmap/vfd_r_minfreq.msgparread.reqlength,0x44BA,UINT
I498=micro820.micro820.vfd_configmap/vfd_r_minfreq.msgparread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I499=micro820.micro820.vfd_configmap/vfd_r_minfreq.msgparread.__adi_resdata,0xFFFFFFFF,UINT
I500=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgparwrite.in,0x4452,BOOL
I501=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgparwrite.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I502=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgparwrite.appcfg,0xFFFFFFFF,CIPAPPCFG
I503=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgparwrite.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I504=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgparwrite.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I505=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgparwrite.reqlength,0x44B8,UINT
I506=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgparwrite.__adi_reqdata,0xFFFFFFFF,UINT
I507=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgtimeout.in,0x4452,BOOL
I508=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgtimeout.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I509=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgtimeout.appcfg,0xFFFFFFFF,CIPAPPCFG
I510=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgtimeout.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I511=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgtimeout.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I512=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgtimeout.reqlength,0x44B8,UINT
I513=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgtimeout.__adi_reqdata,0xFFFFFFFF,UINT
I514=micro820.micro820.vfd_configmap/vfd_r_stopmode.msgparread.in,0x4452,BOOL
I515=micro820.micro820.vfd_configmap/vfd_r_stopmode.msgparread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I516=micro820.micro820.vfd_configmap/vfd_r_stopmode.msgparread.appcfg,0xFFFFFFFF,CIPAPPCFG
I517=micro820.micro820.vfd_configmap/vfd_r_stopmode.msgparread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I518=micro820.micro820.vfd_configmap/vfd_r_stopmode.msgparread.reqlength,0x44BA,UINT
I519=micro820.micro820.vfd_configmap/vfd_r_stopmode.msgparread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I520=micro820.micro820.vfd_configmap/vfd_r_stopmode.msgparread.__adi_resdata,0xFFFFFFFF,UINT
I521=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgparwrite.in,0x4452,BOOL
I522=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgparwrite.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I523=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgparwrite.appcfg,0xFFFFFFFF,CIPAPPCFG
I524=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgparwrite.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I525=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgparwrite.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I526=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgparwrite.reqlength,0x44B8,UINT
I527=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgparwrite.__adi_reqdata,0xFFFFFFFF,UINT
I528=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgtimeout.in,0x4452,BOOL
I529=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgtimeout.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I530=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgtimeout.appcfg,0xFFFFFFFF,CIPAPPCFG
I531=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgtimeout.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I532=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgtimeout.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I533=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgtimeout.reqlength,0x44B8,UINT
I534=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgtimeout.__adi_reqdata,0xFFFFFFFF,UINT
I535=micro820.micro820.vfd_configmap/vfd_r_torqueperfmode.msgparread.in,0x4452,BOOL
I536=micro820.micro820.vfd_configmap/vfd_r_torqueperfmode.msgparread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I537=micro820.micro820.vfd_configmap/vfd_r_torqueperfmode.msgparread.appcfg,0xFFFFFFFF,CIPAPPCFG
I538=micro820.micro820.vfd_configmap/vfd_r_torqueperfmode.msgparread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I539=micro820.micro820.vfd_configmap/vfd_r_torqueperfmode.msgparread.reqlength,0x44BA,UINT
I540=micro820.micro820.vfd_configmap/vfd_r_torqueperfmode.msgparread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I541=micro820.micro820.vfd_configmap/vfd_r_torqueperfmode.msgparread.__adi_resdata,0xFFFFFFFF,UINT
I542=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgparwrite.in,0x4452,BOOL
I543=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgparwrite.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I544=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgparwrite.appcfg,0xFFFFFFFF,CIPAPPCFG
I545=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgparwrite.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I546=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgparwrite.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I547=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgparwrite.reqlength,0x44B8,UINT
I548=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgparwrite.__adi_reqdata,0xFFFFFFFF,UINT
I549=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgtimeout.in,0x4452,BOOL
I550=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgtimeout.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I551=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgtimeout.appcfg,0xFFFFFFFF,CIPAPPCFG
I552=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgtimeout.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I553=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgtimeout.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I554=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgtimeout.reqlength,0x44B8,UINT
I555=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgtimeout.__adi_reqdata,0xFFFFFFFF,UINT
I556=micro820.micro820.vfd_configmap/vfd_w_nphp.fben,0x491,BOOL
I557=micro820.micro820.vfd_configmap/vfd_w_nphp.ipaddress,0x792,STRING
I558=micro820.micro820.vfd_configmap/vfd_w_nphp.enetctrlto_sec,0x4479,USINT
I559=micro820.micro820.vfd_configmap/vfd_w_nphp.parameternumber,0x44D2,UINT
I560=micro820.micro820.vfd_configmap/vfd_w_nphp.parametervalue,0x4C4,UINT
I561=micro820.micro820.vfd_configmap/vfd_w_npfla.fben,0x491,BOOL
I562=micro820.micro820.vfd_configmap/vfd_w_npfla.ipaddress,0x792,STRING
I563=micro820.micro820.vfd_configmap/vfd_w_npfla.enetctrlto_sec,0x4479,USINT
I564=micro820.micro820.vfd_configmap/vfd_w_npfla.parameternumber,0x44D0,UINT
I565=micro820.micro820.vfd_configmap/vfd_w_npfla.parametervalue,0x4C6,UINT
I566=micro820.micro820.vfd_configmap/vfd_w_npvolts.fben,0x491,BOOL
I567=micro820.micro820.vfd_configmap/vfd_w_npvolts.ipaddress,0x792,STRING
I568=micro820.micro820.vfd_configmap/vfd_w_npvolts.enetctrlto_sec,0x4479,USINT
I569=micro820.micro820.vfd_configmap/vfd_w_npvolts.parameternumber,0x44CE,UINT
I570=micro820.micro820.vfd_configmap/vfd_w_npvolts.parametervalue,0x4C8,UINT
I571=micro820.micro820.vfd_configmap/vfd_w_nphz.fben,0x491,BOOL
I572=micro820.micro820.vfd_configmap/vfd_w_nphz.ipaddress,0x792,STRING
I573=micro820.micro820.vfd_configmap/vfd_w_nphz.enetctrlto_sec,0x4479,USINT
I574=micro820.micro820.vfd_configmap/vfd_w_nphz.parameternumber,0x44CC,UINT
I575=micro820.micro820.vfd_configmap/vfd_w_nphz.parametervalue,0x4CA,UINT
I576=micro820.micro820.vfd_configmap/vfd_w_nprpm.fben,0x491,BOOL
I577=micro820.micro820.vfd_configmap/vfd_w_nprpm.ipaddress,0x792,STRING
I578=micro820.micro820.vfd_configmap/vfd_w_nprpm.enetctrlto_sec,0x4479,USINT
I579=micro820.micro820.vfd_configmap/vfd_w_nprpm.parameternumber,0x44CA,UINT
I580=micro820.micro820.vfd_configmap/vfd_w_nprpm.parametervalue,0x4CE,UINT
I581=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.fben,0x491,BOOL
I582=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.ipaddress,0x792,STRING
I583=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.enetctrlto_sec,0x4479,USINT
I584=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.parameternumber,0x44C8,UINT
I585=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.parametervalue,0x4CC,UINT
I586=micro820.micro820.vfd_configmap/vfd_w_motorpoles.fben,0x458,BOOL
I587=micro820.micro820.vfd_configmap/vfd_w_motorpoles.ipaddress,0x792,STRING
I588=micro820.micro820.vfd_configmap/vfd_w_motorpoles.enetctrlto_sec,0x4479,USINT
I589=micro820.micro820.vfd_configmap/vfd_w_motorpoles.parameternumber,0x44C6,UINT
I590=micro820.micro820.vfd_configmap/vfd_w_motorpoles.parametervalue,0x4BA,UINT
I591=micro820.micro820.vfd_configmap/vfd_w_maxfreq.fben,0x491,BOOL
I592=micro820.micro820.vfd_configmap/vfd_w_maxfreq.ipaddress,0x792,STRING
I593=micro820.micro820.vfd_configmap/vfd_w_maxfreq.enetctrlto_sec,0x4479,USINT
I594=micro820.micro820.vfd_configmap/vfd_w_maxfreq.parameternumber,0x44C4,UINT
I595=micro820.micro820.vfd_configmap/vfd_w_maxfreq.parametervalue,0x4D4,UINT
I596=micro820.micro820.vfd_configmap/vfd_w_minfreq.fben,0x491,BOOL
I597=micro820.micro820.vfd_configmap/vfd_w_minfreq.ipaddress,0x792,STRING
I598=micro820.micro820.vfd_configmap/vfd_w_minfreq.enetctrlto_sec,0x4479,USINT
I599=micro820.micro820.vfd_configmap/vfd_w_minfreq.parameternumber,0x44C2,UINT
I600=micro820.micro820.vfd_configmap/vfd_w_minfreq.parametervalue,0x4D6,UINT
I601=micro820.micro820.vfd_configmap/vfd_w_stopmode.fben,0x491,BOOL
I602=micro820.micro820.vfd_configmap/vfd_w_stopmode.ipaddress,0x792,STRING
I603=micro820.micro820.vfd_configmap/vfd_w_stopmode.enetctrlto_sec,0x4479,USINT
I604=micro820.micro820.vfd_configmap/vfd_w_stopmode.parameternumber,0x44C0,UINT
I605=micro820.micro820.vfd_configmap/vfd_w_stopmode.parametervalue,0x44BC,UINT
I606=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.fben,0x491,BOOL
I607=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.ipaddress,0x792,STRING
I608=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.enetctrlto_sec,0x4479,USINT
I609=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.parameternumber,0x44BE,UINT
I610=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.parametervalue,0x44BA,UINT
I611=micro820.micro820.downtime_timer.in,0x59F8,BOOL
I612=micro820.micro820.downtime_timer.pt,0x5A04,TIME
I613=micro820.micro820.vfd_messaging/vfd.msg_drvtype.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I614=micro820.micro820.vfd_messaging/vfd.msg_drvtype.reqlength,0x59FC,UINT
I615=micro820.micro820.vfd_messaging/vfd.msg_drvtype.__adi_reqdata,0xFFFFFFFF,UINT
I616=micro820.micro820.vfd_messaging/vfd.msg_timeout.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I617=micro820.micro820.vfd_messaging/vfd.msg_timeout.__adi_resdata,0xFFFFFFFF,UINT
I618=micro820.micro820.vfd_messaging/vfd.msg_cmd.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I619=micro820.micro820.vfd_messaging/vfd.msg_cmd.__adi_resdata,0xFFFFFFFF,UINT
I620=micro820.micro820.vfd_messaging/vfd.msg_sts.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I621=micro820.micro820.vfd_messaging/vfd.msg_sts.reqlength,0x59FC,UINT
I622=micro820.micro820.vfd_messaging/vfd.msg_sts.__adi_reqdata,0xFFFFFFFF,UINT
I623=micro820.micro820.vfd_configmap/vfd_r_nphp.msgparread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I624=micro820.micro820.vfd_configmap/vfd_r_nphp.msgparread.__adi_reqdata,0xFFFFFFFF,UINT
I625=micro820.micro820.vfd_configmap/vfd_w_nphp.msgparwrite.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I626=micro820.micro820.vfd_configmap/vfd_w_nphp.msgparwrite.__adi_resdata,0xFFFFFFFF,UINT
I627=micro820.micro820.vfd_configmap/vfd_w_nphp.msgtimeout.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I628=micro820.micro820.vfd_configmap/vfd_w_nphp.msgtimeout.__adi_resdata,0xFFFFFFFF,UINT
I629=micro820.micro820.vfd_configmap/vfd_r_npfla.msgparread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I630=micro820.micro820.vfd_configmap/vfd_r_npfla.msgparread.__adi_reqdata,0xFFFFFFFF,UINT
I631=micro820.micro820.vfd_configmap/vfd_w_npfla.msgparwrite.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I632=micro820.micro820.vfd_configmap/vfd_w_npfla.msgparwrite.__adi_resdata,0xFFFFFFFF,UINT
I633=micro820.micro820.vfd_configmap/vfd_w_npfla.msgtimeout.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I634=micro820.micro820.vfd_configmap/vfd_w_npfla.msgtimeout.__adi_resdata,0xFFFFFFFF,UINT
I635=micro820.micro820.vfd_configmap/vfd_r_npvolts.msgparread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I636=micro820.micro820.vfd_configmap/vfd_r_npvolts.msgparread.__adi_reqdata,0xFFFFFFFF,UINT
I637=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgparwrite.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I638=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgparwrite.__adi_resdata,0xFFFFFFFF,UINT
I639=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgtimeout.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I640=micro820.micro820.vfd_configmap/vfd_w_npvolts.msgtimeout.__adi_resdata,0xFFFFFFFF,UINT
I641=micro820.micro820.vfd_configmap/vfd_r_nphz.msgparread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I642=micro820.micro820.vfd_configmap/vfd_r_nphz.msgparread.__adi_reqdata,0xFFFFFFFF,UINT
I643=micro820.micro820.vfd_configmap/vfd_w_nphz.msgparwrite.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I644=micro820.micro820.vfd_configmap/vfd_w_nphz.msgparwrite.__adi_resdata,0xFFFFFFFF,UINT
I645=micro820.micro820.vfd_configmap/vfd_w_nphz.msgtimeout.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I646=micro820.micro820.vfd_configmap/vfd_w_nphz.msgtimeout.__adi_resdata,0xFFFFFFFF,UINT
I647=micro820.micro820.vfd_configmap/vfd_r_nprpm.msgparread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I648=micro820.micro820.vfd_configmap/vfd_r_nprpm.msgparread.__adi_reqdata,0xFFFFFFFF,UINT
I649=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgparwrite.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I650=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgparwrite.__adi_resdata,0xFFFFFFFF,UINT
I651=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgtimeout.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I652=micro820.micro820.vfd_configmap/vfd_w_nprpm.msgtimeout.__adi_resdata,0xFFFFFFFF,UINT
I653=micro820.micro820.vfd_configmap/vfd_r_npolcurrent.msgparread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I654=micro820.micro820.vfd_configmap/vfd_r_npolcurrent.msgparread.__adi_reqdata,0xFFFFFFFF,UINT
I655=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgparwrite.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I656=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgparwrite.__adi_resdata,0xFFFFFFFF,UINT
I657=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgtimeout.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I658=micro820.micro820.vfd_configmap/vfd_w_npolcurrent.msgtimeout.__adi_resdata,0xFFFFFFFF,UINT
I659=micro820.micro820.vfd_configmap/vfd_r_motorpoles.msgparread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I660=micro820.micro820.vfd_configmap/vfd_r_motorpoles.msgparread.__adi_reqdata,0xFFFFFFFF,UINT
I661=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgparwrite.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I662=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgparwrite.__adi_resdata,0xFFFFFFFF,UINT
I663=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgtimeout.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I664=micro820.micro820.vfd_configmap/vfd_w_motorpoles.msgtimeout.__adi_resdata,0xFFFFFFFF,UINT
I665=micro820.micro820.vfd_configmap/vfd_r_acceltime.fben,0x59F8,BOOL
I666=micro820.micro820.vfd_configmap/vfd_r_acceltime.ipaddress,0x5A08,STRING
I667=micro820.micro820.vfd_configmap/vfd_r_acceltime.updaterate_ms,0x59FC,UINT
I668=micro820.micro820.vfd_configmap/vfd_r_acceltime.parameternumber,0x59FC,UINT
I669=micro820.micro820.vfd_configmap/vfd_r_acceltime.msgparread.in,0x59F8,BOOL
I670=micro820.micro820.vfd_configmap/vfd_r_acceltime.msgparread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I671=micro820.micro820.vfd_configmap/vfd_r_acceltime.msgparread.appcfg,0xFFFFFFFF,CIPAPPCFG
I672=micro820.micro820.vfd_configmap/vfd_r_acceltime.msgparread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I673=micro820.micro820.vfd_configmap/vfd_r_acceltime.msgparread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I674=micro820.micro820.vfd_configmap/vfd_r_acceltime.msgparread.reqlength,0x59FC,UINT
I675=micro820.micro820.vfd_configmap/vfd_r_acceltime.msgparread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I676=micro820.micro820.vfd_configmap/vfd_r_acceltime.msgparread.__adi_reqdata,0xFFFFFFFF,UINT
I677=micro820.micro820.vfd_configmap/vfd_r_acceltime.msgparread.__adi_resdata,0xFFFFFFFF,UINT
I678=micro820.micro820.vfd_configmap/vfd_r_acceltime.fben_rtrig.clk,0x59F8,BOOL
I679=micro820.micro820.vfd_configmap/vfd_r_acceltime.msgparread_q_rtrig.clk,0x59F8,BOOL
I680=micro820.micro820.vfd_configmap/vfd_r_acceltime.msgparread_err_rtrig.clk,0x59F8,BOOL
I681=micro820.micro820.vfd_configmap/vfd_w_acceltime.fben,0x59F8,BOOL
I682=micro820.micro820.vfd_configmap/vfd_w_acceltime.ipaddress,0x5A08,STRING
I683=micro820.micro820.vfd_configmap/vfd_w_acceltime.enetctrlto_sec,0x59FA,USINT
I684=micro820.micro820.vfd_configmap/vfd_w_acceltime.parameternumber,0x59FC,UINT
I685=micro820.micro820.vfd_configmap/vfd_w_acceltime.parametervalue,0x59FC,UINT
I686=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgparwrite.in,0x59F8,BOOL
I687=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgparwrite.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I688=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgparwrite.appcfg,0xFFFFFFFF,CIPAPPCFG
I689=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgparwrite.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I690=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgparwrite.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I691=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgparwrite.reqlength,0x59FC,UINT
I692=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgparwrite.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I693=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgparwrite.__adi_reqdata,0xFFFFFFFF,UINT
I694=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgparwrite.__adi_resdata,0xFFFFFFFF,UINT
I695=micro820.micro820.vfd_configmap/vfd_w_acceltime.fben_rtrig.clk,0x59F8,BOOL
I696=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgparwrite_q_rtrig.clk,0x59F8,BOOL
I697=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgparwrite_err_rtrig.clk,0x59F8,BOOL
I698=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgtimeout.in,0x59F8,BOOL
I699=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgtimeout.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I700=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgtimeout.appcfg,0xFFFFFFFF,CIPAPPCFG
I701=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgtimeout.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I702=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgtimeout.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I703=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgtimeout.reqlength,0x59FC,UINT
I704=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgtimeout.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I705=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgtimeout.__adi_reqdata,0xFFFFFFFF,UINT
I706=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgtimeout.__adi_resdata,0xFFFFFFFF,UINT
I707=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgtimeout_err_rtrig.clk,0x59F8,BOOL
I708=micro820.micro820.vfd_configmap/vfd_w_acceltime.msgtimeout_q_rtrig.clk,0x59F8,BOOL
I709=micro820.micro820.vfd_configmap/vfd_r_deceltime.fben,0x59F8,BOOL
I710=micro820.micro820.vfd_configmap/vfd_r_deceltime.ipaddress,0x5A08,STRING
I711=micro820.micro820.vfd_configmap/vfd_r_deceltime.updaterate_ms,0x59FC,UINT
I712=micro820.micro820.vfd_configmap/vfd_r_deceltime.parameternumber,0x59FC,UINT
I713=micro820.micro820.vfd_configmap/vfd_r_deceltime.msgparread.in,0x59F8,BOOL
I714=micro820.micro820.vfd_configmap/vfd_r_deceltime.msgparread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I715=micro820.micro820.vfd_configmap/vfd_r_deceltime.msgparread.appcfg,0xFFFFFFFF,CIPAPPCFG
I716=micro820.micro820.vfd_configmap/vfd_r_deceltime.msgparread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I717=micro820.micro820.vfd_configmap/vfd_r_deceltime.msgparread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I718=micro820.micro820.vfd_configmap/vfd_r_deceltime.msgparread.reqlength,0x59FC,UINT
I719=micro820.micro820.vfd_configmap/vfd_r_deceltime.msgparread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I720=micro820.micro820.vfd_configmap/vfd_r_deceltime.msgparread.__adi_reqdata,0xFFFFFFFF,UINT
I721=micro820.micro820.vfd_configmap/vfd_r_deceltime.msgparread.__adi_resdata,0xFFFFFFFF,UINT
I722=micro820.micro820.vfd_configmap/vfd_r_deceltime.fben_rtrig.clk,0x59F8,BOOL
I723=micro820.micro820.vfd_configmap/vfd_r_deceltime.msgparread_q_rtrig.clk,0x59F8,BOOL
I724=micro820.micro820.vfd_configmap/vfd_r_deceltime.msgparread_err_rtrig.clk,0x59F8,BOOL
I725=micro820.micro820.vfd_configmap/vfd_w_deceltime.fben,0x59F8,BOOL
I726=micro820.micro820.vfd_configmap/vfd_w_deceltime.ipaddress,0x5A08,STRING
I727=micro820.micro820.vfd_configmap/vfd_w_deceltime.enetctrlto_sec,0x59FA,USINT
I728=micro820.micro820.vfd_configmap/vfd_w_deceltime.parameternumber,0x59FC,UINT
I729=micro820.micro820.vfd_configmap/vfd_w_deceltime.parametervalue,0x59FC,UINT
I730=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgparwrite.in,0x59F8,BOOL
I731=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgparwrite.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I732=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgparwrite.appcfg,0xFFFFFFFF,CIPAPPCFG
I733=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgparwrite.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I734=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgparwrite.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I735=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgparwrite.reqlength,0x59FC,UINT
I736=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgparwrite.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I737=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgparwrite.__adi_reqdata,0xFFFFFFFF,UINT
I738=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgparwrite.__adi_resdata,0xFFFFFFFF,UINT
I739=micro820.micro820.vfd_configmap/vfd_w_deceltime.fben_rtrig.clk,0x59F8,BOOL
I740=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgparwrite_q_rtrig.clk,0x59F8,BOOL
I741=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgparwrite_err_rtrig.clk,0x59F8,BOOL
I742=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgtimeout.in,0x59F8,BOOL
I743=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgtimeout.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I744=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgtimeout.appcfg,0xFFFFFFFF,CIPAPPCFG
I745=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgtimeout.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I746=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgtimeout.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I747=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgtimeout.reqlength,0x59FC,UINT
I748=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgtimeout.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I749=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgtimeout.__adi_reqdata,0xFFFFFFFF,UINT
I750=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgtimeout.__adi_resdata,0xFFFFFFFF,UINT
I751=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgtimeout_err_rtrig.clk,0x59F8,BOOL
I752=micro820.micro820.vfd_configmap/vfd_w_deceltime.msgtimeout_q_rtrig.clk,0x59F8,BOOL
I753=micro820.micro820.vfd_configmap/vfd_r_maxfreq.msgparread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I754=micro820.micro820.vfd_configmap/vfd_r_maxfreq.msgparread.__adi_reqdata,0xFFFFFFFF,UINT
I755=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgparwrite.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I756=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgparwrite.__adi_resdata,0xFFFFFFFF,UINT
I757=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgtimeout.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I758=micro820.micro820.vfd_configmap/vfd_w_maxfreq.msgtimeout.__adi_resdata,0xFFFFFFFF,UINT
I759=micro820.micro820.vfd_configmap/vfd_r_minfreq.msgparread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I760=micro820.micro820.vfd_configmap/vfd_r_minfreq.msgparread.__adi_reqdata,0xFFFFFFFF,UINT
I761=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgparwrite.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I762=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgparwrite.__adi_resdata,0xFFFFFFFF,UINT
I763=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgtimeout.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I764=micro820.micro820.vfd_configmap/vfd_w_minfreq.msgtimeout.__adi_resdata,0xFFFFFFFF,UINT
I765=micro820.micro820.vfd_configmap/vfd_r_stopmode.msgparread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I766=micro820.micro820.vfd_configmap/vfd_r_stopmode.msgparread.__adi_reqdata,0xFFFFFFFF,UINT
I767=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgparwrite.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I768=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgparwrite.__adi_resdata,0xFFFFFFFF,UINT
I769=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgtimeout.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I770=micro820.micro820.vfd_configmap/vfd_w_stopmode.msgtimeout.__adi_resdata,0xFFFFFFFF,UINT
I771=micro820.micro820.vfd_configmap/vfd_r_torqueperfmode.msgparread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I772=micro820.micro820.vfd_configmap/vfd_r_torqueperfmode.msgparread.__adi_reqdata,0xFFFFFFFF,UINT
I773=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgparwrite.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I774=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgparwrite.__adi_resdata,0xFFFFFFFF,UINT
I775=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgtimeout.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I776=micro820.micro820.vfd_configmap/vfd_w_torqueperfmode.msgtimeout.__adi_resdata,0xFFFFFFFF,UINT
[END]
