[BEGIN FB INPUTS]
I1=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.enable,0x450,BOOL
I2=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.src,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I3=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.srcoffset,0x21F6,UINT
I4=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I5=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.destoffset,0x21FE,UINT
I6=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.length,0x21F0,UINT
I7=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.swap,0x450,BOOL
I8=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.__adi_src,0xFFFFFFFF,UINT
I9=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.__adi_dest,0xFFFFFFFF,UINT
I10=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.__dti_src,0xFFFFFFFF,SINT
I11=micro820.micro820.vfd_messaging/vfd.cop_outputcurrent.__dti_dest,0xFFFFFFFF,SINT
I12=micro820.micro820.vfd_messaging/vfd.cop_drvtype.enable,0x450,BOOL
I13=micro820.micro820.vfd_messaging/vfd.cop_drvtype.src,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I14=micro820.micro820.vfd_messaging/vfd.cop_drvtype.srcoffset,0x21FE,UINT
I15=micro820.micro820.vfd_messaging/vfd.cop_drvtype.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I16=micro820.micro820.vfd_messaging/vfd.cop_drvtype.destoffset,0x21FE,UINT
I17=micro820.micro820.vfd_messaging/vfd.cop_drvtype.length,0x21F0,UINT
I18=micro820.micro820.vfd_messaging/vfd.cop_drvtype.swap,0x451,BOOL
I19=micro820.micro820.vfd_messaging/vfd.cop_drvtype.__adi_src,0xFFFFFFFF,UINT
I20=micro820.micro820.vfd_messaging/vfd.cop_drvtype.__adi_dest,0xFFFFFFFF,UINT
I21=micro820.micro820.vfd_messaging/vfd.cop_drvtype.__dti_src,0xFFFFFFFF,SINT
I22=micro820.micro820.vfd_messaging/vfd.cop_drvtype.__dti_dest,0xFFFFFFFF,SINT
I23=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.enable,0x450,BOOL
I24=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.src,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I25=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.srcoffset,0x21E8,UINT
I26=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I27=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.destoffset,0x21FE,UINT
I28=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.length,0x21F0,UINT
I29=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.swap,0x450,BOOL
I30=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.__adi_src,0xFFFFFFFF,UINT
I31=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.__adi_dest,0xFFFFFFFF,UINT
I32=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.__dti_src,0xFFFFFFFF,SINT
I33=micro820.micro820.vfd_messaging/vfd.cop_outputvoltage.__dti_dest,0xFFFFFFFF,SINT
I34=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.enable,0x450,BOOL
I35=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.src,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I36=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.srcoffset,0x21E4,UINT
I37=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I38=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.destoffset,0x21FE,UINT
I39=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.length,0x21F0,UINT
I40=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.swap,0x450,BOOL
I41=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.__adi_src,0xFFFFFFFF,UINT
I42=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.__adi_dest,0xFFFFFFFF,UINT
I43=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.__dti_src,0xFFFFFFFF,SINT
I44=micro820.micro820.vfd_messaging/vfd.cop_dcbusvoltage.__dti_dest,0xFFFFFFFF,SINT
I45=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.enable,0x450,BOOL
I46=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.src,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I47=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.srcoffset,0x21F6,UINT
I48=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I49=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.destoffset,0x21FE,UINT
I50=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.length,0x21F0,UINT
I51=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.swap,0x450,BOOL
I52=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.__adi_src,0xFFFFFFFF,UINT
I53=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.__adi_dest,0xFFFFFFFF,UINT
I54=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.__dti_src,0xFFFFFFFF,SINT
I55=micro820.micro820.vfd_messaging/vfd.cop_speedfbk.__dti_dest,0xFFFFFFFF,SINT
I56=micro820.micro820.vfd_messaging/vfd.cop_speedref.enable,0x450,BOOL
I57=micro820.micro820.vfd_messaging/vfd.cop_speedref.src,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I58=micro820.micro820.vfd_messaging/vfd.cop_speedref.srcoffset,0x21FE,UINT
I59=micro820.micro820.vfd_messaging/vfd.cop_speedref.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I60=micro820.micro820.vfd_messaging/vfd.cop_speedref.destoffset,0x21FE,UINT
I61=micro820.micro820.vfd_messaging/vfd.cop_speedref.length,0x21F6,UINT
I62=micro820.micro820.vfd_messaging/vfd.cop_speedref.swap,0x450,BOOL
I63=micro820.micro820.vfd_messaging/vfd.cop_speedref.__adi_src,0xFFFFFFFF,UINT
I64=micro820.micro820.vfd_messaging/vfd.cop_speedref.__adi_dest,0xFFFFFFFF,UINT
I65=micro820.micro820.vfd_messaging/vfd.cop_speedref.__dti_src,0xFFFFFFFF,SINT
I66=micro820.micro820.vfd_messaging/vfd.cop_speedref.__dti_dest,0xFFFFFFFF,SINT
I67=micro820.micro820.vfd_messaging/vfd.cop_deceltime.enable,0x450,BOOL
I68=micro820.micro820.vfd_messaging/vfd.cop_deceltime.src,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I69=micro820.micro820.vfd_messaging/vfd.cop_deceltime.srcoffset,0x21FE,UINT
I70=micro820.micro820.vfd_messaging/vfd.cop_deceltime.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I71=micro820.micro820.vfd_messaging/vfd.cop_deceltime.destoffset,0x21FE,UINT
I72=micro820.micro820.vfd_messaging/vfd.cop_deceltime.length,0x21F6,UINT
I73=micro820.micro820.vfd_messaging/vfd.cop_deceltime.swap,0x450,BOOL
I74=micro820.micro820.vfd_messaging/vfd.cop_deceltime.__adi_src,0xFFFFFFFF,UINT
I75=micro820.micro820.vfd_messaging/vfd.cop_deceltime.__adi_dest,0xFFFFFFFF,UINT
I76=micro820.micro820.vfd_messaging/vfd.cop_deceltime.__dti_src,0xFFFFFFFF,SINT
I77=micro820.micro820.vfd_messaging/vfd.cop_deceltime.__dti_dest,0xFFFFFFFF,SINT
I78=micro820.micro820.vfd_messaging/vfd.cop_acceltime.enable,0x450,BOOL
I79=micro820.micro820.vfd_messaging/vfd.cop_acceltime.src,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I80=micro820.micro820.vfd_messaging/vfd.cop_acceltime.srcoffset,0x21FE,UINT
I81=micro820.micro820.vfd_messaging/vfd.cop_acceltime.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I82=micro820.micro820.vfd_messaging/vfd.cop_acceltime.destoffset,0x21FE,UINT
I83=micro820.micro820.vfd_messaging/vfd.cop_acceltime.length,0x21F6,UINT
I84=micro820.micro820.vfd_messaging/vfd.cop_acceltime.swap,0x450,BOOL
I85=micro820.micro820.vfd_messaging/vfd.cop_acceltime.__adi_src,0xFFFFFFFF,UINT
I86=micro820.micro820.vfd_messaging/vfd.cop_acceltime.__adi_dest,0xFFFFFFFF,UINT
I87=micro820.micro820.vfd_messaging/vfd.cop_acceltime.__dti_src,0xFFFFFFFF,SINT
I88=micro820.micro820.vfd_messaging/vfd.cop_acceltime.__dti_dest,0xFFFFFFFF,SINT
I89=micro820.micro820.vfd_messaging/vfd.cop_faultcode.enable,0x450,BOOL
I90=micro820.micro820.vfd_messaging/vfd.cop_faultcode.src,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I91=micro820.micro820.vfd_messaging/vfd.cop_faultcode.srcoffset,0x21FA,UINT
I92=micro820.micro820.vfd_messaging/vfd.cop_faultcode.dest,0xFFFFFFFF,____FB_INIT_CONST_0000000D
I93=micro820.micro820.vfd_messaging/vfd.cop_faultcode.destoffset,0x21FE,UINT
I94=micro820.micro820.vfd_messaging/vfd.cop_faultcode.length,0x21F0,UINT
I95=micro820.micro820.vfd_messaging/vfd.cop_faultcode.swap,0x450,BOOL
I96=micro820.micro820.vfd_messaging/vfd.cop_faultcode.__adi_src,0xFFFFFFFF,UINT
I97=micro820.micro820.vfd_messaging/vfd.cop_faultcode.__adi_dest,0xFFFFFFFF,UINT
I98=micro820.micro820.vfd_messaging/vfd.cop_faultcode.__dti_src,0xFFFFFFFF,SINT
I99=micro820.micro820.vfd_messaging/vfd.cop_faultcode.__dti_dest,0xFFFFFFFF,SINT
I100=micro820.micro820.readdownholedata/modbuscycletimer.in,0x2186,BOOL
I101=micro820.micro820.readdownholedata/modbuscycletimer.pt,0x518,TIME
I102=micro820.micro820.control/linearscale_pressure.raw_min,0x2800,REAL
I103=micro820.micro820.control/linearscale_pressure.raw_max,0x27FC,REAL
I104=micro820.micro820.control/linearscale_pressure.eu_min,0x4D4,REAL
I105=micro820.micro820.control/linearscale_pressure.eu_max,0x4D8,REAL
I106=micro820.micro820.control/linearscale_pressure.raw_inp,0x2810,REAL
I107=micro820.micro820.vfd_messaging/vfd.fben,0x218F,BOOL
I108=micro820.micro820.vfd_messaging/vfd.ipaddress,0x73A,STRING
I109=micro820.micro820.vfd_messaging/vfd.updaterate_ms,0x2200,UINT
I110=micro820.micro820.vfd_messaging/vfd.enetctrlto_sec,0x21C0,USINT
I111=micro820.micro820.vfd_messaging/vfd.stop,0x472,BOOL
I112=micro820.micro820.vfd_messaging/vfd.start,0x473,BOOL
I113=micro820.micro820.vfd_messaging/vfd.jog,0x474,BOOL
I114=micro820.micro820.vfd_messaging/vfd.clrfault,0x475,BOOL
I115=micro820.micro820.vfd_messaging/vfd.setfwd,0x450,BOOL
I116=micro820.micro820.vfd_messaging/vfd.setrev,0x451,BOOL
I117=micro820.micro820.vfd_messaging/vfd.speedref,0x4E0,REAL
I118=micro820.micro820.vfd_messaging/vfd.acceltime1,0x4E4,REAL
I119=micro820.micro820.vfd_messaging/vfd.deceltime1,0x4E8,REAL
I120=micro820.micro820.vfd_messaging/vfd.msgtimeout_q_rtrig.clk,0x2199,BOOL
I121=micro820.micro820.vfd_messaging/vfd.msgparread_err_rtrig.clk,0x2199,BOOL
I122=micro820.micro820.vfd_messaging/vfd.msgparwrite_q_rtrig.clk,0x2199,BOOL
I123=micro820.micro820.vfd_messaging/vfd.msgparread_q_rtrig.clk,0x2199,BOOL
I124=micro820.micro820.vfd_messaging/vfd.fben_rtrig.clk,0x2199,BOOL
I125=micro820.micro820.vfd_messaging/vfd.msgtimeout_err_rtrig.clk,0x2199,BOOL
I126=micro820.micro820.vfd_messaging/vfd.msgsts_err_rtrig.clk,0x2199,BOOL
I127=micro820.micro820.vfd_messaging/vfd.msgcmd_err_rtrig.clk,0x2199,BOOL
I128=micro820.micro820.vfd_messaging/vfd.msgdrvtype_q_rtrig.clk,0x2199,BOOL
I129=micro820.micro820.vfd_messaging/vfd.msgdrvtype_err_rtrig.clk,0x2199,BOOL
I130=micro820.micro820.vfd_messaging/vfd.msgsts_q_rtrig.clk,0x2199,BOOL
I131=micro820.micro820.vfd_messaging/vfd.msgparwrite_err_rtrig.clk,0x2199,BOOL
I132=micro820.micro820.vfd_messaging/vfd.msgcmd_q_rtrig.clk,0x2199,BOOL
I133=micro820.micro820.readdownholedata/modbusdata_0.in,0x2187,BOOL
I134=micro820.micro820.readdownholedata/modbusdata_0.cancel,0x480,BOOL
I135=micro820.micro820.readdownholedata/modbusdata_0.localcfg,0xFFFFFFFF,MODBUSLOCPARA
I136=micro820.micro820.readdownholedata/modbusdata_0.targetcfg,0xFFFFFFFF,MODBUSTARPARA
I137=micro820.micro820.readdownholedata/modbusdata_0.localaddr,0xFFFFFFFF,MODBUSLOCADDR
I138=micro820.micro820.readdownholedata/modbusdata_0.__adi_localaddr,0xFFFFFFFF,UINT
I139=micro820.micro820.readdownholedata/modbusdata_1000.in,0x2187,BOOL
I140=micro820.micro820.readdownholedata/modbusdata_1000.cancel,0x480,BOOL
I141=micro820.micro820.readdownholedata/modbusdata_1000.localcfg,0xFFFFFFFF,MODBUSLOCPARA
I142=micro820.micro820.readdownholedata/modbusdata_1000.targetcfg,0xFFFFFFFF,MODBUSTARPARA
I143=micro820.micro820.readdownholedata/modbusdata_1000.localaddr,0xFFFFFFFF,MODBUSLOCADDR
I144=micro820.micro820.readdownholedata/modbusdata_1000.__adi_localaddr,0xFFFFFFFF,UINT
I145=micro820.micro820.vfd_messaging/vfd.msg_parread.in,0x21A3,BOOL
I146=micro820.micro820.vfd_messaging/vfd.msg_parread.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I147=micro820.micro820.vfd_messaging/vfd.msg_parread.appcfg,0xFFFFFFFF,CIPAPPCFG
I148=micro820.micro820.vfd_messaging/vfd.msg_parread.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I149=micro820.micro820.vfd_messaging/vfd.msg_parread.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I150=micro820.micro820.vfd_messaging/vfd.msg_parread.reqlength,0x2214,UINT
I151=micro820.micro820.vfd_messaging/vfd.msg_parread.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I152=micro820.micro820.vfd_messaging/vfd.msg_parread.__adi_reqdata,0xFFFFFFFF,UINT
I153=micro820.micro820.vfd_messaging/vfd.msg_parread.__adi_resdata,0xFFFFFFFF,UINT
I154=micro820.micro820.vfd_messaging/vfd.msg_cmd.in,0x21A3,BOOL
I155=micro820.micro820.vfd_messaging/vfd.msg_cmd.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I156=micro820.micro820.vfd_messaging/vfd.msg_cmd.appcfg,0xFFFFFFFF,CIPAPPCFG
I157=micro820.micro820.vfd_messaging/vfd.msg_cmd.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I158=micro820.micro820.vfd_messaging/vfd.msg_cmd.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I159=micro820.micro820.vfd_messaging/vfd.msg_cmd.reqlength,0x2214,UINT
I160=micro820.micro820.vfd_messaging/vfd.msg_cmd.__adi_reqdata,0xFFFFFFFF,UINT
I161=micro820.micro820.vfd_messaging/vfd.msg_sts.in,0x21A3,BOOL
I162=micro820.micro820.vfd_messaging/vfd.msg_sts.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I163=micro820.micro820.vfd_messaging/vfd.msg_sts.appcfg,0xFFFFFFFF,CIPAPPCFG
I164=micro820.micro820.vfd_messaging/vfd.msg_sts.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I165=micro820.micro820.vfd_messaging/vfd.msg_sts.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I166=micro820.micro820.vfd_messaging/vfd.msg_sts.__adi_resdata,0xFFFFFFFF,UINT
I167=micro820.micro820.vfd_messaging/vfd.msg_timeout.in,0x21A3,BOOL
I168=micro820.micro820.vfd_messaging/vfd.msg_timeout.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I169=micro820.micro820.vfd_messaging/vfd.msg_timeout.appcfg,0xFFFFFFFF,CIPAPPCFG
I170=micro820.micro820.vfd_messaging/vfd.msg_timeout.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I171=micro820.micro820.vfd_messaging/vfd.msg_timeout.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I172=micro820.micro820.vfd_messaging/vfd.msg_timeout.reqlength,0x21FC,UINT
I173=micro820.micro820.vfd_messaging/vfd.msg_timeout.__adi_reqdata,0xFFFFFFFF,UINT
I174=micro820.micro820.vfd_messaging/vfd.msg_parwrite.in,0x21A3,BOOL
I175=micro820.micro820.vfd_messaging/vfd.msg_parwrite.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I176=micro820.micro820.vfd_messaging/vfd.msg_parwrite.appcfg,0xFFFFFFFF,CIPAPPCFG
I177=micro820.micro820.vfd_messaging/vfd.msg_parwrite.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I178=micro820.micro820.vfd_messaging/vfd.msg_parwrite.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I179=micro820.micro820.vfd_messaging/vfd.msg_parwrite.reqlength,0x2214,UINT
I180=micro820.micro820.vfd_messaging/vfd.msg_parwrite.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I181=micro820.micro820.vfd_messaging/vfd.msg_parwrite.__adi_reqdata,0xFFFFFFFF,UINT
I182=micro820.micro820.vfd_messaging/vfd.msg_parwrite.__adi_resdata,0xFFFFFFFF,UINT
I183=micro820.micro820.vfd_messaging/vfd.msg_drvtype.in,0x21A3,BOOL
I184=micro820.micro820.vfd_messaging/vfd.msg_drvtype.ctrlcfg,0xFFFFFFFF,CIPCONTROLCFG
I185=micro820.micro820.vfd_messaging/vfd.msg_drvtype.appcfg,0xFFFFFFFF,CIPAPPCFG
I186=micro820.micro820.vfd_messaging/vfd.msg_drvtype.targetcfg,0xFFFFFFFF,CIPTARGETCFG
I187=micro820.micro820.vfd_messaging/vfd.msg_drvtype.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I188=micro820.micro820.vfd_messaging/vfd.msg_drvtype.__adi_resdata,0xFFFFFFFF,UINT
I189=micro820.micro820.downtime_timer.in,0x21D3,BOOL
I190=micro820.micro820.downtime_timer.pt,0x2D84,TIME
I191=micro820.micro820.vfd_messaging/vfd.msg_drvtype.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I192=micro820.micro820.vfd_messaging/vfd.msg_drvtype.reqlength,0x2216,UINT
I193=micro820.micro820.vfd_messaging/vfd.msg_drvtype.__adi_reqdata,0xFFFFFFFF,UINT
I194=micro820.micro820.vfd_messaging/vfd.msg_timeout.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I195=micro820.micro820.vfd_messaging/vfd.msg_timeout.__adi_resdata,0xFFFFFFFF,UINT
I196=micro820.micro820.vfd_messaging/vfd.msg_cmd.resdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I197=micro820.micro820.vfd_messaging/vfd.msg_cmd.__adi_resdata,0xFFFFFFFF,UINT
I198=micro820.micro820.vfd_messaging/vfd.msg_sts.reqdata,0xFFFFFFFF,____FB_INIT_CONST_0000000C
I199=micro820.micro820.vfd_messaging/vfd.msg_sts.reqlength,0x2216,UINT
I200=micro820.micro820.vfd_messaging/vfd.msg_sts.__adi_reqdata,0xFFFFFFFF,UINT
[END]
