Archive member included to satisfy reference by file (symbol)

/Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
                              (Reset_Handler)
/Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o (delay)
/Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o) (yield)
/Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(startup.c.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o) (SystemInit)
/Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o (SystemCoreClock)
/Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o) (analogReference)
/Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o (pinMode)
/Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_private.c.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o) (pinPeripheral)
/Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o) (tickReset)
/Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o (SERCOM::SERCOM(Sercom*))
/Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o (Uart::Uart(SERCOM*, unsigned char, unsigned char, SercomRXPad, SercomUartTXPad))
/Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o (map(long, long, long, long, long))
/Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o) (arduino::Print::write(unsigned char const*, unsigned int))
/Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o (main)
/Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o) (USBDeviceClass::attach())
/Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(abi.cpp.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o) (__cxa_pure_virtual)
/Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o) (arduino::PluggableUSB_::getInterface(unsigned char*))
/Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o) (operator new(unsigned int))
/Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o) (Serial_::begin(unsigned long))
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_thumb1_case_uqi.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o) (__gnu_thumb1_case_uqi)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivsi3.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o (__aeabi_uidiv)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_divsi3.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o) (__aeabi_idiv)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_dvmd_tls.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivsi3.o) (__aeabi_idiv0)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_arm_cmpdf2.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o) (__aeabi_dcmplt)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_aeabi_uldivmod.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o) (__aeabi_uldivmod)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_fixunsdfsi.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o) (__aeabi_d2uiz)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivmoddi4.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_aeabi_uldivmod.o) (__udivmoddi4)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(adddf3.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o) (__aeabi_dadd)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(divdf3.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o) (__aeabi_ddiv)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(eqdf2.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_arm_cmpdf2.o) (__eqdf2)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(gedf2.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_arm_cmpdf2.o) (__gedf2)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(ledf2.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_arm_cmpdf2.o) (__ledf2)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(muldf3.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o) (__aeabi_dmul)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(subdf3.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o) (__aeabi_dsub)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(unorddf2.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o) (__aeabi_dcmpun)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(fixdfsi.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_fixunsdfsi.o) (__aeabi_d2iz)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(floatunsidf.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o) (__aeabi_ui2d)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_clzsi2.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(adddf3.o) (__clzsi2)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_clzdi2.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivmoddi4.o) (__clzdi2)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-exit.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o (exit)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-impure.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-exit.o) (_global_impure_ptr)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-init.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o (__libc_init_array)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-malloc.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o) (malloc)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-memcpy-stub.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o) (memcpy)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-memset.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o (memset)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-freer.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-malloc.o) (_free_r)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-mallocr.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-malloc.o) (_malloc_r)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-sbrkr.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-mallocr.o) (_sbrk_r)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-strlen.o)
                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o) (strlen)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-mlock.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-freer.o) (__malloc_lock)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-reent.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-sbrkr.o) (errno)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a(sbrk.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-sbrkr.o) (_sbrk)
/Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a(_exit.o)
                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-exit.o) (_exit)

Allocating common symbols
Common symbol       size              file

errno               0x4               /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-reent.o)

Discarded input sections

 .text          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crti.o
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crti.o
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crti.o
 .data          0x0000000000000000        0x4 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtbegin.o
 .text          0x0000000000000000       0x78 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
 .ARM.extab     0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
 .ARM.exidx     0x0000000000000000        0x8 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
 .ARM.attributes
                0x0000000000000000       0x1b /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
 .text._Z9openBlindv
                0x0000000000000000       0x2c /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
 .text._Z10closeBlindv
                0x0000000000000000       0x2c /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
 .bss.position  0x0000000000000000        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/avr/Servo.cpp.o
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/avr/Servo.cpp.o
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/avr/Servo.cpp.o
 .debug_line    0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/avr/Servo.cpp.o
 .debug_str     0x0000000000000000      0x16e /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/avr/Servo.cpp.o
 .comment       0x0000000000000000       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/avr/Servo.cpp.o
 .ARM.attributes
                0x0000000000000000       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/avr/Servo.cpp.o
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/mbed/Servo.cpp.o
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/mbed/Servo.cpp.o
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/mbed/Servo.cpp.o
 .debug_line    0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/mbed/Servo.cpp.o
 .debug_str     0x0000000000000000      0x16f /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/mbed/Servo.cpp.o
 .comment       0x0000000000000000       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/mbed/Servo.cpp.o
 .ARM.attributes
                0x0000000000000000       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/mbed/Servo.cpp.o
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/megaavr/Servo.cpp.o
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/megaavr/Servo.cpp.o
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/megaavr/Servo.cpp.o
 .debug_line    0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/megaavr/Servo.cpp.o
 .debug_str     0x0000000000000000      0x172 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/megaavr/Servo.cpp.o
 .comment       0x0000000000000000       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/megaavr/Servo.cpp.o
 .ARM.attributes
                0x0000000000000000       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/megaavr/Servo.cpp.o
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/nrf52/Servo.cpp.o
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/nrf52/Servo.cpp.o
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/nrf52/Servo.cpp.o
 .debug_line    0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/nrf52/Servo.cpp.o
 .debug_str     0x0000000000000000      0x170 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/nrf52/Servo.cpp.o
 .comment       0x0000000000000000       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/nrf52/Servo.cpp.o
 .ARM.attributes
                0x0000000000000000       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/nrf52/Servo.cpp.o
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/sam/Servo.cpp.o
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/sam/Servo.cpp.o
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/sam/Servo.cpp.o
 .debug_line    0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/sam/Servo.cpp.o
 .debug_str     0x0000000000000000      0x16e /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/sam/Servo.cpp.o
 .comment       0x0000000000000000       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/sam/Servo.cpp.o
 .ARM.attributes
                0x0000000000000000       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/sam/Servo.cpp.o
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 .text._ZN5Servo6detachEv
                0x0000000000000000       0x40 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 .text._ZN5Servo17writeMicrosecondsEi
                0x0000000000000000       0x50 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 .text._ZN5Servo5writeEi
                0x0000000000000000       0x44 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 .text._ZN5Servo16readMicrosecondsEv
                0x0000000000000000       0x38 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 .text._ZN5Servo4readEv
                0x0000000000000000       0x2c /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 .text._ZN5Servo8attachedEv
                0x0000000000000000       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/stm32f4/Servo.cpp.o
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/stm32f4/Servo.cpp.o
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/stm32f4/Servo.cpp.o
 .debug_line    0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/stm32f4/Servo.cpp.o
 .debug_str     0x0000000000000000      0x172 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/stm32f4/Servo.cpp.o
 .comment       0x0000000000000000       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/stm32f4/Servo.cpp.o
 .ARM.attributes
                0x0000000000000000       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/stm32f4/Servo.cpp.o
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
 .text.PINCOUNT_fn
                0x0000000000000000        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
 .data.g_apTCInstances
                0x0000000000000000       0x18 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
 .text.delayMicroseconds
                0x0000000000000000       0x16 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
 .text.__halt   0x0000000000000000        0x2 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(startup.c.o)
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(startup.c.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(startup.c.o)
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .text.analogReadResolution
                0x0000000000000000       0x4c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .text.analogWriteResolution
                0x0000000000000000        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .text.analogWrite
                0x0000000000000000      0x1d4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .rodata        0x0000000000000000       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .bss.tcEnabled.13064
                0x0000000000000000        0x6 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .data._writeResolution
                0x0000000000000000        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
 .text.digitalRead
                0x0000000000000000       0x30 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_private.c.o)
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_private.c.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_private.c.o)
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
 .text.resetExternalChip
                0x0000000000000000        0x2 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM25isBufferOverflowErrorUARTEv
                0x0000000000000000        0xa /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM17isParityErrorUARTEv
                0x0000000000000000        0xa /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM12initSPIClockE18SercomSpiClockModem
                0x0000000000000000       0x30 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM8resetSPIEv
                0x0000000000000000       0x1a /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM9enableSPIEv
                0x0000000000000000       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM10disableSPIEv
                0x0000000000000000       0x12 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM15setDataOrderSPIE15SercomDataOrder
                0x0000000000000000       0x28 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM15getDataOrderSPIEv
                0x0000000000000000        0xa /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM14setBaudrateSPIEh
                0x0000000000000000       0x30 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM15setClockModeSPIE18SercomSpiClockMode
                0x0000000000000000       0x40 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM15transferDataSPIEh
                0x0000000000000000       0x1a /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM24isBufferOverflowErrorSPIEv
                0x0000000000000000        0xa /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM22isDataRegisterEmptySPIEv
                0x0000000000000000        0xa /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM28calculateBaudrateSynchronousEm
                0x0000000000000000       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM9resetWIREEv
                0x0000000000000000       0x1a /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM10enableWIREEv
                0x0000000000000000       0x2a /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM11disableWIREEv
                0x0000000000000000       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM18prepareNackBitWIREEv
                0x0000000000000000       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM17prepareAckBitWIREEv
                0x0000000000000000       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM22prepareCommandBitsWireEh
                0x0000000000000000       0x2c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM21startTransmissionWIREEh23SercomWireReadWriteFlag
                0x0000000000000000       0x84 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM18sendDataMasterWIREEh
                0x0000000000000000       0x30 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM17sendDataSlaveWIREEh
                0x0000000000000000       0x1c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM12isMasterWIREEv
                0x0000000000000000       0x12 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM11isSlaveWIREEv
                0x0000000000000000       0x12 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM13isBusIdleWIREEv
                0x0000000000000000       0x12 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM14isBusOwnerWIREEv
                0x0000000000000000       0x12 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM13isArbLostWIREEv
                0x0000000000000000        0xa /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM13isBusBusyWIREEv
                0x0000000000000000       0x12 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM15isDataReadyWIREEv
                0x0000000000000000        0xa /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM18isStopDetectedWIREEv
                0x0000000000000000        0xa /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM21isRestartDetectedWIREEv
                0x0000000000000000        0xa /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM14isAddressMatchEv
                0x0000000000000000        0xa /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM25isMasterReadOperationWIREEv
                0x0000000000000000        0xa /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM20isRXNackReceivedWIREEv
                0x0000000000000000        0xa /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM13availableWIREEv
                0x0000000000000000       0x18 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM12readDataWIREEv
                0x0000000000000000       0x20 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM7initSPIE14SercomSpiTXPad11SercomRXPad17SercomSpiCharSize15SercomDataOrder
                0x0000000000000000       0x4a /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM13initSlaveWIREEhb
                0x0000000000000000       0x4a /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .text._ZN6SERCOM14initMasterWIREEm
                0x0000000000000000       0x54 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .group         0x0000000000000000        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
 .group         0x0000000000000000        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
 .group         0x0000000000000000        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
 .group         0x0000000000000000        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
 .group         0x0000000000000000        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
 .text._ZN4UartC2EP6SERCOMhh11SercomRXPad15SercomUartTXPadhh
                0x0000000000000000       0x88 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
 .text._Z3maplllll
                0x0000000000000000       0x16 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
 .text._Z8makeWordt
                0x0000000000000000        0x2 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
 .text._Z8makeWordhh
                0x0000000000000000        0x6 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
 .debug_info    0x0000000000000000      0x160 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
 .debug_abbrev  0x0000000000000000       0xa9 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
 .debug_loc     0x0000000000000000       0xb0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
 .debug_aranges
                0x0000000000000000       0x30 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
 .debug_ranges  0x0000000000000000       0x20 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
 .debug_line    0x0000000000000000      0x1aa /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
 .debug_str     0x0000000000000000      0x282 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
 .comment       0x0000000000000000       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
 .debug_frame   0x0000000000000000       0x48 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
 .ARM.attributes
                0x0000000000000000       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
 .group         0x0000000000000000        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .group         0x0000000000000000        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .group         0x0000000000000000        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print17availableForWriteEv
                0x0000000000000000        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5flushEv
                0x0000000000000000        0x2 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5writeEPKc.part.2
                0x0000000000000000       0x1a /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5writeEPKc
                0x0000000000000000       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEPKNS_19__FlashStringHelperE
                0x0000000000000000        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printERKNS_6StringE
                0x0000000000000000        0xe /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEPKc
                0x0000000000000000        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEc
                0x0000000000000000        0xa /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printERKNS_9PrintableE
                0x0000000000000000       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnEv
                0x0000000000000000       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnEPKNS_19__FlashStringHelperE
                0x0000000000000000       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnERKNS_6StringE
                0x0000000000000000       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnEPKc
                0x0000000000000000       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnEc
                0x0000000000000000       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnERKNS_9PrintableE
                0x0000000000000000       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print11printNumberEmh
                0x0000000000000000       0x48 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEli
                0x0000000000000000       0x3e /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEii
                0x0000000000000000        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnEii
                0x0000000000000000       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnEli
                0x0000000000000000       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEmi
                0x0000000000000000       0x18 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEhi
                0x0000000000000000        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnEhi
                0x0000000000000000       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEji
                0x0000000000000000        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnEji
                0x0000000000000000       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnEmi
                0x0000000000000000       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print14printULLNumberEyh
                0x0000000000000000       0xe0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printExi
                0x0000000000000000       0x50 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnExi
                0x0000000000000000       0x18 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEyi
                0x0000000000000000       0x1e /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnEyi
                0x0000000000000000       0x18 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print10printFloatEdi
                0x0000000000000000      0x170 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEdi
                0x0000000000000000        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnEdi
                0x0000000000000000       0x18 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .rodata._ZN7arduino5Print10printFloatEdi.str1.1
                0x0000000000000000        0xe /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .rodata._ZN7arduino5Print7printlnEv.str1.1
                0x0000000000000000        0x3 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .rodata._ZTVN7arduino5PrintE
                0x0000000000000000       0x18 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
 .group         0x0000000000000000       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .group         0x0000000000000000        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .group         0x0000000000000000        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .group         0x0000000000000000        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .group         0x0000000000000000        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .group         0x0000000000000000        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .group         0x0000000000000000        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .group         0x0000000000000000        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .group         0x0000000000000000        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .group         0x0000000000000000        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .group         0x0000000000000000        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .group         0x0000000000000000        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .text._ZN7__GuardD2Ev
                0x0000000000000000        0xe /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .text._ZN14USBDeviceClass7standbyEv
                0x0000000000000000       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .text._ZN14USBDeviceClass6detachEv
                0x0000000000000000       0x18 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .text._ZN14USBDeviceClass3endEv
                0x0000000000000000       0x18 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .text._ZN14USBDeviceClass10configuredEv
                0x0000000000000000       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .text._ZN14USBDeviceClass5stallEm
                0x0000000000000000       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .text._ZN14USBDeviceClass9connectedEv
                0x0000000000000000       0x24 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .text._ZN14USBDeviceClass12packMessagesEb
                0x0000000000000000       0x2c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(abi.cpp.o)
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(abi.cpp.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(abi.cpp.o)
 .text.__cxa_pure_virtual
                0x0000000000000000        0x2 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(abi.cpp.o)
 .text.__cxa_deleted_virtual
                0x0000000000000000        0x2 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(abi.cpp.o)
 .debug_info    0x0000000000000000      0xe6d /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(abi.cpp.o)
 .debug_abbrev  0x0000000000000000      0x26f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(abi.cpp.o)
 .debug_aranges
                0x0000000000000000       0x28 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(abi.cpp.o)
 .debug_ranges  0x0000000000000000       0x18 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(abi.cpp.o)
 .debug_line    0x0000000000000000      0x347 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(abi.cpp.o)
 .debug_str     0x0000000000000000      0x76e /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(abi.cpp.o)
 .comment       0x0000000000000000       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(abi.cpp.o)
 .debug_frame   0x0000000000000000       0x30 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(abi.cpp.o)
 .ARM.attributes
                0x0000000000000000       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(abi.cpp.o)
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
 .text._Znaj    0x0000000000000000        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
 .text._ZdaPv   0x0000000000000000        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
 .text          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
 .data          0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
 .text.resetExternalChip
                0x0000000000000000        0x2 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
 .text._ZN7Serial_9readBytesEPcj
                0x0000000000000000       0x3e /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
 .text._ZN7Serial_9readBreakEv
                0x0000000000000000       0x1c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
 .text._ZN7Serial_4baudEv
                0x0000000000000000        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
 .text._ZN7Serial_8stopbitsEv
                0x0000000000000000        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
 .text._ZN7Serial_10paritytypeEv
                0x0000000000000000        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
 .text._ZN7Serial_7numbitsEv
                0x0000000000000000        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
 .text._ZN7Serial_3dtrEv
                0x0000000000000000       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
 .text._ZN7Serial_3rtsEv
                0x0000000000000000       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_thumb1_case_uqi.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_thumb1_case_uqi.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivsi3.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivsi3.o)
 .text          0x0000000000000000      0x1d4 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_divsi3.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_divsi3.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_divsi3.o)
 .debug_frame   0x0000000000000000       0x20 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_divsi3.o)
 .ARM.attributes
                0x0000000000000000       0x1e /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_divsi3.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_dvmd_tls.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_dvmd_tls.o)
 .text          0x0000000000000000       0x7c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_arm_cmpdf2.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_arm_cmpdf2.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_arm_cmpdf2.o)
 .ARM.attributes
                0x0000000000000000       0x1e /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_arm_cmpdf2.o)
 .text          0x0000000000000000       0x40 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_aeabi_uldivmod.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_aeabi_uldivmod.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_aeabi_uldivmod.o)
 .ARM.attributes
                0x0000000000000000       0x1e /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_aeabi_uldivmod.o)
 .text          0x0000000000000000       0x3c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_fixunsdfsi.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_fixunsdfsi.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_fixunsdfsi.o)
 .debug_frame   0x0000000000000000       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_fixunsdfsi.o)
 .ARM.attributes
                0x0000000000000000       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_fixunsdfsi.o)
 .text          0x0000000000000000      0x184 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivmoddi4.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivmoddi4.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivmoddi4.o)
 .ARM.extab     0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivmoddi4.o)
 .ARM.exidx     0x0000000000000000        0x8 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivmoddi4.o)
 .debug_frame   0x0000000000000000       0x3c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivmoddi4.o)
 .ARM.attributes
                0x0000000000000000       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivmoddi4.o)
 .text          0x0000000000000000      0x638 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(adddf3.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(adddf3.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(adddf3.o)
 .debug_frame   0x0000000000000000       0x38 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(adddf3.o)
 .ARM.attributes
                0x0000000000000000       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(adddf3.o)
 .text          0x0000000000000000      0x604 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(divdf3.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(divdf3.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(divdf3.o)
 .rodata        0x0000000000000000       0x40 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(divdf3.o)
 .debug_frame   0x0000000000000000       0x3c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(divdf3.o)
 .ARM.attributes
                0x0000000000000000       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(divdf3.o)
 .text          0x0000000000000000       0x78 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(eqdf2.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(eqdf2.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(eqdf2.o)
 .debug_frame   0x0000000000000000       0x38 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(eqdf2.o)
 .ARM.attributes
                0x0000000000000000       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(eqdf2.o)
 .text          0x0000000000000000       0xc8 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(gedf2.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(gedf2.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(gedf2.o)
 .debug_frame   0x0000000000000000       0x38 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(gedf2.o)
 .ARM.attributes
                0x0000000000000000       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(gedf2.o)
 .text          0x0000000000000000       0xd0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(ledf2.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(ledf2.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(ledf2.o)
 .debug_frame   0x0000000000000000       0x38 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(ledf2.o)
 .ARM.attributes
                0x0000000000000000       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(ledf2.o)
 .text          0x0000000000000000      0x4e4 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(muldf3.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(muldf3.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(muldf3.o)
 .rodata        0x0000000000000000       0x40 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(muldf3.o)
 .debug_frame   0x0000000000000000       0x3c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(muldf3.o)
 .ARM.attributes
                0x0000000000000000       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(muldf3.o)
 .text          0x0000000000000000      0x690 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(subdf3.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(subdf3.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(subdf3.o)
 .debug_frame   0x0000000000000000       0x3c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(subdf3.o)
 .ARM.attributes
                0x0000000000000000       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(subdf3.o)
 .text          0x0000000000000000       0x38 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(unorddf2.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(unorddf2.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(unorddf2.o)
 .debug_frame   0x0000000000000000       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(unorddf2.o)
 .ARM.attributes
                0x0000000000000000       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(unorddf2.o)
 .text          0x0000000000000000       0x6c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(fixdfsi.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(fixdfsi.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(fixdfsi.o)
 .debug_frame   0x0000000000000000       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(fixdfsi.o)
 .ARM.attributes
                0x0000000000000000       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(fixdfsi.o)
 .text          0x0000000000000000       0x64 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(floatunsidf.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(floatunsidf.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(floatunsidf.o)
 .debug_frame   0x0000000000000000       0x28 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(floatunsidf.o)
 .ARM.attributes
                0x0000000000000000       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(floatunsidf.o)
 .text          0x0000000000000000       0x3c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_clzsi2.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_clzsi2.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_clzsi2.o)
 .ARM.attributes
                0x0000000000000000       0x1e /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_clzsi2.o)
 .text          0x0000000000000000       0x18 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_clzdi2.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_clzdi2.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_clzdi2.o)
 .ARM.attributes
                0x0000000000000000       0x1e /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_clzdi2.o)
 .text          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-exit.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-exit.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-exit.o)
 .text.exit     0x0000000000000000       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-exit.o)
 .debug_frame   0x0000000000000000       0x28 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-exit.o)
 .ARM.attributes
                0x0000000000000000       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-exit.o)
 .text          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-impure.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-impure.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-impure.o)
 .rodata._global_impure_ptr
                0x0000000000000000        0x4 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-impure.o)
 .text          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-init.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-init.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-init.o)
 .text          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-malloc.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-malloc.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-malloc.o)
 .text          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-memcpy-stub.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-memcpy-stub.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-memcpy-stub.o)
 .text          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-memset.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-memset.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-memset.o)
 .text          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-freer.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-freer.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-freer.o)
 .text          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-mallocr.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-mallocr.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-mallocr.o)
 .text          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-sbrkr.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-sbrkr.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-sbrkr.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-strlen.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-strlen.o)
 .text          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-mlock.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-mlock.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-mlock.o)
 .text          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-reent.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-reent.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-reent.o)
 .text.cleanup_glue
                0x0000000000000000       0x1a /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-reent.o)
 .text._reclaim_reent
                0x0000000000000000       0xcc /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-reent.o)
 .text          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a(sbrk.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a(sbrk.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a(sbrk.o)
 .text          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a(_exit.o)
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a(_exit.o)
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a(_exit.o)
 .text._exit    0x0000000000000000        0x4 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a(_exit.o)
 .debug_frame   0x0000000000000000       0x20 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a(_exit.o)
 .ARM.attributes
                0x0000000000000000       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a(_exit.o)
 .text          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtend.o
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtend.o
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtend.o
 .text          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtn.o
 .data          0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtn.o
 .bss           0x0000000000000000        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtn.o

Memory Configuration

Name             Origin             Length             Attributes
FLASH            0x0000000000002000 0x000000000003e000 xr
RAM              0x0000000020000000 0x0000000000008000 xrw
*default*        0x0000000000000000 0xffffffffffffffff

Linker script and memory map

LOAD /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crti.o
LOAD /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtbegin.o
LOAD /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
LOAD /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
LOAD /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/avr/Servo.cpp.o
LOAD /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/mbed/Servo.cpp.o
LOAD /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/megaavr/Servo.cpp.o
LOAD /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/nrf52/Servo.cpp.o
LOAD /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/sam/Servo.cpp.o
LOAD /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
LOAD /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/stm32f4/Servo.cpp.o
LOAD /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
START GROUP
LOAD /Users/nico/Library/Arduino15/packages/arduino/tools/CMSIS/4.5.0/CMSIS/Lib/GCC//libarm_cortexM0l_math.a
LOAD /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a
END GROUP
LOAD /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libstdc++_nano.a
LOAD /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libm.a
START GROUP
LOAD /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a
LOAD /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a
END GROUP
START GROUP
LOAD /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a
LOAD /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a
LOAD /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a
END GROUP
START GROUP
LOAD /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a
LOAD /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a
LOAD /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a
END GROUP
LOAD /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtend.o
LOAD /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtn.o

.text           0x0000000000002000     0x2f00
                0x0000000000002000                __text_start__ = .
 *(.sketch_boot)
                0x0000000000002000                . = ALIGN (0x2000)
 *(.isr_vector)
 .isr_vector    0x0000000000002000       0xb4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
                0x0000000000002000                exception_table
 *(.text*)
 .text          0x00000000000020b4       0x48 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtbegin.o
 .text.setup    0x00000000000020fc       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
                0x00000000000020fc                setup
 .text.loop     0x000000000000210c       0x1c /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
                0x000000000000210c                loop
 .text.startup._GLOBAL__sub_I_blind
                0x0000000000002128       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
 .text._Z13Servo_Handler18timer16_Sequence_tP2Tchh
                0x0000000000002138      0x120 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
                0x0000000000002138                Servo_Handler(timer16_Sequence_t, Tc*, unsigned char, unsigned char)
 .text.TC4_Handler
                0x0000000000002258       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
                0x0000000000002258                TC4_Handler
 .text._ZN5ServoC2Ev
                0x000000000000226c       0x48 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
                0x000000000000226c                Servo::Servo()
                0x000000000000226c                Servo::Servo()
 .text._ZN5Servo6attachEiii
                0x00000000000022b4      0x144 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
                0x00000000000022b4                Servo::attach(int, int, int)
 .text._ZN5Servo6attachEi
                0x00000000000023f8       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
                0x00000000000023f8                Servo::attach(int)
 .text.SERCOM5_Handler
                0x0000000000002408       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
                0x0000000000002408                SERCOM5_Handler
 .text.startup._GLOBAL__sub_I_g_APinDescription
                0x0000000000002418       0x80 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
 .text.Dummy_Handler
                0x0000000000002498        0x2 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
                0x0000000000002498                SYSCTRL_Handler
                0x0000000000002498                HardFault_Handler
                0x0000000000002498                AC_Handler
                0x0000000000002498                PendSV_Handler
                0x0000000000002498                NMI_Handler
                0x0000000000002498                TC7_Handler
                0x0000000000002498                SERCOM1_Handler
                0x0000000000002498                ADC_Handler
                0x0000000000002498                TCC1_Handler
                0x0000000000002498                SERCOM2_Handler
                0x0000000000002498                TCC0_Handler
                0x0000000000002498                RTC_Handler
                0x0000000000002498                EIC_Handler
                0x0000000000002498                TC6_Handler
                0x0000000000002498                WDT_Handler
                0x0000000000002498                TC3_Handler
                0x0000000000002498                Dummy_Handler
                0x0000000000002498                PM_Handler
                0x0000000000002498                SVC_Handler
                0x0000000000002498                TCC2_Handler
                0x0000000000002498                EVSYS_Handler
                0x0000000000002498                SERCOM3_Handler
                0x0000000000002498                SERCOM4_Handler
                0x0000000000002498                I2S_Handler
                0x0000000000002498                NVMCTRL_Handler
                0x0000000000002498                SERCOM0_Handler
                0x0000000000002498                DAC_Handler
                0x0000000000002498                PTC_Handler
                0x0000000000002498                DMAC_Handler
 *fill*         0x000000000000249a        0x2 
 .text.USB_Handler
                0x000000000000249c       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
                0x000000000000249c                USB_Handler
 .text.Reset_Handler
                0x00000000000024b0       0x54 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
                0x00000000000024b0                Reset_Handler
 .text.SysTick_Handler
                0x0000000000002504       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
                0x0000000000002504                SysTick_Handler
 .text.USB_SetHandler
                0x0000000000002514        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
                0x0000000000002514                USB_SetHandler
 .text.millis   0x0000000000002520        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
                0x0000000000002520                millis
 .text.micros   0x000000000000252c       0x60 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
                0x000000000000252c                micros
 .text.delay    0x000000000000258c       0x30 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
                0x000000000000258c                delay
 .text.resetExternalChip
                0x00000000000025bc        0x2 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
                0x00000000000025bc                resetExternalChip
 *fill*         0x00000000000025be        0x2 
 .text.SysTick_DefaultHandler
                0x00000000000025c0       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
                0x00000000000025c0                SysTick_DefaultHandler
 .text.__empty  0x00000000000025d4        0x2 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
                0x00000000000025d4                yield
 .text.__false  0x00000000000025d6        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
                0x00000000000025d6                sysTickHook
 *fill*         0x00000000000025da        0x2 
 .text.SystemInit
                0x00000000000025dc      0x160 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(startup.c.o)
                0x00000000000025dc                SystemInit
 .text.init     0x000000000000273c       0xf0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
                0x000000000000273c                init
 .text.mapResolution
                0x000000000000282c       0x12 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 *fill*         0x000000000000283e        0x2 
 .text.analogReference
                0x0000000000002840       0x64 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
                0x0000000000002840                analogReference
 .text.analogRead
                0x00000000000028a4       0xdc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
                0x00000000000028a4                analogRead
 .text.pinMode  0x0000000000002980       0x98 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
                0x0000000000002980                pinMode
 .text.digitalWrite
                0x0000000000002a18       0x58 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
                0x0000000000002a18                digitalWrite
 .text.pinPeripheral
                0x0000000000002a70       0xc0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_private.c.o)
                0x0000000000002a70                pinPeripheral
 .text.initiateReset
                0x0000000000002b30       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
                0x0000000000002b30                initiateReset
 .text.cancelReset
                0x0000000000002b44       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
                0x0000000000002b44                cancelReset
 .text.tickReset
                0x0000000000002b54       0x78 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
                0x0000000000002b54                tickReset
 .text._ZN6SERCOMC2EP6Sercom
                0x0000000000002bcc        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                0x0000000000002bcc                SERCOM::SERCOM(Sercom*)
                0x0000000000002bcc                SERCOM::SERCOM(Sercom*)
 .text._ZN6SERCOM9initFrameE18SercomUartCharSize15SercomDataOrder16SercomParityMode19SercomNumberStopBit
                0x0000000000002bd4       0x3a /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                0x0000000000002bd4                SERCOM::initFrame(SercomUartCharSize, SercomDataOrder, SercomParityMode, SercomNumberStopBit)
 .text._ZN6SERCOM8initPadsE15SercomUartTXPad11SercomRXPad
                0x0000000000002c0e       0x26 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                0x0000000000002c0e                SERCOM::initPads(SercomUartTXPad, SercomRXPad)
 .text._ZN6SERCOM9resetUARTEv
                0x0000000000002c34       0x1a /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                0x0000000000002c34                SERCOM::resetUART()
 .text._ZN6SERCOM10enableUARTEv
                0x0000000000002c4e       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                0x0000000000002c4e                SERCOM::enableUART()
 .text._ZN6SERCOM9flushUARTEv
                0x0000000000002c62       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                0x0000000000002c62                SERCOM::flushUART()
 .text._ZN6SERCOM15clearStatusUARTEv
                0x0000000000002c76        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                0x0000000000002c76                SERCOM::clearStatusUART()
 .text._ZN6SERCOM17availableDataUARTEv
                0x0000000000002c7e        0xa /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                0x0000000000002c7e                SERCOM::availableDataUART()
 .text._ZN6SERCOM11isUARTErrorEv
                0x0000000000002c88        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                0x0000000000002c88                SERCOM::isUARTError()
 .text._ZN6SERCOM20acknowledgeUARTErrorEv
                0x0000000000002c90        0xe /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                0x0000000000002c90                SERCOM::acknowledgeUARTError()
 .text._ZN6SERCOM16isFrameErrorUARTEv
                0x0000000000002c9e        0xa /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                0x0000000000002c9e                SERCOM::isFrameErrorUART()
 .text._ZN6SERCOM19clearFrameErrorUARTEv
                0x0000000000002ca8        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                0x0000000000002ca8                SERCOM::clearFrameErrorUART()
 .text._ZN6SERCOM23isDataRegisterEmptyUARTEv
                0x0000000000002cb4        0xa /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                0x0000000000002cb4                SERCOM::isDataRegisterEmptyUART()
 .text._ZN6SERCOM12readDataUARTEv
                0x0000000000002cbe        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                0x0000000000002cbe                SERCOM::readDataUART()
 .text._ZN6SERCOM13writeDataUARTEh
                0x0000000000002cc6       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                0x0000000000002cc6                SERCOM::writeDataUART(unsigned char)
 .text._ZN6SERCOM36enableDataRegisterEmptyInterruptUARTEv
                0x0000000000002cda        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                0x0000000000002cda                SERCOM::enableDataRegisterEmptyInterruptUART()
 .text._ZN6SERCOM37disableDataRegisterEmptyInterruptUARTEv
                0x0000000000002ce2        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                0x0000000000002ce2                SERCOM::disableDataRegisterEmptyInterruptUART()
 *fill*         0x0000000000002cea        0x2 
 .text._ZN6SERCOM13initClockNVICEv
                0x0000000000002cec       0xa8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                0x0000000000002cec                SERCOM::initClockNVIC()
 .text._ZN6SERCOM8initUARTE14SercomUartMode20SercomUartSampleRatem
                0x0000000000002d94       0x6c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                0x0000000000002d94                SERCOM::initUART(SercomUartMode, SercomUartSampleRate, unsigned long)
 .text._ZN4UartcvbEv
                0x0000000000002e00        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x0000000000002e00                Uart::operator bool()
 .text._ZN4Uart5beginEm
                0x0000000000002e04       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x0000000000002e04                Uart::begin(unsigned long)
 .text._ZN4Uart9availableEv
                0x0000000000002e14        0x6 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x0000000000002e14                Uart::available()
 .text._ZN4Uart17availableForWriteEv
                0x0000000000002e1a       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x0000000000002e1a                Uart::availableForWrite()
 .text._ZN4Uart4peekEv
                0x0000000000002e2a       0x18 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x0000000000002e2a                Uart::peek()
 .text._ZN4Uart3endEv
                0x0000000000002e42       0x24 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x0000000000002e42                Uart::end()
 .text._ZN4Uart5flushEv
                0x0000000000002e66       0x16 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x0000000000002e66                Uart::flush()
 .text._ZN7__GuardD2Ev
                0x0000000000002e7c        0xe /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x0000000000002e7c                __Guard::~__Guard()
                0x0000000000002e7c                __Guard::~__Guard()
 .text._ZN4Uart16extractNbStopBitEt
                0x0000000000002e8a        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x0000000000002e8a                Uart::extractNbStopBit(unsigned short)
 .text._ZN4Uart15extractCharSizeEt
                0x0000000000002e96       0x28 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x0000000000002e96                Uart::extractCharSize(unsigned short)
 .text._ZN4Uart13extractParityEt
                0x0000000000002ebe       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x0000000000002ebe                Uart::extractParity(unsigned short)
 *fill*         0x0000000000002ed2        0x2 
 .text._ZN4Uart5beginEmt
                0x0000000000002ed4       0xf8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x0000000000002ed4                Uart::begin(unsigned long, unsigned short)
 .text._ZN7arduino11RingBufferNILi256EEC2Ev
                0x0000000000002fcc       0x1e /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x0000000000002fcc                arduino::RingBufferN<256>::RingBufferN()
                0x0000000000002fcc                arduino::RingBufferN<256>::RingBufferN()
 *fill*         0x0000000000002fea        0x2 
 .text._ZN4UartC2EP6SERCOMhh11SercomRXPad15SercomUartTXPad
                0x0000000000002fec       0x74 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x0000000000002fec                Uart::Uart(SERCOM*, unsigned char, unsigned char, SercomRXPad, SercomUartTXPad)
                0x0000000000002fec                Uart::Uart(SERCOM*, unsigned char, unsigned char, SercomRXPad, SercomUartTXPad)
 .text._ZN7arduino15SafeRingBufferNILi256EE10store_charEh
                0x0000000000003060       0x4a /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x0000000000003060                arduino::SafeRingBufferN<256>::store_char(unsigned char)
 .text._ZN7arduino15SafeRingBufferNILi256EE9read_charEv
                0x00000000000030aa       0x50 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x00000000000030aa                arduino::SafeRingBufferN<256>::read_char()
 .text._ZN4Uart10IrqHandlerEv
                0x00000000000030fa       0xa4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x00000000000030fa                Uart::IrqHandler()
 *fill*         0x000000000000319e        0x2 
 .text._ZN4Uart5writeEh
                0x00000000000031a0       0x9c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x00000000000031a0                Uart::write(unsigned char)
 .text._ZN4Uart4readEv
                0x000000000000323c       0x34 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x000000000000323c                Uart::read()
 .text._ZN7arduino5Print5writeEPKhj
                0x0000000000003270       0x28 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
                0x0000000000003270                arduino::Print::write(unsigned char const*, unsigned int)
 .text.initVariant
                0x0000000000003298        0x2 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
                0x0000000000003298                initVariant
 *fill*         0x000000000000329a        0x2 
 .text.startup.main
                0x000000000000329c       0x40 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
                0x000000000000329c                main
 .text._ZN26DoubleBufferedEPOutHandlerD2Ev
                0x00000000000032dc        0x2 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x00000000000032dc                DoubleBufferedEPOutHandler::~DoubleBufferedEPOutHandler()
                0x00000000000032dc                DoubleBufferedEPOutHandler::~DoubleBufferedEPOutHandler()
 .text._ZN26DoubleBufferedEPOutHandlerD0Ev
                0x00000000000032de        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x00000000000032de                DoubleBufferedEPOutHandler::~DoubleBufferedEPOutHandler()
 *fill*         0x00000000000032ea        0x2 
 .text._ZN14USBDeviceClass6initEPEmm.part.7
                0x00000000000032ec       0xc4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .text._ZN7__GuardC2Ev
                0x00000000000033b0        0xe /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x00000000000033b0                __Guard::__Guard()
                0x00000000000033b0                __Guard::__Guard()
 .text._ZNK26DoubleBufferedEPOutHandler10_availableEv
                0x00000000000033be       0x70 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x00000000000033be                DoubleBufferedEPOutHandler::_available() const
 *fill*         0x000000000000342e        0x2 
 .text._ZN26DoubleBufferedEPOutHandler7releaseEv
                0x0000000000003430       0x38 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000003430                DoubleBufferedEPOutHandler::release()
 .text._ZN26DoubleBufferedEPOutHandler14handleEndpointEv
                0x0000000000003468       0xe2 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000003468                DoubleBufferedEPOutHandler::handleEndpoint()
 .text._ZN14USBDeviceClass14SendInterfacesEPm
                0x000000000000354a       0x20 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x000000000000354a                USBDeviceClass::SendInterfaces(unsigned long*)
 *fill*         0x000000000000356a        0x2 
 .text._ZN14USBDeviceClass6attachEv
                0x000000000000356c       0x34 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x000000000000356c                USBDeviceClass::attach()
 .text._ZN14USBDeviceClass10setAddressEm
                0x00000000000035a0       0x48 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x00000000000035a0                USBDeviceClass::setAddress(unsigned long)
 .text._ZN14USBDeviceClass25handleClassInterfaceSetupERN7arduino8USBSetupE
                0x00000000000035e8       0x24 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x00000000000035e8                USBDeviceClass::handleClassInterfaceSetup(arduino::USBSetup&)
 .text._ZN14USBDeviceClass6initEPEmm
                0x000000000000360c      0x10c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x000000000000360c                USBDeviceClass::initEP(unsigned long, unsigned long)
 .text._ZN14USBDeviceClass13initEndpointsEv
                0x0000000000003718       0x24 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000003718                USBDeviceClass::initEndpoints()
 .text._ZN14USBDeviceClass5clearEm
                0x000000000000373c       0x38 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x000000000000373c                USBDeviceClass::clear(unsigned long)
 .text._ZN14USBDeviceClass9availableEm
                0x0000000000003774       0x2c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000003774                USBDeviceClass::available(unsigned long)
 .text._ZN14USBDeviceClass5flushEm
                0x00000000000037a0       0x2c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x00000000000037a0                USBDeviceClass::flush(unsigned long)
 .text._ZN14USBDeviceClass4recvEmPvm
                0x00000000000037cc       0xc0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x00000000000037cc                USBDeviceClass::recv(unsigned long, void*, unsigned long)
 .text._ZN14USBDeviceClass4recvEm
                0x000000000000388c       0x1c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x000000000000388c                USBDeviceClass::recv(unsigned long)
 .text._ZN14USBDeviceClass14armRecvCtrlOUTEm
                0x00000000000038a8       0x5c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x00000000000038a8                USBDeviceClass::armRecvCtrlOUT(unsigned long)
 .text._ZN14USBDeviceClass11recvControlEPvm
                0x0000000000003904       0x28 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000003904                USBDeviceClass::recvControl(void*, unsigned long)
 .text._ZN14USBDeviceClass4sendEmPKvm
                0x000000000000392c      0x10c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x000000000000392c                USBDeviceClass::send(unsigned long, void const*, unsigned long)
 .text._ZN14USBDeviceClass7armSendEmPKvm
                0x0000000000003a38       0x48 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000003a38                USBDeviceClass::armSend(unsigned long, void const*, unsigned long)
 .text._ZN14USBDeviceClass11sendControlEPKvm
                0x0000000000003a80       0x54 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000003a80                USBDeviceClass::sendControl(void const*, unsigned long)
 .text._ZN14USBDeviceClass20sendStringDescriptorEPKhm
                0x0000000000003ad4       0x64 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000003ad4                USBDeviceClass::sendStringDescriptor(unsigned char const*, unsigned long)
 .text._ZN14USBDeviceClass17sendConfigurationEm
                0x0000000000003b38       0x80 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000003b38                USBDeviceClass::sendConfiguration(unsigned long)
 .text._ZN14USBDeviceClass14sendDescriptorERN7arduino8USBSetupE
                0x0000000000003bb8       0xd8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000003bb8                USBDeviceClass::sendDescriptor(arduino::USBSetup&)
 .text._ZN14USBDeviceClass7sendZlpEm
                0x0000000000003c90       0x18 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000003c90                USBDeviceClass::sendZlp(unsigned long)
 .text._ZN14USBDeviceClass19handleStandardSetupERN7arduino8USBSetupE
                0x0000000000003ca8       0xf0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000003ca8                USBDeviceClass::handleStandardSetup(arduino::USBSetup&)
 .text._ZN14USBDeviceClass10ISRHandlerEv
                0x0000000000003d98      0x108 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000003d98                USBDeviceClass::ISRHandler()
 .text.UDD_Handler
                0x0000000000003ea0       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000003ea0                UDD_Handler
 .text._ZN7arduino13PluggableUSB_C2Ev
                0x0000000000003eb0       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000003eb0                arduino::PluggableUSB_::PluggableUSB_()
                0x0000000000003eb0                arduino::PluggableUSB_::PluggableUSB_()
 .text._Z8epBufferj
                0x0000000000003ec0        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000003ec0                epBuffer(unsigned int)
 .text._ZN7arduino11RingBufferNILi64EE10store_charEh
                0x0000000000003ecc       0x1c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000003ecc                arduino::RingBufferN<64>::store_char(unsigned char)
 .text._ZN26DoubleBufferedEPOutHandler5_recvEv
                0x0000000000003ee8      0x15e /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000003ee8                DoubleBufferedEPOutHandler::_recv()
 .text._ZN26DoubleBufferedEPOutHandler9availableEv
                0x0000000000004046        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000004046                DoubleBufferedEPOutHandler::available()
 .text._ZN26DoubleBufferedEPOutHandler4peekEv
                0x0000000000004052       0x1c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000004052                DoubleBufferedEPOutHandler::peek()
 .text._ZN26DoubleBufferedEPOutHandler4recvEPvm
                0x000000000000406e       0x60 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x000000000000406e                DoubleBufferedEPOutHandler::recv(void*, unsigned long)
 *fill*         0x00000000000040ce        0x2 
 .text.startup._GLOBAL__sub_I_usbd
                0x00000000000040d0       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .text._ZN14USBDeviceClass4initEv
                0x00000000000040e0      0x15c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x00000000000040e0                USBDeviceClass::init()
 .text._ZN7arduino13PluggableUSB_12getInterfaceEPh
                0x000000000000423c       0x28 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
                0x000000000000423c                arduino::PluggableUSB_::getInterface(unsigned char*)
 .text._ZN7arduino13PluggableUSB_13getDescriptorERNS_8USBSetupE
                0x0000000000004264       0x20 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
                0x0000000000004264                arduino::PluggableUSB_::getDescriptor(arduino::USBSetup&)
 .text._ZN7arduino13PluggableUSB_12getShortNameEPc
                0x0000000000004284       0x1e /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
                0x0000000000004284                arduino::PluggableUSB_::getShortName(char*)
 .text._ZN7arduino13PluggableUSB_5setupERNS_8USBSetupE
                0x00000000000042a2       0x20 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
                0x00000000000042a2                arduino::PluggableUSB_::setup(arduino::USBSetup&)
 .text._ZN7arduino13PluggableUSB_4plugEPNS_18PluggableUSBModuleE
                0x00000000000042c2       0x5c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
                0x00000000000042c2                arduino::PluggableUSB_::plug(arduino::PluggableUSBModule*)
 *fill*         0x000000000000431e        0x2 
 .text._Z12PluggableUSBv
                0x0000000000004320       0x24 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
                0x0000000000004320                PluggableUSB()
 .text._Znwj    0x0000000000004344        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
                0x0000000000004344                operator new(unsigned int)
 .text._ZdlPv   0x000000000000434c        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
                0x000000000000434c                operator delete(void*)
 .text._ZN7Serial_13getDescriptorERN7arduino8USBSetupE
                0x0000000000004354        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x0000000000004354                Serial_::getDescriptor(arduino::USBSetup&)
 .text._ZL5utox8mPc
                0x0000000000004358       0x24 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
 .text._ZN7Serial_12getShortNameEPc
                0x000000000000437c       0x44 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x000000000000437c                Serial_::getShortName(char*)
 .text._ZThn16_N7Serial_12getShortNameEPc
                0x00000000000043c0       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x00000000000043c0                non-virtual thunk to Serial_::getShortName(char*)
 .text._ZN7Serial_5beginEm
                0x00000000000043d0        0x2 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x00000000000043d0                Serial_::begin(unsigned long)
 .text._ZN7Serial_5beginEmt
                0x00000000000043d2        0x2 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x00000000000043d2                Serial_::begin(unsigned long, unsigned short)
 .text._ZN7Serial_17availableForWriteEv
                0x00000000000043d4        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x00000000000043d4                Serial_::availableForWrite()
 .text._ZN7Serial_5writeEh
                0x00000000000043d8       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x00000000000043d8                Serial_::write(unsigned char)
 .text._ZN7Serial_12getInterfaceEPh
                0x00000000000043ec      0x11c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x00000000000043ec                Serial_::getInterface(unsigned char*)
 .text._ZThn16_N7Serial_12getInterfaceEPh
                0x0000000000004508       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x0000000000004508                non-virtual thunk to Serial_::getInterface(unsigned char*)
 .text._ZN7Serial_5setupERN7arduino8USBSetupE
                0x0000000000004518       0x98 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x0000000000004518                Serial_::setup(arduino::USBSetup&)
 .text._ZThn16_N7Serial_5setupERN7arduino8USBSetupE
                0x00000000000045b0       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x00000000000045b0                non-virtual thunk to Serial_::setup(arduino::USBSetup&)
 .text._ZN7Serial_3endEv
                0x00000000000045c0       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x00000000000045c0                Serial_::end()
 .text._ZN7Serial_9availableEv
                0x00000000000045d4       0x20 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x00000000000045d4                Serial_::available()
 .text._ZN7Serial_5flushEv
                0x00000000000045f4        0xe /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x00000000000045f4                Serial_::flush()
 .text._ZN7Serial_5clearEv
                0x0000000000004602        0xe /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x0000000000004602                Serial_::clear()
 .text._ZN7Serial_5writeEPKhj
                0x0000000000004610       0x1e /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x0000000000004610                Serial_::write(unsigned char const*, unsigned int)
 *fill*         0x000000000000462e        0x2 
 .text._ZN7Serial_4peekEv
                0x0000000000004630       0x1c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x0000000000004630                Serial_::peek()
 .text._ZN7Serial_4readEv
                0x000000000000464c       0x24 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x000000000000464c                Serial_::read()
 .text._ZN7Serial_cvbEv
                0x0000000000004670       0x28 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x0000000000004670                Serial_::operator bool()
 .text._ZThn16_N7Serial_13getDescriptorERN7arduino8USBSetupE
                0x0000000000004698        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x0000000000004698                non-virtual thunk to Serial_::getDescriptor(arduino::USBSetup&)
 .text._ZN7Serial_14handleEndpointEi
                0x000000000000469c        0x2 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x000000000000469c                Serial_::handleEndpoint(int)
 *fill*         0x000000000000469e        0x2 
 .text._ZN7Serial_C2ER14USBDeviceClass
                0x00000000000046a0       0x50 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x00000000000046a0                Serial_::Serial_(USBDeviceClass&)
                0x00000000000046a0                Serial_::Serial_(USBDeviceClass&)
 .text._ZN7Serial_15enableInterruptEv
                0x00000000000046f0       0x30 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x00000000000046f0                Serial_::enableInterrupt()
 .text.startup._GLOBAL__sub_I__ZN7Serial_12getInterfaceEPh
                0x0000000000004720       0x14 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
 .text          0x0000000000004734       0x14 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_thumb1_case_uqi.o)
                0x0000000000004734                __gnu_thumb1_case_uqi
 .text          0x0000000000004748      0x114 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivsi3.o)
                0x0000000000004748                __udivsi3
                0x0000000000004748                __aeabi_uidiv
                0x0000000000004854                __aeabi_uidivmod
 .text          0x000000000000485c        0x4 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_dvmd_tls.o)
                0x000000000000485c                __aeabi_ldiv0
                0x000000000000485c                __aeabi_idiv0
 .text.__libc_init_array
                0x0000000000004860       0x48 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-init.o)
                0x0000000000004860                __libc_init_array
 .text.malloc   0x00000000000048a8       0x14 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-malloc.o)
                0x00000000000048a8                malloc
 .text.free     0x00000000000048bc       0x14 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-malloc.o)
                0x00000000000048bc                free
 .text.memcpy   0x00000000000048d0       0x12 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-memcpy-stub.o)
                0x00000000000048d0                memcpy
 .text.memset   0x00000000000048e2       0x10 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-memset.o)
                0x00000000000048e2                memset
 *fill*         0x00000000000048f2        0x2 
 .text._free_r  0x00000000000048f4       0x94 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-freer.o)
                0x00000000000048f4                _free_r
 .text._malloc_r
                0x0000000000004988       0xbc /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-mallocr.o)
                0x0000000000004988                _malloc_r
 .text._sbrk_r  0x0000000000004a44       0x24 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-sbrkr.o)
                0x0000000000004a44                _sbrk_r
 .text          0x0000000000004a68        0xe /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-strlen.o)
                0x0000000000004a68                strlen
 .text.__malloc_lock
                0x0000000000004a76        0x2 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-mlock.o)
                0x0000000000004a76                __malloc_lock
 .text.__malloc_unlock
                0x0000000000004a78        0x2 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-mlock.o)
                0x0000000000004a78                __malloc_unlock
 *fill*         0x0000000000004a7a        0x2 
 .text._sbrk    0x0000000000004a7c       0x1c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a(sbrk.o)
                0x0000000000004a7c                _sbrk
 *(.init)
 .init          0x0000000000004a98        0x4 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crti.o
                0x0000000000004a98                _init
 .init          0x0000000000004a9c        0x8 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtn.o
 *(.fini)
 .fini          0x0000000000004aa4        0x4 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crti.o
                0x0000000000004aa4                _fini
 .fini          0x0000000000004aa8        0x8 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtn.o
 *crtbegin.o(.ctors)
 *crtbegin?.o(.ctors)
 *(EXCLUDE_FILE(*crtend.o *crtend?.o) .ctors)
 *(SORT_BY_NAME(.ctors.*))
 *(.ctors)
 *crtbegin.o(.dtors)
 *crtbegin?.o(.dtors)
 *(EXCLUDE_FILE(*crtend.o *crtend?.o) .dtors)
 *(SORT_BY_NAME(.dtors.*))
 *(.dtors)
 *(.rodata*)
 .rodata.g_APinDescription
                0x0000000000004ab0      0x360 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
                0x0000000000004ab0                g_APinDescription
 .rodata._ZTV4Uart
                0x0000000000004e10       0x34 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                0x0000000000004e10                vtable for Uart
 .rodata._ZTV26DoubleBufferedEPOutHandler
                0x0000000000004e44       0x24 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000000004e44                vtable for DoubleBufferedEPOutHandler
 .rodata._ZL14STRING_PRODUCT
                0x0000000000004e68       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .rodata._ZL15STRING_LANGUAGE
                0x0000000000004e78        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .rodata._ZL19STRING_MANUFACTURER
                0x0000000000004e7c        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .rodata._ZL21USB_DeviceDescriptorB
                0x0000000000004e88       0x12 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 *fill*         0x0000000000004e9a        0x2 
 .rodata._ZTV7Serial_
                0x0000000000004e9c       0x60 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x0000000000004e9c                vtable for Serial_
 *(.eh_frame*)
 .eh_frame      0x0000000000004efc        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtbegin.o
 .eh_frame      0x0000000000004efc        0x4 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtend.o

.glue_7         0x0000000000004f00        0x0
 .glue_7        0x0000000000004f00        0x0 linker stubs

.glue_7t        0x0000000000004f00        0x0
 .glue_7t       0x0000000000004f00        0x0 linker stubs

.vfp11_veneer   0x0000000000004f00        0x0
 .vfp11_veneer  0x0000000000004f00        0x0 linker stubs

.v4_bx          0x0000000000004f00        0x0
 .v4_bx         0x0000000000004f00        0x0 linker stubs

.iplt           0x0000000000004f00        0x0
 .iplt          0x0000000000004f00        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtbegin.o

.rel.dyn        0x0000000000004f00        0x0
 .rel.iplt      0x0000000000004f00        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtbegin.o

.ARM.extab
 *(.ARM.extab* .gnu.linkonce.armextab.*)
                0x0000000000004f00                __exidx_start = .

.ARM.exidx
 *(.ARM.exidx* .gnu.linkonce.armexidx.*)
                0x0000000000004f00                __exidx_end = .
                0x0000000000004f00                __etext = .

.data           0x0000000020000000       0xa0 load address 0x0000000000004f00
                0x0000000020000000                __data_start__ = .
 *(vtable)
 *(.data*)
 .data.photoDiode
                0x0000000020000000        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
                0x0000000020000000                photoDiode
 .data.SystemCoreClock
                0x0000000020000004        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
                0x0000000020000004                SystemCoreClock
 .data._ADCResolution
                0x0000000020000008        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .data._readResolution
                0x000000002000000c        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .data._ZL5ticks
                0x0000000020000010        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
 .data._ZL10breakValue
                0x0000000020000014        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
 .data._ZL12_usbLineInfo
                0x0000000020000018        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
 .data._serialPeek
                0x0000000020000020        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x0000000020000020                _serialPeek
 .data._impure_ptr
                0x0000000020000024        0x4 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-impure.o)
                0x0000000020000024                _impure_ptr
 .data.impure_data
                0x0000000020000028       0x60 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-impure.o)
                0x0000000020000088                . = ALIGN (0x4)
                0x0000000020000088                PROVIDE (__preinit_array_start, .)
 *(.preinit_array)
                0x0000000020000088                PROVIDE (__preinit_array_end, .)
                0x0000000020000088                . = ALIGN (0x4)
                0x0000000020000088                PROVIDE (__init_array_start, .)
 *(SORT_BY_NAME(.init_array.*))
 *(.init_array)
 .init_array    0x0000000020000088        0x4 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtbegin.o
 .init_array    0x000000002000008c        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
 .init_array    0x0000000020000090        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
 .init_array    0x0000000020000094        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .init_array    0x0000000020000098        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x000000002000009c                PROVIDE (__init_array_end, .)
                0x000000002000009c                . = ALIGN (0x4)
                [!provide]                        PROVIDE (__fini_array_start, .)
 *(SORT_BY_NAME(.fini_array.*))
 *(.fini_array)
 .fini_array    0x000000002000009c        0x4 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtbegin.o
                [!provide]                        PROVIDE (__fini_array_end, .)
 *(.jcr*)
                0x00000000200000a0                . = ALIGN (0x10)
                0x00000000200000a0                __data_end__ = .

.igot.plt       0x00000000200000a0        0x0 load address 0x0000000000004fa0
 .igot.plt      0x00000000200000a0        0x0 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtbegin.o

.bss            0x00000000200000a0      0x93c load address 0x0000000000004fa0
                0x00000000200000a0                . = ALIGN (0x4)
                0x00000000200000a0                __bss_start__ = .
 *(.bss*)
 .bss           0x00000000200000a0       0x1c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtbegin.o
 .bss.blind     0x00000000200000bc        0x3 /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
                0x00000000200000bc                blind
 *fill*         0x00000000200000bf        0x1 
 .bss.pdValue   0x00000000200000c0        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
                0x00000000200000c0                pdValue
 .bss.ServoCount
                0x00000000200000c4        0x1 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
                0x00000000200000c4                ServoCount
 .bss._ZL17currentServoIndex
                0x00000000200000c5        0x1 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 *fill*         0x00000000200000c6        0x2 
 .bss._ZL6servos
                0x00000000200000c8       0x60 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 .bss.Serial1   0x0000000020000128      0x244 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
                0x0000000020000128                Serial1
 .bss.sercom0   0x000000002000036c        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
                0x000000002000036c                sercom0
 .bss.sercom1   0x0000000020000374        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
                0x0000000020000374                sercom1
 .bss.sercom2   0x000000002000037c        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
                0x000000002000037c                sercom2
 .bss.sercom3   0x0000000020000384        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
                0x0000000020000384                sercom3
 .bss.sercom4   0x000000002000038c        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
                0x000000002000038c                sercom4
 .bss.sercom5   0x0000000020000394        0x8 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
                0x0000000020000394                sercom5
 .bss.usb_isr   0x000000002000039c        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
 .bss._ulTickCount
                0x00000000200003a0        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
 .bss.EndPoints
                0x00000000200003a4       0x28 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x00000000200003a4                EndPoints
 .bss.USBDevice
                0x00000000200003cc        0x1 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x00000000200003cc                USBDevice
 *fill*         0x00000000200003cd        0x3 
 .bss._ZL10epHandlers
                0x00000000200003d0       0x1c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .bss._ZL14isEndpointHalt
                0x00000000200003ec        0x1 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .bss._ZL20LastTransmitTimedOut
                0x00000000200003ed        0x7 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .bss._ZL21isRemoteWakeUpEnabled
                0x00000000200003f4        0x1 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 *fill*         0x00000000200003f5        0x3 
 .bss._ZL22udd_ep_in_cache_buffer
                0x00000000200003f8      0x1c0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .bss._ZL23udd_ep_out_cache_buffer
                0x00000000200005b8      0x1c0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .bss._dry_run  0x0000000020000778        0x1 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000020000778                _dry_run
 .bss._pack_buffer
                0x0000000020000779      0x100 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000020000779                _pack_buffer
 .bss._pack_message
                0x0000000020000879        0x1 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000020000879                _pack_message
 .bss._pack_size
                0x000000002000087a        0x2 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x000000002000087a                _pack_size
 .bss._usbConfiguration
                0x000000002000087c        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x000000002000087c                _usbConfiguration
 .bss._usbSetInterface
                0x0000000020000880        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000020000880                _usbSetInterface
 .bss.usbd      0x0000000020000884      0x104 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                0x0000000020000884                usbd
 .bss._ZGVZ12PluggableUSBvE3obj
                0x0000000020000988        0x4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
 .bss._ZZ12PluggableUSBvE3obj
                0x000000002000098c        0xc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
 .bss.SerialUSB
                0x0000000020000998       0x34 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                0x0000000020000998                SerialUSB
 .bss.__malloc_free_list
                0x00000000200009cc        0x4 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-mallocr.o)
                0x00000000200009cc                __malloc_free_list
 .bss.__malloc_sbrk_start
                0x00000000200009d0        0x4 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-mallocr.o)
                0x00000000200009d0                __malloc_sbrk_start
 .bss.heap_end.4102
                0x00000000200009d4        0x4 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a(sbrk.o)
 *(COMMON)
 COMMON         0x00000000200009d8        0x4 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-reent.o)
                0x00000000200009d8                errno
                0x00000000200009dc                . = ALIGN (0x4)
                0x00000000200009dc                __bss_end__ = .

.heap           0x00000000200009dc        0x0
                0x00000000200009dc                __end__ = .
                0x00000000200009dc                PROVIDE (end, .)
 *(.heap*)
                0x00000000200009dc                __HeapLimit = .

.stack_dummy    0x00000000200009dc        0x0
 *(.stack*)
                0x0000000020008000                __StackTop = (ORIGIN (RAM) + LENGTH (RAM))
                0x0000000020008000                __StackLimit = (__StackTop - SIZEOF (.stack_dummy))
                0x0000000020008000                PROVIDE (__stack, __StackTop)
                0x0000000020007fff                __ram_end__ = ((ORIGIN (RAM) + LENGTH (RAM)) - 0x1)
                0x0000000000000001                ASSERT ((__StackLimit >= __HeapLimit), region RAM overflowed with stack)
OUTPUT(/Users/nico/Documents/GitHub/blinds-controller/build/blinds-controller.ino.elf elf32-littlearm)

.ARM.attributes
                0x0000000000000000       0x28
 .ARM.attributes
                0x0000000000000000       0x1e /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crti.o
 .ARM.attributes
                0x000000000000001e       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtbegin.o
 .ARM.attributes
                0x000000000000004a       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
 .ARM.attributes
                0x000000000000007c       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 .ARM.attributes
                0x00000000000000ae       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
 .ARM.attributes
                0x00000000000000e0       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
 .ARM.attributes
                0x0000000000000112       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
 .ARM.attributes
                0x0000000000000144       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
 .ARM.attributes
                0x0000000000000176       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(startup.c.o)
 .ARM.attributes
                0x00000000000001a8       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
 .ARM.attributes
                0x00000000000001da       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .ARM.attributes
                0x000000000000020c       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
 .ARM.attributes
                0x000000000000023e       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_private.c.o)
 .ARM.attributes
                0x0000000000000270       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
 .ARM.attributes
                0x00000000000002a2       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .ARM.attributes
                0x00000000000002d4       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
 .ARM.attributes
                0x0000000000000306       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .ARM.attributes
                0x0000000000000338       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
 .ARM.attributes
                0x000000000000036a       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .ARM.attributes
                0x000000000000039c       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
 .ARM.attributes
                0x00000000000003ce       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
 .ARM.attributes
                0x0000000000000400       0x32 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
 .ARM.attributes
                0x0000000000000432       0x1e /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_thumb1_case_uqi.o)
 .ARM.attributes
                0x0000000000000450       0x1e /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivsi3.o)
 .ARM.attributes
                0x000000000000046e       0x1e /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_dvmd_tls.o)
 .ARM.attributes
                0x000000000000048c       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-impure.o)
 .ARM.attributes
                0x00000000000004b8       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-init.o)
 .ARM.attributes
                0x00000000000004e4       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-malloc.o)
 .ARM.attributes
                0x0000000000000510       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-memcpy-stub.o)
 .ARM.attributes
                0x000000000000053c       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-memset.o)
 .ARM.attributes
                0x0000000000000568       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-freer.o)
 .ARM.attributes
                0x0000000000000594       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-mallocr.o)
 .ARM.attributes
                0x00000000000005c0       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-sbrkr.o)
 .ARM.attributes
                0x00000000000005ec       0x1c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-strlen.o)
 .ARM.attributes
                0x0000000000000608       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-mlock.o)
 .ARM.attributes
                0x0000000000000634       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-reent.o)
 .ARM.attributes
                0x0000000000000660       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a(sbrk.o)
 .ARM.attributes
                0x000000000000068c       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtend.o
 .ARM.attributes
                0x00000000000006b8       0x1e /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtn.o

.comment        0x0000000000000000       0x7e
 .comment       0x0000000000000000       0x7e /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
                                         0x7f (size before relaxing)
 .comment       0x000000000000007e       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 .comment       0x000000000000007e       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
 .comment       0x000000000000007e       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
 .comment       0x000000000000007e       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
 .comment       0x000000000000007e       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
 .comment       0x000000000000007e       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(startup.c.o)
 .comment       0x000000000000007e       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
 .comment       0x000000000000007e       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .comment       0x000000000000007e       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
 .comment       0x000000000000007e       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_private.c.o)
 .comment       0x000000000000007e       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
 .comment       0x000000000000007e       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .comment       0x000000000000007e       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
 .comment       0x000000000000007e       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .comment       0x000000000000007e       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
 .comment       0x000000000000007e       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .comment       0x000000000000007e       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
 .comment       0x000000000000007e       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
 .comment       0x000000000000007e       0x7f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)

.debug_info     0x0000000000000000    0x5d98b
 .debug_info    0x0000000000000000     0x6058 /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
 .debug_info    0x0000000000006058     0x77a3 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 .debug_info    0x000000000000d7fb     0x77e7 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
 .debug_info    0x0000000000014fe2     0x1101 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
 .debug_info    0x00000000000160e3     0x13c7 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
 .debug_info    0x00000000000174aa       0x64 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
 .debug_info    0x000000000001750e     0x34c3 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(startup.c.o)
 .debug_info    0x000000000001a9d1     0x2d8f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
 .debug_info    0x000000000001d760     0x4f58 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .debug_info    0x00000000000226b8     0x1862 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
 .debug_info    0x0000000000023f1a     0x17ec /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_private.c.o)
 .debug_info    0x0000000000025706     0x640a /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
 .debug_info    0x000000000002bb10     0x731b /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .debug_info    0x0000000000032e2b     0x7f9d /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
 .debug_info    0x000000000003adc8     0x41d3 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .debug_info    0x000000000003ef9b     0x5e44 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
 .debug_info    0x0000000000044ddf     0xdab0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .debug_info    0x000000000005288f      0x686 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
 .debug_info    0x0000000000052f15      0xf3b /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
 .debug_info    0x0000000000053e50     0x9b3b /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)

.debug_abbrev   0x0000000000000000     0x6d59
 .debug_abbrev  0x0000000000000000      0x637 /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
 .debug_abbrev  0x0000000000000637      0x855 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 .debug_abbrev  0x0000000000000e8c      0x617 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
 .debug_abbrev  0x00000000000014a3      0x29a /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
 .debug_abbrev  0x000000000000173d      0x33c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
 .debug_abbrev  0x0000000000001a79       0x49 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
 .debug_abbrev  0x0000000000001ac2      0x2ac /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(startup.c.o)
 .debug_abbrev  0x0000000000001d6e      0x3a1 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
 .debug_abbrev  0x000000000000210f      0x487 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .debug_abbrev  0x0000000000002596      0x339 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
 .debug_abbrev  0x00000000000028cf      0x303 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_private.c.o)
 .debug_abbrev  0x0000000000002bd2      0x671 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
 .debug_abbrev  0x0000000000003243      0x836 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .debug_abbrev  0x0000000000003a79      0x913 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
 .debug_abbrev  0x000000000000438c      0x709 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .debug_abbrev  0x0000000000004a95      0x5dd /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
 .debug_abbrev  0x0000000000005072      0xc7b /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .debug_abbrev  0x0000000000005ced      0x2b2 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
 .debug_abbrev  0x0000000000005f9f      0x301 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
 .debug_abbrev  0x00000000000062a0      0xab9 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)

.debug_loc      0x0000000000000000     0x71e8
 .debug_loc     0x0000000000000000       0x2a /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
 .debug_loc     0x000000000000002a      0x53a /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 .debug_loc     0x0000000000000564       0x2a /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
 .debug_loc     0x000000000000058e       0x3c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
 .debug_loc     0x00000000000005ca      0x12f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
 .debug_loc     0x00000000000006f9       0x2e /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(startup.c.o)
 .debug_loc     0x0000000000000727       0xa0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
 .debug_loc     0x00000000000007c7      0x4b9 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .debug_loc     0x0000000000000c80       0xc0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
 .debug_loc     0x0000000000000d40      0x131 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_private.c.o)
 .debug_loc     0x0000000000000e71       0x2d /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
 .debug_loc     0x0000000000000e9e      0xb3f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .debug_loc     0x00000000000019dd      0xb0f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
 .debug_loc     0x00000000000024ec     0x1a81 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .debug_loc     0x0000000000003f6d     0x27c7 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .debug_loc     0x0000000000006734      0x256 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
 .debug_loc     0x000000000000698a       0x42 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
 .debug_loc     0x00000000000069cc      0x81c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)

.debug_aranges  0x0000000000000000      0x9c8
 .debug_aranges
                0x0000000000000000       0x40 /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
 .debug_aranges
                0x0000000000000040       0x70 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 .debug_aranges
                0x00000000000000b0       0x30 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
 .debug_aranges
                0x00000000000000e0       0x40 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
 .debug_aranges
                0x0000000000000120       0x48 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
 .debug_aranges
                0x0000000000000168       0x30 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
 .debug_aranges
                0x0000000000000198       0x20 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(startup.c.o)
 .debug_aranges
                0x00000000000001b8       0x20 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
 .debug_aranges
                0x00000000000001d8       0x48 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .debug_aranges
                0x0000000000000220       0x30 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
 .debug_aranges
                0x0000000000000250       0x20 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_private.c.o)
 .debug_aranges
                0x0000000000000270       0x38 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
 .debug_aranges
                0x00000000000002a8      0x1f0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .debug_aranges
                0x0000000000000498       0xb8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
 .debug_aranges
                0x0000000000000550      0x130 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .debug_aranges
                0x0000000000000680       0x28 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
 .debug_aranges
                0x00000000000006a8      0x190 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .debug_aranges
                0x0000000000000838       0x48 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
 .debug_aranges
                0x0000000000000880       0x28 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
 .debug_aranges
                0x00000000000008a8      0x120 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)

.debug_ranges   0x0000000000000000     0x1480
 .debug_ranges  0x0000000000000000       0x30 /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
 .debug_ranges  0x0000000000000030       0xd8 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 .debug_ranges  0x0000000000000108       0x20 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
 .debug_ranges  0x0000000000000128       0x30 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
 .debug_ranges  0x0000000000000158       0x38 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
 .debug_ranges  0x0000000000000190       0x20 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
 .debug_ranges  0x00000000000001b0       0x10 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(startup.c.o)
 .debug_ranges  0x00000000000001c0       0x28 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
 .debug_ranges  0x00000000000001e8       0x98 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .debug_ranges  0x0000000000000280       0x20 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
 .debug_ranges  0x00000000000002a0       0x38 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_private.c.o)
 .debug_ranges  0x00000000000002d8       0x40 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
 .debug_ranges  0x0000000000000318      0x2a0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .debug_ranges  0x00000000000005b8      0x238 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
 .debug_ranges  0x00000000000007f0      0x198 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .debug_ranges  0x0000000000000988       0x18 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
 .debug_ranges  0x00000000000009a0      0x8b0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .debug_ranges  0x0000000000001250       0x68 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
 .debug_ranges  0x00000000000012b8       0x18 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
 .debug_ranges  0x00000000000012d0      0x1b0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)

.debug_line     0x0000000000000000     0x900a
 .debug_line    0x0000000000000000      0x7b6 /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
 .debug_line    0x00000000000007b6      0x943 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 .debug_line    0x00000000000010f9      0x61f /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
 .debug_line    0x0000000000001718      0x39b /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
 .debug_line    0x0000000000001ab3      0x5f0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
 .debug_line    0x00000000000020a3       0xa9 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
 .debug_line    0x000000000000214c      0x470 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(startup.c.o)
 .debug_line    0x00000000000025bc      0x5de /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
 .debug_line    0x0000000000002b9a      0x6f5 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .debug_line    0x000000000000328f      0x54c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
 .debug_line    0x00000000000037db      0x534 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_private.c.o)
 .debug_line    0x0000000000003d0f      0x7c1 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
 .debug_line    0x00000000000044d0      0xd1d /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .debug_line    0x00000000000051ed      0xafd /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
 .debug_line    0x0000000000005cea      0x822 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .debug_line    0x000000000000650c      0x6f6 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
 .debug_line    0x0000000000006c02     0x1321 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .debug_line    0x0000000000007f23      0x29d /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
 .debug_line    0x00000000000081c0      0x34c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
 .debug_line    0x000000000000850c      0xafe /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)

.debug_str      0x0000000000000000     0xaa59
 .debug_str     0x0000000000000000     0x40f1 /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
                                       0x4977 (size before relaxing)
 .debug_str     0x00000000000040f1      0x701 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
                                       0x51c1 (size before relaxing)
 .debug_str     0x00000000000047f2      0x6ce /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
                                       0x4920 (size before relaxing)
 .debug_str     0x0000000000004ec0      0x4b8 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
                                        0xf95 (size before relaxing)
 .debug_str     0x0000000000005378       0xeb /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
                                        0xec0 (size before relaxing)
 .debug_str     0x0000000000005463       0x71 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
                                        0x15f (size before relaxing)
 .debug_str     0x00000000000054d4      0x829 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(startup.c.o)
                                       0x16d2 (size before relaxing)
 .debug_str     0x0000000000005cfd      0x19e /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
                                       0x179d (size before relaxing)
 .debug_str     0x0000000000005e9b      0x174 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
                                       0x1c1c (size before relaxing)
 .debug_str     0x000000000000600f      0x109 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
                                        0xffe (size before relaxing)
 .debug_str     0x0000000000006118       0x75 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_private.c.o)
                                        0xfb3 (size before relaxing)
 .debug_str     0x000000000000618d      0x1a6 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
                                       0x4a63 (size before relaxing)
 .debug_str     0x0000000000006333      0x1c7 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                       0x4c7e (size before relaxing)
 .debug_str     0x00000000000064fa      0xab0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                                       0x56f1 (size before relaxing)
 .debug_str     0x0000000000006faa      0x5e9 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
                                       0x1dd7 (size before relaxing)
 .debug_str     0x0000000000007593       0xa6 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
                                       0x4808 (size before relaxing)
 .debug_str     0x0000000000007639     0x2c8f /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                       0x82d7 (size before relaxing)
 .debug_str     0x000000000000a2c8       0x86 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
                                        0x63b (size before relaxing)
 .debug_str     0x000000000000a34e       0x8a /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
                                        0x7b0 (size before relaxing)
 .debug_str     0x000000000000a3d8      0x681 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                                       0x7aa3 (size before relaxing)

.debug_frame    0x0000000000000000     0x1a50
 .debug_frame   0x0000000000000000       0x88 /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
 .debug_frame   0x0000000000000088      0x138 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
 .debug_frame   0x00000000000001c0       0x54 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
 .debug_frame   0x0000000000000214       0x7c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
 .debug_frame   0x0000000000000290       0xa0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
 .debug_frame   0x0000000000000330       0x40 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
 .debug_frame   0x0000000000000370       0x2c /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(startup.c.o)
 .debug_frame   0x000000000000039c       0x28 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
 .debug_frame   0x00000000000003c4       0x90 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
 .debug_frame   0x0000000000000454       0x64 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
 .debug_frame   0x00000000000004b8       0x30 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_private.c.o)
 .debug_frame   0x00000000000004e8       0x60 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
 .debug_frame   0x0000000000000548      0x478 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
 .debug_frame   0x00000000000009c0      0x1e4 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
 .debug_frame   0x0000000000000ba4      0x3cc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
 .debug_frame   0x0000000000000f70       0x38 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
 .debug_frame   0x0000000000000fa8      0x4b0 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
 .debug_frame   0x0000000000001458       0xbc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
 .debug_frame   0x0000000000001514       0x70 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
 .debug_frame   0x0000000000001584      0x2dc /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
 .debug_frame   0x0000000000001860       0x20 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivsi3.o)
 .debug_frame   0x0000000000001880       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-init.o)
 .debug_frame   0x00000000000018ac       0x40 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-malloc.o)
 .debug_frame   0x00000000000018ec       0x28 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-memcpy-stub.o)
 .debug_frame   0x0000000000001914       0x20 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-memset.o)
 .debug_frame   0x0000000000001934       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-freer.o)
 .debug_frame   0x0000000000001960       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-mallocr.o)
 .debug_frame   0x000000000000198c       0x2c /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-sbrkr.o)
 .debug_frame   0x00000000000019b8       0x30 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-mlock.o)
 .debug_frame   0x00000000000019e8       0x48 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-reent.o)
 .debug_frame   0x0000000000001a30       0x20 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a(sbrk.o)

Cross Reference Table

Symbol                                            File
AC_Handler                                        /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
ADC_Handler                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
DAC_Handler                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
DMAC_Handler                                      /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
DoubleBufferedEPOutHandler::_available() const    /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
DoubleBufferedEPOutHandler::_recv()               /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
DoubleBufferedEPOutHandler::available()           /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
DoubleBufferedEPOutHandler::handleEndpoint()      /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
DoubleBufferedEPOutHandler::peek()                /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
DoubleBufferedEPOutHandler::recv(void*, unsigned long) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
DoubleBufferedEPOutHandler::release()             /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
DoubleBufferedEPOutHandler::~DoubleBufferedEPOutHandler() /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
DoubleBufferedEPOutHandler::~DoubleBufferedEPOutHandler() /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
DoubleBufferedEPOutHandler::~DoubleBufferedEPOutHandler() /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
Dummy_Handler                                     /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
EIC_Handler                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
EVSYS_Handler                                     /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
EndPoints                                         /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
HardFault_Handler                                 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
I2S_Handler                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
NMI_Handler                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
NVMCTRL_Handler                                   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
PINCOUNT_fn                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
PM_Handler                                        /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
PTC_Handler                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
PendSV_Handler                                    /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
PluggableUSB()                                    /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
RTC_Handler                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
Reset_Handler                                     /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
SERCOM0_Handler                                   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
SERCOM1_Handler                                   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
SERCOM2_Handler                                   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
SERCOM3_Handler                                   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
SERCOM4_Handler                                   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
SERCOM5_Handler                                   /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
SERCOM::SERCOM(Sercom*)                           /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
SERCOM::SERCOM(Sercom*)                           /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::acknowledgeUARTError()                    /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
SERCOM::availableDataUART()                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
SERCOM::availableWIRE()                           /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::calculateBaudrateSynchronous(unsigned long) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::clearFrameErrorUART()                     /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
SERCOM::clearStatusUART()                         /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
SERCOM::disableDataRegisterEmptyInterruptUART()   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
SERCOM::disableSPI()                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::disableWIRE()                             /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::enableDataRegisterEmptyInterruptUART()    /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
SERCOM::enableSPI()                               /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::enableUART()                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
SERCOM::enableWIRE()                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::flushUART()                               /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
SERCOM::getDataOrderSPI()                         /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::initClockNVIC()                           /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::initFrame(SercomUartCharSize, SercomDataOrder, SercomParityMode, SercomNumberStopBit) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
SERCOM::initMasterWIRE(unsigned long)             /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::initPads(SercomUartTXPad, SercomRXPad)    /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
SERCOM::initSPI(SercomSpiTXPad, SercomRXPad, SercomSpiCharSize, SercomDataOrder) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::initSPIClock(SercomSpiClockMode, unsigned long) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::initSlaveWIRE(unsigned char, bool)        /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::initUART(SercomUartMode, SercomUartSampleRate, unsigned long) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
SERCOM::isAddressMatch()                          /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::isArbLostWIRE()                           /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::isBufferOverflowErrorSPI()                /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::isBufferOverflowErrorUART()               /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::isBusBusyWIRE()                           /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::isBusIdleWIRE()                           /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::isBusOwnerWIRE()                          /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::isDataReadyWIRE()                         /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::isDataRegisterEmptySPI()                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::isDataRegisterEmptyUART()                 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
SERCOM::isFrameErrorUART()                        /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
SERCOM::isMasterReadOperationWIRE()               /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::isMasterWIRE()                            /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::isParityErrorUART()                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::isRXNackReceivedWIRE()                    /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::isRestartDetectedWIRE()                   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::isSlaveWIRE()                             /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::isStopDetectedWIRE()                      /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::isUARTError()                             /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
SERCOM::prepareAckBitWIRE()                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::prepareCommandBitsWire(unsigned char)     /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::prepareNackBitWIRE()                      /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::readDataUART()                            /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
SERCOM::readDataWIRE()                            /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::resetSPI()                                /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::resetUART()                               /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
SERCOM::resetWIRE()                               /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::sendDataMasterWIRE(unsigned char)         /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::sendDataSlaveWIRE(unsigned char)          /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::setBaudrateSPI(unsigned char)             /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::setClockModeSPI(SercomSpiClockMode)       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::setDataOrderSPI(SercomDataOrder)          /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::startTransmissionWIRE(unsigned char, SercomWireReadWriteFlag) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::transferDataSPI(unsigned char)            /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
SERCOM::writeDataUART(unsigned char)              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
SVC_Handler                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
SYSCTRL_Handler                                   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
Serial1                                           /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
SerialUSB                                         /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
Serial_::Serial_(USBDeviceClass&)                 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::Serial_(USBDeviceClass&)                 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::available()                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::availableForWrite()                      /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::baud()                                   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::begin(unsigned long)                     /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
Serial_::begin(unsigned long, unsigned short)     /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::clear()                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::dtr()                                    /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::enableInterrupt()                        /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
Serial_::end()                                    /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::flush()                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::getDescriptor(arduino::USBSetup&)        /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::getInterface(unsigned char*)             /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::getShortName(char*)                      /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::handleEndpoint(int)                      /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
Serial_::numbits()                                /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::operator bool()                          /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::paritytype()                             /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::peek()                                   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::read()                                   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::readBreak()                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::readBytes(char*, unsigned int)           /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::rts()                                    /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::setup(arduino::USBSetup&)                /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::stopbits()                               /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::write(unsigned char const*, unsigned int) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Serial_::write(unsigned char)                     /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
Servo::Servo()                                    /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
Servo::Servo()                                    /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
Servo::attach(int)                                /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
Servo::attach(int, int, int)                      /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
Servo::attached()                                 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
Servo::detach()                                   /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
Servo::read()                                     /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
Servo::readMicroseconds()                         /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
Servo::write(int)                                 /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
Servo::writeMicroseconds(int)                     /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
ServoCount                                        /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
Servo_Handler(timer16_Sequence_t, Tc*, unsigned char, unsigned char) /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
SysTick_DefaultHandler                            /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
SysTick_Handler                                   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
SystemCoreClock                                   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(startup.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
SystemInit                                        /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(startup.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
TC3_Handler                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
TC4_Handler                                       /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
TC5_Handler                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
TC6_Handler                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
TC7_Handler                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
TCC0_Handler                                      /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
TCC1_Handler                                      /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
TCC2_Handler                                      /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
UDD_Handler                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USBDevice                                         /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
USBDeviceClass::ISRHandler()                      /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USBDeviceClass::SendInterfaces(unsigned long*)    /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USBDeviceClass::armRecvCtrlOUT(unsigned long)     /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USBDeviceClass::armSend(unsigned long, void const*, unsigned long) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USBDeviceClass::attach()                          /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
USBDeviceClass::available(unsigned long)          /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
USBDeviceClass::clear(unsigned long)              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
USBDeviceClass::configured()                      /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USBDeviceClass::connected()                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USBDeviceClass::detach()                          /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USBDeviceClass::end()                             /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USBDeviceClass::flush(unsigned long)              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
USBDeviceClass::handleClassInterfaceSetup(arduino::USBSetup&) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USBDeviceClass::handleStandardSetup(arduino::USBSetup&) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USBDeviceClass::init()                            /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
USBDeviceClass::initEP(unsigned long, unsigned long) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USBDeviceClass::initEndpoints()                   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USBDeviceClass::packMessages(bool)                /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USBDeviceClass::recv(unsigned long)               /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
USBDeviceClass::recv(unsigned long, void*, unsigned long) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
USBDeviceClass::recvControl(void*, unsigned long) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
USBDeviceClass::send(unsigned long, void const*, unsigned long) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
USBDeviceClass::sendConfiguration(unsigned long)  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USBDeviceClass::sendControl(void const*, unsigned long) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
USBDeviceClass::sendDescriptor(arduino::USBSetup&) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USBDeviceClass::sendStringDescriptor(unsigned char const*, unsigned long) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USBDeviceClass::sendZlp(unsigned long)            /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
USBDeviceClass::setAddress(unsigned long)         /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USBDeviceClass::stall(unsigned long)              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USBDeviceClass::standby()                         /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
USB_Handler                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
USB_SetHandler                                    /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
Uart::IrqHandler()                                /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
Uart::Uart(SERCOM*, unsigned char, unsigned char, SercomRXPad, SercomUartTXPad) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
Uart::Uart(SERCOM*, unsigned char, unsigned char, SercomRXPad, SercomUartTXPad) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
Uart::Uart(SERCOM*, unsigned char, unsigned char, SercomRXPad, SercomUartTXPad, unsigned char, unsigned char) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
Uart::Uart(SERCOM*, unsigned char, unsigned char, SercomRXPad, SercomUartTXPad, unsigned char, unsigned char) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
Uart::available()                                 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
Uart::availableForWrite()                         /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
Uart::begin(unsigned long)                        /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
Uart::begin(unsigned long, unsigned short)        /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
Uart::end()                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
Uart::extractCharSize(unsigned short)             /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
Uart::extractNbStopBit(unsigned short)            /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
Uart::extractParity(unsigned short)               /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
Uart::flush()                                     /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
Uart::operator bool()                             /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
Uart::peek()                                      /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
Uart::read()                                      /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
Uart::write(unsigned char)                        /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
WDT_Handler                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
__Guard::__Guard()                                /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
__Guard::__Guard()                                /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
__Guard::~__Guard()                               /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
__Guard::~__Guard()                               /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
__StackTop                                        /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
__aeabi_cdcmpeq                                   /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_arm_cmpdf2.o)
__aeabi_cdcmple                                   /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_arm_cmpdf2.o)
__aeabi_cdrcmple                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_arm_cmpdf2.o)
__aeabi_d2iz                                      /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(fixdfsi.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_fixunsdfsi.o)
__aeabi_d2uiz                                     /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_fixunsdfsi.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
__aeabi_dadd                                      /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(adddf3.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
__aeabi_dcmpeq                                    /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_arm_cmpdf2.o)
__aeabi_dcmpge                                    /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_arm_cmpdf2.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_fixunsdfsi.o)
__aeabi_dcmpgt                                    /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_arm_cmpdf2.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
__aeabi_dcmple                                    /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_arm_cmpdf2.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
__aeabi_dcmplt                                    /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_arm_cmpdf2.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
__aeabi_dcmpun                                    /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(unorddf2.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
__aeabi_ddiv                                      /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(divdf3.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
__aeabi_dmul                                      /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(muldf3.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
__aeabi_dsub                                      /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(subdf3.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_fixunsdfsi.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
__aeabi_idiv                                      /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_divsi3.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
__aeabi_idiv0                                     /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_dvmd_tls.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_divsi3.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivsi3.o)
__aeabi_idivmod                                   /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_divsi3.o)
__aeabi_ldiv0                                     /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_dvmd_tls.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_aeabi_uldivmod.o)
__aeabi_ui2d                                      /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(floatunsidf.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
__aeabi_uidiv                                     /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivsi3.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(SERCOM.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
__aeabi_uidivmod                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivsi3.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(divdf3.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
__aeabi_uldivmod                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_aeabi_uldivmod.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
__bss_end__                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
__bss_start__                                     /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
__call_exitprocs                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-exit.o)
__clzdi2                                          /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_clzdi2.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivmoddi4.o)
__clzsi2                                          /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_clzsi2.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_clzdi2.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(floatunsidf.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(subdf3.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(muldf3.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(divdf3.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(adddf3.o)
__cxa_deleted_virtual                             /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(abi.cpp.o)
__cxa_pure_virtual                                /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(abi.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
__data_end__                                      /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
__data_start__                                    /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
__deregister_frame_info                           /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtbegin.o
__divsi3                                          /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_divsi3.o)
__dso_handle                                      /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtbegin.o
__eqdf2                                           /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(eqdf2.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_arm_cmpdf2.o)
__etext                                           /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
__fixunsdfsi                                      /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_fixunsdfsi.o)
__gedf2                                           /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(gedf2.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_arm_cmpdf2.o)
__gnu_thumb1_case_uqi                             /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_thumb1_case_uqi.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_private.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
__gtdf2                                           /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(gedf2.o)
__init_array_end                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-init.o)
__init_array_start                                /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-init.o)
__ledf2                                           /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(ledf2.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_arm_cmpdf2.o)
__libc_fini_array                                 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
__libc_init_array                                 /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-init.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
__ltdf2                                           /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(ledf2.o)
__malloc_free_list                                /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-mallocr.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-freer.o)
__malloc_lock                                     /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-mlock.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-mallocr.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-freer.o)
__malloc_sbrk_start                               /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-mallocr.o)
__malloc_unlock                                   /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-mlock.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-mallocr.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-freer.o)
__nedf2                                           /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(eqdf2.o)
__preinit_array_end                               /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-init.o)
__preinit_array_start                             /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-init.o)
__register_frame_info                             /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crtbegin.o
__sf_fake_stderr                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-impure.o)
__sf_fake_stdin                                   /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-impure.o)
__sf_fake_stdout                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-impure.o)
__stack                                           /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
__text_start__                                    /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
__udivmoddi4                                      /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivmoddi4.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_aeabi_uldivmod.o)
__udivsi3                                         /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/libgcc.a(_udivsi3.o)
_dry_run                                          /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
_exit                                             /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a(_exit.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-exit.o)
_fini                                             /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crti.o
_free_r                                           /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-freer.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-reent.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-malloc.o)
_global_impure_ptr                                /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-impure.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-exit.o)
_impure_ptr                                       /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-impure.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-reent.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-malloc.o)
_init                                             /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/thumb/v6-m/crti.o
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-init.o)
_mainCRTStartup                                   /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
_malloc_r                                         /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-mallocr.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-malloc.o)
_pack_buffer                                      /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
_pack_message                                     /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
_pack_size                                        /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
_reclaim_reent                                    /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-reent.o)
_sbrk                                             /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a(sbrk.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-sbrkr.o)
_sbrk_r                                           /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-sbrkr.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-nano-mallocr.o)
_serialPeek                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
_start                                            /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
_usbConfiguration                                 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
_usbSetInterface                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
analogRead                                        /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
analogReadResolution                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
analogReference                                   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
analogWrite                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
analogWriteResolution                             /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
arduino::PluggableUSB_::PluggableUSB_()           /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
arduino::PluggableUSB_::PluggableUSB_()           /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
arduino::PluggableUSB_::getDescriptor(arduino::USBSetup&) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
arduino::PluggableUSB_::getInterface(unsigned char*) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
arduino::PluggableUSB_::getShortName(char*)       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
arduino::PluggableUSB_::plug(arduino::PluggableUSBModule*) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
arduino::PluggableUSB_::setup(arduino::USBSetup&) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
arduino::Print::availableForWrite()               /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::flush()                           /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::print(arduino::Printable const&)  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::print(arduino::String const&)     /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::print(arduino::__FlashStringHelper const*) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::print(char const*)                /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::print(char)                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::print(double, int)                /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::print(int, int)                   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::print(long long, int)             /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::print(long, int)                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::print(unsigned char, int)         /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::print(unsigned int, int)          /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::print(unsigned long long, int)    /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::print(unsigned long, int)         /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::printFloat(double, int)           /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::printNumber(unsigned long, unsigned char) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::printULLNumber(unsigned long long, unsigned char) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::println()                         /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::println(arduino::Printable const&) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::println(arduino::String const&)   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::println(arduino::__FlashStringHelper const*) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::println(char const*)              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::println(char)                     /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::println(double, int)              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::println(int, int)                 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::println(long long, int)           /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::println(long, int)                /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::println(unsigned char, int)       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::println(unsigned int, int)        /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::println(unsigned long long, int)  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::println(unsigned long, int)       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::write(char const*)                /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
arduino::Print::write(unsigned char const*, unsigned int) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
arduino::RingBufferN<256>::RingBufferN()          /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
arduino::RingBufferN<256>::RingBufferN()          /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
arduino::RingBufferN<64>::store_char(unsigned char) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
arduino::SafeRingBufferN<256>::read_char()        /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
arduino::SafeRingBufferN<256>::store_char(unsigned char) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
arduino::serialEventRun()                         /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
atexit                                            /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
blind                                             /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
cancelReset                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
cleanup_glue                                      /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-reent.o)
closeBlind()                                      /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
delay                                             /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
delayMicroseconds                                 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
digitalRead                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
digitalWrite                                      /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
end                                               /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libnosys.a(sbrk.o)
epBuffer(unsigned int)                            /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(PluggableUSB.cpp.o)
errno                                             /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-reent.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-sbrkr.o)
exception_table                                   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
exit                                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-exit.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
free                                              /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-malloc.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
g_APinDescription                                 /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_private.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
g_apTCInstances                                   /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
hardware_init_hook                                /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
init                                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
initVariant                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
initiateReset                                     /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
loop                                              /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
main                                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
makeWord(unsigned char, unsigned char)            /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
makeWord(unsigned short)                          /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
malloc                                            /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-malloc.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
map(long, long, long, long, long)                 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Common.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
memcpy                                            /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-memcpy-stub.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
memset                                            /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-memset.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                                                  /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
micros                                            /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
millis                                            /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
non-virtual thunk to Serial_::getDescriptor(arduino::USBSetup&) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
non-virtual thunk to Serial_::getInterface(unsigned char*) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
non-virtual thunk to Serial_::getShortName(char*) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
non-virtual thunk to Serial_::setup(arduino::USBSetup&) /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
openBlind()                                       /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
operator delete(void*)                            /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
operator delete[](void*)                          /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
operator new(unsigned int)                        /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
operator new[](unsigned int)                      /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(new.cpp.o)
pdValue                                           /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
pendSVHook                                        /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
photoDiode                                        /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
pinMode                                           /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_digital.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_private.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/libraries/Servo/samd/Servo.cpp.o
pinPeripheral                                     /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_private.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(wiring_analog.c.o)
position                                          /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
resetExternalChip                                 /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
sercom0                                           /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
sercom1                                           /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
sercom2                                           /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
sercom3                                           /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
sercom4                                           /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
sercom5                                           /Users/nico/Documents/GitHub/blinds-controller/build/core/variant.cpp.o
setup                                             /Users/nico/Documents/GitHub/blinds-controller/build/sketch/blinds-controller.ino.cpp.o
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(main.cpp.o)
software_init_hook                                /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/crt0.o
strlen                                            /Users/nico/Library/Arduino15/packages/arduino/tools/arm-none-eabi-gcc/7-2017q4/bin/../lib/gcc/arm-none-eabi/7.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/libc_nano.a(lib_a-strlen.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
svcHook                                           /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
sysTickHook                                       /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(cortex_handlers.c.o)
tickReset                                         /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Reset.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
usbd                                              /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
vtable for DoubleBufferedEPOutHandler             /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(USBCore.cpp.o)
vtable for Serial_                                /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(CDC.cpp.o)
vtable for Uart                                   /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Uart.cpp.o)
vtable for arduino::Print                         /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(Print.cpp.o)
yield                                             /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(hooks.c.o)
                                                  /Users/nico/Documents/GitHub/blinds-controller/build/core/core.a(delay.c.o)
